# Understanding RAID technology

Redundant array of independent disk (RAID) is the technology of grouping several physical drives in a computer into an array that you can define as one or more logical drives. Each logical drive appears to the operating system as a single drive. This grouping technique greatly enhances logical-drive capacity and performance beyond the physical limitations of a single physical drive.

When you group multiple physical drives into a logical drive, the ServeRAID controller can transfer data in parallel from the multiple drives in the array. This parallel transfer yields data-transfer rates that are many times higher than with nonarrayed drives. This increased speed makes the system better able to meet the throughput (the amount of data processed in a given amount of time) or productivity needs of the multiple-user network environment.

The ability to respond to multiple data requests provides not only an increase in throughput, but also a decrease in response time. The combination of parallel transfers and simultaneous responses to multiple requests enables disk arrays to provide a high level of performance in network environments.

## More information

- Things to consider when changing the RAID level
- Understanding stripe-unit size
- RAID level-0
- RAID level-1
- RAID level-1E
- RAID level-5
- RAID level-5 Enhanced
- RAID level-5EE
- RAID level-x0

Glossary | Contents

x-1050-SRM-00-04-EN