# ServeRAID software features

You can use the ServeRAID software with the following controllers. Most components and features are available only with ServeRAID controllers.

ServeRAID features | Integrated RAID controller | ServeRAID-6M | ServeRAID-5i | ServeRAID-4
ServeRAID ROM Update Wizard | No | Yes | Yes | Yes
ServeRAID Manager | Yes | Yes | Yes | Yes
ServeRAID Mini-Configuration program | No | Yes | Yes | Yes
IPSSEND | No | Yes | Yes | Yes
IPSSEND FlashCopy function (Windows XP Professional, Windows 2000, Windows .NET, and Windows NT only) | No | Yes | No | Yes
IPSMON (NetWare only) | No | Yes | Yes | Yes
Clustering (Windows NT, Windows 2000 only) | No | Yes (Windows 2000 only) | No | Yes
Failover (Windows NT, Windows 2000 only) | No | Yes (Windows 2000 only) | No | Yes
RAID level-1 | Yes | Yes | Yes | Yes
RAID level-0, RAID level-1E, RAID level-5 | No | Yes | Yes | Yes
RAID level-5E | No | No | No | Yes
RAID level-5EE | No | Yes | No | Yes (except 4H)
RAID level-x0 | No | Yes | Yes | Yes

ServeRAID features | ServeRAID-3 | ServeRAID-II
ServeRAID ROM Update Wizard | Yes | Yes
ServeRAID Manager | Yes | Yes
ServeRAID Mini-Configuration program | Yes | Yes
IPSSEND | Yes | Yes
IPSSEND FlashCopy function (Windows XP Professional, Windows 2000, Windows .NET, and Windows NT only) | Yes | Yes
IPSMON (NetWare only) | Yes | Yes
Clustering (Windows NT, Windows 2000 only) | Yes | Yes
Failover (Windows NT, Windows 2000 only) | Yes | Yes
RAID level-1 | Yes | Yes
RAID level-0, RAID level-1E, RAID level-5 | Yes | Yes
RAID level-5E | Yes | No
RAID level-5EE | No | No
RAID level-x0 | No | No

Glossary | Contents

x-1089-SRM-00-04-EN