The Media Kit Table of Contents | The Media Kit Index

# BTimeCode

Derived from: none

Declared in: be/media/TimeCode.h

Library: libmedia.so

###### Summary

Include here information about types etc.

## Constructor and Destructor

### BTimeCode()

`BTimeCode()`
`BTimeCode(bigtime_t` us, timecode_type type = B_TIMECODE_DEFAULT`)`

The constructor prepares the BTimeCode object for use. If you use the first form of the constructor, without arguments, you'll have to call an appropriate function to set the BTimeCode's time information before using it for translation purposes. This can be done by calling one or more of `SetData()`, `SetType()`, `SetMicroseconds()`, or `SetLinearFrames()`.

The second form of the constructor accepts as input a time in microseconds, us, and the timecode type.

The third form of the constructor duplicates an existing BTimeCode object.

The fourth form accepts as input a time in hours, minutes, seconds, and frames, as well as the timecode type.

### ~BTimeCode()

`~BTimeCode()`

A typical destructor

## Member Functions

### Frames() see Hours()

### GetData() , SetData()

`void` `GetData(int *`outHours`, int *`outMinutes`, int *`outSeconds`,` int *outFrames`, timecode_type *`outType = NULL`)`
`void` `SetData(int` hours`, int` minutes`, int` seconds`, int` frames`)`

`GetData()` returns the timecode's value in hours, minutes, seconds, and frames, and also returns the timecode type, if you specify a valid pointer for outType. `SetData()` lets you set the timecode's value.

### GetString()

`void` `GetString(char *`str`)` const

Fills str, which must be at least 24 bytes long, with a string indicating the current time in hours, minutes, seconds, and frames. The string is formatted in a manner appropriate to the timecode type. A typical example would be "01:24:09.18", which is 1 hour, 24 minutes, 9 seconds, and 18 frames.

### Hours() , Minutes() , Seconds() , Frames()

`int` `Hours(void``)` const
`int` `Minutes(void``)` const
`int` `Seconds(void``)` const
`int` `Frames(void``)` const

These functions return the time's hours, minutes, seconds, and frames portions.

### LinearFrames() , SetLinearFrames()

`int32` `LinearFrames(void``)` const
`void` `SetLinearFrames(int32` linearFrames`)`

`LinearFrames()` returns the BTimeCode object's time in linear frames. `SetLinearFrames()` lets you change the time, specifying the new time in linear frames.

### Microseconds() , SetMicroseconds()

`bigtime_t` `Microseconds(void``)` const``
`void` `SetMicroseconds(bigtime_t` us`)`

`Microseconds()` returns the BTimeCode object's time, in microseconds. `SetMicroseconds()` lets you change the time, specifying the new time in microseconds.

### Minutes() see Hours()

### Seconds() see Hours()

### SetData() see GetData()

### SetLinearFrames() see LinearFrames()

### SetMicroseconds() see Microseconds()

### SetType() see Type()

### Type() , SetType()

`timecode_type` `Type(void``)` const``
`status_t` `SetType(timecode_type` type`)`

`Type()` returns the BTimeCode object's timecode type. `SetType()` lets you change the timecode type.

RETURN CODES

- `B_OK`. The type was returned safely.

- `B_ERROR`. The timecode type specified is invalid.

## Operators

### = (assignment)

BTimeCode &`operator =(`const BTimeCode &clone`)`

Makes the current BTimeCode identical to the BTimeCode object specified

### == (equality)

BTimeCode &`operator ==(`const BTimeCode &other`)`

Determines whether or not the two BTimeCode objects are equal (their times are the same, regardless of their timecode types).

### < (less than)

BTimeCode &`operator <(`const BTimeCode &other`)`

Indicates whether or not one BTimeCode's time, in microseconds, is less than the other's.

### += (expression plus)

BTimeCode &`operator +=(`const BTimeCode &other`)`

Adds the time of the BTimeCode object other to the current BTimeCode's time.

### -= (expression minus)

BTimeCode &`operator -=(`const BTimeCode &other`)`

Subtracts the time of the BTimeCode object other from the current BTimeCode's time.

### + (plus)

BTimeCode &`operator +(`const BTimeCode &other`)`

Adds two BTimeCode values together, returning a new BTimeCode.

### - (minus)

BTimeCode &`operator -(`const BTimeCode &other`)`

Subtracts two BTimeCode values, returning a new one.

## Global C Functions

### count_timecodes()

`status_t` `count_timecodes(void``)`

Returns the number of recognized time code types.

### frames_to_timecode() , timecode_to_frames()

`status_t` `frames_to_timecode(`int32 linearFrames, int * hours, int * minutes, int * seconds, int * frames, const timecode_info * code = NULL`)`
`status_t` `timecode_to_frames(`int hours, int minutes, int seconds, int frames, int32 * linearFrames, const timecode_info * code = NULL`)`

`frames_to_timecode()` converts the frame offset linearFrames into hours, minutes, seconds, and frames.

`timecode_to_frames()` converts the time from hours, minutes, seconds, and frames into a linear frame offset, storing the result in linearFrames.

The timecode_info structure code is used to determine how the conversion should be made, if you specify it. Otherwise `B_TIMECODE_DEFAULT` is assumed.

Currently these functions always return `B_OK`, but you should still check for errors because you'd hate it if your app broke in the future, wouldn't you?

### get_timecode_description()

`status_t` `get_timecode_description(`timecode_type type, timecode_info * outTimeCode`)`

Fills out the timecode_info structure specified by outTimeCode with information describing the specified timecode type.

RETURN CODES

- `B_OK`. No error.

- `B_ERROR`. The specified timecode type isn't valid.

### timecode_to_frames() see frames_to_timecode()

### timecode_to_us() see us_to_timecode()

### us_to_timecode() , timecode_to_us()

`status_t` `us_to_timecode(`bigtime_t micros, int * hours, int * minutes, int * seconds, int * frames, const timecode_info * code = NULL`)`
`status_t` `timecode_to_us(`int hours, int minutes, int seconds, int frames, bigtime_t * micros, const timecode_info * code = NULL`)`

`us_to_timecode()` converts the time micros, which is specified in microseconds, into hours, minutes, seconds, and frames.

`timecode_to_us()` converts the time from hours, minutes, seconds, and frames into microseconds, storing the result in micros.

The timecode_info structure code is used to determine how the conversion should be made, if you specify it. Otherwise `B_TIMECODE_DEFAULT` is assumed.

Currently these functions always return `B_OK`, but you should still check for errors because you'd hate it if your app broke in the future, wouldn't you?

## Constants

### timecode_type

Declared in: be/media/TimeCode.h

Constant | Description
`B_TIMECODE_DEFAULT` | The default time code
`B_TIMECODE_100` | 100 frames per second.
`B_TIMECODE_75` | CD audio
`B_TIMECODE_30` | MIDI
`B_TIMECODE_30_DROP_2` | NTSC
`B_TIMECODE_30_DROP_4` | Brazil
`B_TIMECODE_25` | PAL
`B_TIMECODE_24` | Film
`B_TIMECODE_18` | Super8

Constants identifying the various timecode types supported by BTimeCode.

## Structures

### timecode_info

Declared in: be/media/TimeCode.h

struct `timecode_info` { timecode_type `type`; int `drop_frames`; int `every_nth`; int `except_nth`; int `fps_div`; char `name`[32]; char `format`[32]; char `_reserved_`[64]; };

The timecode_info structure describes the attributes of a timecode type. You probably should just use the BTimeCode class, or the global C functions, though. It just makes your life easier.

- type indicates the timecode type described by the structure.

- drop_frames indicates how many frames this timecode drops every every_nth minute, except every_nth minute.

- fps_div indicates the nominal frame rate of the format.

- name is a printable name that can be used in constructing user interfaces.

- format is a format to be used in calling `sprintf()`; it's used by `GetString()`.

The Media Kit Table of Contents | The Media Kit Index

The B e Book,
...in lovely HTML...
for BeOS Release 5.

Copyright © 2000 Be, Inc. All rights reserved..