
GUYMAGER ACQUISITION INFO FILE
==============================

Guymager
========

Version            : 0.8.13-1                                                                                            
Version timestamp  : 2021-08-04-17.00.00 UTC                                                                             
Compiled with      : gcc 8.3.0                                                                                           
libewf version     : 20140804 (not used as Guymager is configured to use its own EWF module)                             
libguytools version: 2.1.0                                                                                               
Host name          : bitcurator                                                                                          
Domain name        : (none)                                                                                              
System             : Linux bitcurator 6.8.0-49-generic #49-Ubuntu SMP PREEMPT_DYNAMIC Mon Nov  4 02:06:24 UTC 2024 x86_64


Device information
==================
Command executed: bash -c "search="`basename /dev/sdb`: H..t P.......d A..a de.....d" && dmesg | grep -A3 "$search" || echo "No kernel HPA messages for /dev/sdb""
Information returned:
----------------------------------------------------------------------------------------------------
   No kernel HPA messages for /dev/sdb

Command executed: bash -c "smartctl -s on /dev/sdb ; smartctl -a /dev/sdb"
Information returned:
----------------------------------------------------------------------------------------------------
   smartctl 7.4 2023-08-01 r5530 [x86_64-linux-6.8.0-49-generic] (local build)
   Copyright (C) 2002-23, Bruce Allen, Christian Franke, www.smartmontools.org
   
   /dev/sdb: Unknown USB bridge [0x0644:0x0000 (0x000)]
   Please specify device type with the -d option.
   
   Use smartctl -h to get a usage summary
   
   smartctl 7.4 2023-08-01 r5530 [x86_64-linux-6.8.0-49-generic] (local build)
   Copyright (C) 2002-23, Bruce Allen, Christian Franke, www.smartmontools.org
   
   /dev/sdb: Unknown USB bridge [0x0644:0x0000 (0x000)]
   Please specify device type with the -d option.
   
   Use smartctl -h to get a usage summary

Command executed: bash -c "hdparm -I /dev/sdb"
Information returned:
----------------------------------------------------------------------------------------------------
   /dev/sdb:
   
   ATA device, with non-removable media
   Standards:
   	Likely used: 1
   Configuration:
   	Logical		max	current
   	cylinders	0	0
   	heads		0	0
   	sectors/track	0	0
   	--
   	Logical/Physical Sector size:           512 bytes
   	device size with M = 1024*1024:           0 MBytes
   	device size with M = 1000*1000:           0 MBytes 
   	cache/buffer size  = unknown
   Capabilities:
   	IORDY not likely
   	Cannot perform double-word IO
   	R/W multiple sector transfer: not supported
   	DMA: not supported
   	PIO: pio0

Command executed: bash -c "CIDFILE=/sys/block/$(basename /dev/sdb)/device/cid; echo -n "CID: " ; if [ -e $CIDFILE ] ; then cat $CIDFILE  ; else echo "not available" ; fi "
Information returned:
----------------------------------------------------------------------------------------------------
   CID: not available

Hidden areas: unknown


Acquisition
===========

Linux device            : /dev/sdb                                                  
Device size             : 1474560 (1.5MB)                                           
Format                  : Linux dd raw image - file extension is .dd                
Image path and file name: /media/sf_shared/svr42/Foundation_Extra_pkg_XADD_1of3.dd  
Info  path and file name: /media/sf_shared/svr42/Foundation_Extra_pkg_XADD_1of3.info
Hash calculation        : MD5 and SHA-1                                             
Source verification     : on                                                        
Image verification      : off                                                       

During acquisition, 1 bad sectors have been encountered. They have been replaced by zeroed sectors. The sector numbers are:
   2872
No bad sectors encountered during verification.
State: Finished successfully (with 1 bad sectors)

MD5 hash                   : 5f5e7e09bd5819c01fc05941e8fee666        
MD5 hash verified source   : 423b4932f9290ef8bbf753ec7e5d8b6e        
MD5 hash verified image    : --                                      
SHA1 hash                  : 8f3ae01d5b78ef15171131d8741bd8d918d4ddcc
SHA1 hash verified source  : e9f90758802c57da1ab208041871cbd63f0e0942
SHA1 hash verified image   : --                                      
SHA256 hash                : --                                      
SHA256 hash verified source: --                                      
SHA256 hash verified image : --                                      
Source verification FAILED. The device didn't deliver the same data during acquisition and verification. Check if the defect sector list was the same during acquisition and verification (see above).
Maybe you try to acquire the device again.

Acquisition started : 2024-12-06 22:37:45 (ISO format YYYY-MM-DD HH:MM:SS)  
Verification started: 2024-12-06 22:39:56                                   
Ended               : 2024-12-06 22:40:50 (0 hours, 3 minutes and 4 seconds)
Acquisition speed   : 0.01 MByte/s (0 hours, 2 minutes and 10 seconds)      
Verification speed  : 0.03 MByte/s (0 hours, 0 minutes and 53 seconds)      


Generated image files and their MD5 hashes
==========================================

No MD5 hashes available (configuration parameter CalcImageFileMD5 is off)
MD5                               Image file
