
GUYMAGER ACQUISITION INFO FILE
==============================

Guymager
========

Version            : 0.8.13-1                                                                                            
Version timestamp  : 2021-08-04-17.00.00 UTC                                                                             
Compiled with      : gcc 8.3.0                                                                                           
libewf version     : 20140804 (not used as Guymager is configured to use its own EWF module)                             
libguytools version: 2.1.0                                                                                               
Host name          : bitcurator                                                                                          
Domain name        : (none)                                                                                              
System             : Linux bitcurator 6.8.0-49-generic #49-Ubuntu SMP PREEMPT_DYNAMIC Mon Nov  4 02:06:24 UTC 2024 x86_64


Device information
==================
Command executed: bash -c "search="`basename /dev/sdb`: H..t P.......d A..a de.....d" && dmesg | grep -A3 "$search" || echo "No kernel HPA messages for /dev/sdb""
Information returned:
----------------------------------------------------------------------------------------------------
   No kernel HPA messages for /dev/sdb

Command executed: bash -c "smartctl -s on /dev/sdb ; smartctl -a /dev/sdb"
Information returned:
----------------------------------------------------------------------------------------------------
   smartctl 7.4 2023-08-01 r5530 [x86_64-linux-6.8.0-49-generic] (local build)
   Copyright (C) 2002-23, Bruce Allen, Christian Franke, www.smartmontools.org
   
   /dev/sdb: Unknown USB bridge [0x0644:0x0000 (0x000)]
   Please specify device type with the -d option.
   
   Use smartctl -h to get a usage summary
   
   smartctl 7.4 2023-08-01 r5530 [x86_64-linux-6.8.0-49-generic] (local build)
   Copyright (C) 2002-23, Bruce Allen, Christian Franke, www.smartmontools.org
   
   /dev/sdb: Unknown USB bridge [0x0644:0x0000 (0x000)]
   Please specify device type with the -d option.
   
   Use smartctl -h to get a usage summary

Command executed: bash -c "hdparm -I /dev/sdb"
Information returned:
----------------------------------------------------------------------------------------------------
   /dev/sdb:
   
   ATA device, with non-removable media
   Standards:
   	Likely used: 1
   Configuration:
   	Logical		max	current
   	cylinders	0	0
   	heads		0	0
   	sectors/track	0	0
   	--
   	Logical/Physical Sector size:           512 bytes
   	device size with M = 1024*1024:           0 MBytes
   	device size with M = 1000*1000:           0 MBytes 
   	cache/buffer size  = unknown
   Capabilities:
   	IORDY not likely
   	Cannot perform double-word IO
   	R/W multiple sector transfer: not supported
   	DMA: not supported
   	PIO: pio0

Command executed: bash -c "CIDFILE=/sys/block/$(basename /dev/sdb)/device/cid; echo -n "CID: " ; if [ -e $CIDFILE ] ; then cat $CIDFILE  ; else echo "not available" ; fi "
Information returned:
----------------------------------------------------------------------------------------------------
   CID: not available

Hidden areas: unknown


Acquisition
===========

Linux device            : /dev/sdb                                           
Device size             : 1474560 (1.5MB)                                    
Format                  : Linux dd raw image - file extension is .dd         
Image path and file name: /media/sf_shared/svr42/Foundation_pkg_NSU_1of1.dd  
Info  path and file name: /media/sf_shared/svr42/Foundation_pkg_NSU_1of1.info
Hash calculation        : MD5 and SHA-1                                      
Source verification     : on                                                 
Image verification      : off                                                

No bad sectors encountered during acquisition.
No bad sectors encountered during verification.
State: Finished successfully

MD5 hash                   : d059d6f5c5185442710366c68ba1dada        
MD5 hash verified source   : d059d6f5c5185442710366c68ba1dada        
MD5 hash verified image    : --                                      
SHA1 hash                  : fe5027b8d1d1390fd90c04b4d5d2e33aecc3864d
SHA1 hash verified source  : fe5027b8d1d1390fd90c04b4d5d2e33aecc3864d
SHA1 hash verified image   : --                                      
SHA256 hash                : --                                      
SHA256 hash verified source: --                                      
SHA256 hash verified image : --                                      
Source verification OK. The device delivered the same data during acquisition and verification.

Acquisition started : 2024-12-06 21:38:06 (ISO format YYYY-MM-DD HH:MM:SS)   
Verification started: 2024-12-06 21:39:01                                    
Ended               : 2024-12-06 21:39:55 (0 hours, 1 minutes and 48 seconds)
Acquisition speed   : 0.03 MByte/s (0 hours, 0 minutes and 54 seconds)       
Verification speed  : 0.03 MByte/s (0 hours, 0 minutes and 53 seconds)       


Generated image files and their MD5 hashes
==========================================

No MD5 hashes available (configuration parameter CalcImageFileMD5 is off)
MD5                               Image file
