This is ISC INTERACTIVE UNIX 3.0 for 86Box

This setup has working networking and 1024x768 X11.

Setup guide:
Before startingIn 86Box you need to attach PCap to your LAN NIC.
Go to Tools -> Settings -> Network -> PCap Device

Once system boots login as root password root

IP address can be set /etc/netd.cf, gateway is /etc/rc3.d/S05hbtcp
By default IX uses entries from /etc/hosts but you can set to IP
addresses just fine.

Looking Glass will complain for lack of license server. I suspect
this is something to do with name server and network configuration.
An easy workaround is to temporairly disable NIC. Either go back to
the text mode console or open an xterm and run:

/etc/ifconfig ne0 down

Re-run looking glass (lg&) or login back to X11 via xdm. Then run:

/etc/ifconfig ne0 up

Most system admin tasks are performed using "sysadm" command.

A few open source apps are included, bash, emacs, gzip, gtar, mosaic.

Have fun!
-tenox