SYSSETMOD       - SYSTEM SERVICES TO SET PROCESS MODES           21-AUG-1978 20:43:14   VAX-11 MACRO X0.3-11               Page   0

TABLE OF CONTENTS   



   (1)      49  SET RESOURCE WAIT MODE

   (1)      80  SET SYSTEM SERVICE FAILURE EXCEPTION MODE

   (1)     113  SET PROCESS SWAP MODE

SYSSETMOD       - SYSTEM SERVICES TO SET PROCESS MODES           21-AUG-1978 20:43:14   VAX-11 MACRO X0.3-11               Page   1

01                                                                                                                               (1)



                                     0000     1 	.TITLE	SYSSETMOD - SYSTEM SERVICES TO SET PROCESS MODES

                                     0000     2 	.IDENT	/01/

                                     0000     3  

                                     0000     4 ;

                                     0000     5 ; COPYRIGHT (C) 1977

                                     0000     6 ; DIGITAL EQUIPMENT CORPORATION, MAYNARD, MASS.

                                     0000     7 ;

                                     0000     8 ; THIS SOFTWARE IS FURNISHED UNDER  A LICENSE FOR USE ONLY  ON  A

                                     0000     9 ; SINGLE COMPUTER SYSTEM AND MAY BE  COPIED ONLY WITH  THE INCLU-

                                     0000    10 ; SION OF  THE  ABOVE  COPYRIGHT NOTICE.  THIS SOFTWARE,  OR  ANY

                                     0000    11 ; OTHER COPIES THEREOF, MAY NOT BE  PROVIDED  OR  OTHERWISE  MADE

                                     0000    12 ; AVAILABLE TO ANY OTHER PERSON EXCEPT  FOR  USE  ON  SUCH SYSTEM

                                     0000    13 ; AND TO  ONE WHO AGREES  TO  THESE LICENSE  TERMS.  TITLE TO AND

                                     0000    14 ; OWNERSHIP OF THE SOFTWARE SHALL AT ALL TIMES REMAIN IN DEC.

                                     0000    15 ;

                                     0000    16 ; THE INFORMATION IN THIS SOFTWARE  IS  SUBJECT TO CHANGE WITHOUT

                                     0000    17 ; NOTICE AND SHOULD NOT BE CONSTRUED  AS  A COMMITMENT BY DIGITAL

                                     0000    18 ; EQUIPMENT CORPORATION.

                                     0000    19 ;

                                     0000    20 ; DEC ASSUMES NO RESPONSIBILITY FOR THE USE OR RELIABILITY OF ITS

                                     0000    21 ; SOFTWARE ON EQUIPMENT WHICH IS NOT SUPPLIED BY DEC.

                                     0000    22 ;

                                     0000    23 ; D. N. CUTLER 17-AUG-76

                                     0000    24 ;

                                     0000    25 ; SYSTEM SERVICES TO SET PROCESS MODES

                                     0000    26 ;

                                     0000    27 ;	SET RESOURCE WAIT MODE

                                     0000    28 ;	SET SYSTEM SERVICE FAILURE EXCEPTION MODE

                                     0000    29 ;	SET PROCESS SWAP MODE

                                     0000    30 ;

                                     0000    31 ; MACRO LIBRARY CALLS

                                     0000    32 ;

                                     0000    33  

                                     0000    34 	$PCBDEF				;DEFINE PCB OFFSETS

                                     0000    35 	$PRVDEF				;DEFINE PRIVILEGE BITS

                                     0000    36 	$PSLDEF				;DEFINE PROCESSOR STATUS FIELDS

                                     0000    37 	$SSDEF				;DEFINE SYSTEM STATUS VALUES

                                     0000    38  

                                     0000    39 ;

                                     0000    40 ; LOCAL SYMBOLS

                                     0000    41 ;

                                     0000    42 ; ARGUMENT LIST OFFSET DEFINITIONS

                                     0000    43 ;

                                     0000    44  

                           00000004  0000    45 ENBFLG=4				;FAILURE MODE INDICATOR

                           00000004  0000    46 SWPFLG=4				;SWAP MODE INDICATOR

                           00000004  0000    47 WATFLG=4				;WAIT MODE INDICATOR

SYSSETMOD       - SYSTEM SERVICES TO SET PROCESS MODES           21-AUG-1978 20:43:14   VAX-11 MACRO X0.3-11               Page   2

01              SET RESOURCE WAIT MODE                                                                                           (1)



                                     0000    49 	.SBTTL	SET RESOURCE WAIT MODE

                                     0000    50 ;+

                                     0000    51 ; EXE$SETRWM - SET RESOURCE WAIT MODE

                                     0000    52 ;

                                     0000    53 ; THIS SERVICE PROVIDES THE CAPABILITY TO CONTROL WHETHER IMPLICIT WAITS

                                     0000    54 ; ARE TO BE PERFORMED BY THE SYSTEM WHEN A REQUEST FOR A RESOURCE FAILS.

                                     0000    55 ;

                                     0000    56 ; INPUTS:

                                     0000    57 ;

                                     0000    58 ;	WATFLG(AP) = WAIT MODE INDICATOR.

                                     0000    59 ;		LOW BIT CLEAR TO ENABLE IMPLIED RESOURCE WAIT.

                                     0000    60 ;		LOW BIT SET TO DISABLE IMPLIED RESOURCE WAIT.

                                     0000    61 ;

                                     0000    62 ;	R4 = CURRENT PROCESS PCB ADDRESS.

                                     0000    63 ;

                                     0000    64 ; OUTPUTS:

                                     0000    65 ;

                                     0000    66 ;	R0 LOW BIT SET INDICATES SUCCESSFUL COMPLETION.

                                     0000    67 ;

                                     0000    68 ;		R0 = SS$_WASCLR - NORMAL COMPLETION, RESOURCE WAIT WAS

                                     0000    69 ;			PREVIOUSLY ENABLED.

                                     0000    70 ;

                                     0000    71 ;		R0 = SS$_WASSET - NORMAL COMPLETION, RESOURCE WAIT WAS

                                     0000    72 ;			PREVIOUSLY DISABLED.

                                     0000    73 ;-

                                     0000    74  

                                 00000000    75 	.PSECT	Y$EXEPAGED

                               0010' 0000    76 	.ENTRY	EXE$SETRWM,^M<R4>

            51            0A     9A  0002    77 	MOVZBL	#PCB$V_SSRWAIT,R1	;SET RESOURCE WAIT BIT NUMBER

                          1B     11  0005    78 	BRB	SETMOD			;FINISH IN COMMON CODE

SYSSETMOD       - SYSTEM SERVICES TO SET PROCESS MODES           21-AUG-1978 20:43:14   VAX-11 MACRO X0.3-11               Page   3

01              SET SYSTEM SERVICE FAILURE EXCEPTION MODE                                                                        (1)



                                     0007    80 	.SBTTL	SET SYSTEM SERVICE FAILURE EXCEPTION MODE

                                     0007    81 ;+

                                     0007    82 ; EXE$SETSFM - SET SYSTEM SERVICE FAILURE EXCEPTION MODE

                                     0007    83 ;

                                     0007    84 ; THIS SERVICE PROVIDES THE CAPABILITY TO CONTROL THE GENERATION OF SYSTEM

                                     0007    85 ; SERVICE FAILURE EXCEPTIONS WHEN A SERVICE RETURNS A STATUS VALUE WITH A

                                     0007    86 ; SEVERITY OF ERROR OR SEVERE ERROR.

                                     0007    87 ;

                                     0007    88 ; INPUTS:

                                     0007    89 ;

                                     0007    90 ;	ENBFLG(AP) = FAILURE MODE INDICATOR.

                                     0007    91 ;		LOW BIT CLEAR TO DISABLE FAILURE EXCEPTIONS.

                                     0007    92 ;		LOW BIT SET TO ENABLE FAILURE EXCEPTIONS.

                                     0007    93 ;

                                     0007    94 ;	R4 = CURRENT PROCESS PCB ADDRESS.

                                     0007    95 ;

                                     0007    96 ; OUTPUTS:

                                     0007    97 ;

                                     0007    98 ;	R0 LOW BIT SET INDICATES SUCCESSFUL COMPLETION.

                                     0007    99 ;

                                     0007   100 ;		R0 = SS$_WASCLR - NORMAL COMPLETION, FAILURE EXCEPTIONS

                                     0007   101 ;			WERE PREVIOUSLY DISABLED.

                                     0007   102 ;

                                     0007   103 ;		R0 = SS$_WASSET - NORMAL COMPLETION, FAILURE EXCEPTIONS

                                     0007   104 ;			WERE PREVIOUSLY ENABLED.

                                     0007   105 ;-

                                     0007   106  

                               0010' 0007   107 	.ENTRY	EXE$SETSFM,^M<R4>

                          51     DC  0009   108 	MOVPSL	R1			;READ CURRENT PSL

            02            16     EF  000B   109 	EXTZV	#PSL$V_PRVMOD,#PSL$S_PRVMOD,R1,R1 ;EXTRACT PREVIOUS MODE

            51            51         000E       

            51            06     C0  0010   110 	ADDL	#PCB$V_SSFEXC,R1	;ADD BASE FAILURE ENABLE BIT NUMBER

                          0D     11  0013   111 	BRB	SETMOD			;FINISH IN COMMON CODE

SYSSETMOD       - SYSTEM SERVICES TO SET PROCESS MODES           21-AUG-1978 20:43:14   VAX-11 MACRO X0.3-11               Page   4

01              SET PROCESS SWAP MODE                                                                                            (1)



                                     0015   113 	.SBTTL	SET PROCESS SWAP MODE

                                     0015   114 ;+

                                     0015   115 ; EXE$SETSWM - SET PROCESS SWAP MODE

                                     0015   116 ;

                                     0015   117 ; THIS SERVICE PROVIDES THE CAPABILITY TO LOCK OR UNLOCK A PROCESS FROM

                                     0015   118 ; THE BALANCE SET. LOCKED IN THE BALANCE SET PREVENTS A PROCESS FROM BEING

                                     0015   119 ; SWAPPED OUT OF MEMORY.

                                     0015   120 ;

                                     0015   121 ; INPUTS:

                                     0015   122 ;

                                     0015   123 ;	SWPFLG(AP) = PROCESS SWAP MODE INDICATOR.

                                     0015   124 ;		LOW BIT CLEAR TO DISABLE PROCESS SWAPPING.

                                     0015   125 ;		LOW BIT SET TO ENABLE PROCESS SWAPPING.

                                     0015   126 ;

                                     0015   127 ;	R4 = CURRENT PROCESS PCB ADDRESS.

                                     0015   128 ;

                                     0015   129 ; OUTPUTS:

                                     0015   130 ;

                                     0015   131 ;	R0 LOW BIT CLEAR INDICATES FAILURE TO SET PROCESS SWAP MODE.

                                     0015   132 ;

                                     0015   133 ;		R0 = SS$_NOPRIV - PROCESS DOES NOT HAVE PRIVILEGE TO

                                     0015   134 ;			CHANGE ITS SWAP MODE.

                                     0015   135 ;

                                     0015   136 ;	R0 LOW BIT SET INDICATES SUCCESSFUL COMPLETION.

                                     0015   137 ;

                                     0015   138 ;		R0 = SS$_WASCLR - NORMAL COMPLETION, PROCESS WAS PREVIOUSLY

                                     0015   139 ;			NOT LOCKED IN BALANCE SET.

                                     0015   140 ;

                                     0015   141 ;		R0 = SS$_WASSET - NORMAL COMPLETION, PROCESS WAS PREVIOUSLY

                                     0015   142 ;			LOCKED IN BALANCE SET.

                                     0015   143 ;-

                                     0015   144  

                                     0015   145 	.ENABL	LSB

                               0010' 0015   146 	.ENTRY	EXE$SETSWM,^M<R4>

            50            24     3C  0017   147 	MOVZWL	#SS$_NOPRIV,R0		;ASSUME PROCESS CANNOT CHANGE SWAP MODE

                                     001A   148 	IFNPRIV	PSWAPM,20$		;PROCESS HAVE PRIVILEGE TO CHANGE SWAP MODE?

            51            04     9A  001F   149 	MOVZBL	#PCB$V_PSWAPM,R1	;SET PROCESS SWAP BIT NUMBER

            50            09     3C  0022   150 SETMOD:	MOVZWL	#SS$_WASSET,R0		;ASSUME PREVIOUSLY SET

         28 A4            51     E0  0025   151 	BBS	R1,PCB$L_STS(R4),10$	;IF SET, MODE CURRENTLY SET

                          03         0029       

            50            01     3C  002A   152 	MOVZWL	#SS$_WASCLR,R0		;PREVIOUSLY CLEAR

            51         04 AC     F0  002D   153 10$:	INSV	ENBFLG(AP),R1,#1,PCB$L_STS(R4) ;SET NEW MODE

         28 A4            01         0031       

                                 04  0034   154 20$:	RET				;

                                     0035   155 	.DSABL	LSB

                                     0035   156  

                                     0035   157 	.END

SYSSETMOD       - SYSTEM SERVICES TO SET PROCESS MODES           21-AUG-1978 20:43:14   VAX-11 MACRO X0.3-11               Page   5

SYMBOL TABLE                                                                                                                     (1)



BIT...         = 00000000            PCB$W_APTCNT     00000034            PSL$M_PRVMOD   = 00C00000            

ENBFLG         = 00000004            PCB$W_ASTCNT     0000003C            PSL$M_SAFBITS  = 000037FF            

EXE$SETRWM       00000000 RG    03   PCB$W_BIOCNT     0000003E            PSL$M_TBIT     = 00000010            

EXE$SETSFM       00000007 RG    03   PCB$W_BIOLM      00000040            PSL$M_TP       = 40000000            

EXE$SETSWM       00000015 RG    03   PCB$W_BYTCNT     00000042            PSL$S_CURMOD   = 00000002            

GBL...         = 00000000            PCB$W_BYTLM      00000068            PSL$S_IPL      = 00000005            

PCB$B_ASTACT     0000000C            PCB$W_DIOCNT     00000044            PSL$S_PRVMOD   = 00000002            

PCB$B_ASTEN      0000000D            PCB$W_DIOLM      00000046            PSL$V_CM       = 0000001F            

PCB$B_PRI        0000000B            PCB$W_FILCNT     00000048            PSL$V_CURMOD   = 00000018            

PCB$B_PRIB       00000033            PCB$W_GPGCNT     00000038            PSL$V_DV       = 00000007            

PCB$B_TYPE       0000000A            PCB$W_GRP        00000022            PSL$V_FPD      = 0000001B            

PCB$B_WEFC       00000032            PCB$W_MEM        00000020            PSL$V_FU       = 00000006            

PCB$C_LENGTH     0000007C            PCB$W_MTXCNT     0000000E            PSL$V_IPL      = 00000010            

PCB$K_LENGTH     0000007C            PCB$W_PPGCNT     0000003A            PSL$V_IS       = 0000001A            

PCB$L_ASTQBL     00000014            PCB$W_PRCCNT     0000006A            PSL$V_IV       = 00000005            

PCB$L_ASTQFL     00000010            PCB$W_SIZE       00000008            PSL$V_PRVMOD   = 00000016            

PCB$L_EFC2P      00000058            PCB$W_STATE      00000030            PSL$V_TBIT     = 00000004            

PCB$L_EFC3P      0000005C            PCB$W_TMBU       00000036            PSL$V_TP       = 0000001E            

PCB$L_EFCS       00000050            PCB$W_TQCNT      0000004A            SETMOD           00000022 R     03   

PCB$L_EFCU       00000054            PRV$V_ALLSPOOL = 00000004            SS$_ABORT      = 0000002C            

PCB$L_EFWM       0000004C            PRV$V_BUGCHK   = 00000017            SS$_ACCONFLICT = 00000800            

PCB$L_OWNER      0000001C            PRV$V_CMEXEC   = 00000001            SS$_ACCVIO     = 0000000C            

PCB$L_PHD        00000064            PRV$V_CMKRNL   = 00000000            SS$_ACPVAFUL   = 000002FC            

PCB$L_PHYPCB     00000018            PRV$V_DETACH   = 00000005            SS$_ARTRES     = 00000474            

PCB$L_PID        00000060            PRV$V_DIAGNOSE = 00000006            SS$_ASTFLT     = 0000040C            

PCB$L_PQB        0000004C            PRV$V_EXQUOTA  = 00000013            SS$_BADATTRIB  = 00000034            

PCB$L_SQBL       00000004            PRV$V_GROUP    = 00000008            SS$_BADCHKSUM  = 00000808            

PCB$L_SQFL       00000000            PRV$V_GRPNAM   = 00000003            SS$_BADESCAPE  = 0000003C            

PCB$L_STS        00000028            PRV$V_LOG_IO   = 00000007            SS$_BADFILEHDR = 00000810            

PCB$L_UIC        00000020            PRV$V_MOUNT    = 00000011            SS$_BADFILENAME= 00000818            

PCB$L_WSSWP      00000024            PRV$V_NETMBX   = 00000014            SS$_BADFILEVER = 00000820            

PCB$L_WTIME      0000002C            PRV$V_NOACNT   = 00000009            SS$_BADIMGHDR  = 00000044            

PCB$T_LNAME      0000006C            PRV$V_OPER     = 00000012            SS$_BADIRECTORY= 00000828            

PCB$V_ASTPEN   = 00000011            PRV$V_PHY_IO   = 00000016            SS$_BADPARAM   = 00000014            

PCB$V_BATCH    = 0000000E            PRV$V_PRMCEB   = 0000000A            SS$_BADSTACK   = 000002B4            

PCB$V_DELPEN   = 00000001            PRV$V_PRMGBL   = 00000018            SS$_BEGOFFILE  = 00000938            

PCB$V_FORCPEN  = 00000002            PRV$V_PRMMBX   = 0000000B            SS$_BLOCKCNTERR= 00000940            

PCB$V_HIBER    = 00000013            PRV$V_PSWAPM   = 0000000C            SS$_BREAK      = 00000414            

PCB$V_INQUAN   = 00000003            PRV$V_SETPRI   = 0000000D            SS$_BUFBYTALI  = 0000030C            

PCB$V_LOGIN    = 00000014            PRV$V_SETPRV   = 0000000E            SS$_BUFFEROVF  = 00000601            

PCB$V_NETWRK   = 00000015            PRV$V_SYSGBL   = 00000019            SS$_BUGCHECK   = 000002A4            

PCB$V_NOACNT   = 0000000F            PRV$V_SYSNAM   = 00000002            SS$_CANCEL     = 00000830            

PCB$V_NODELET  = 00000017            PRV$V_TMPMBX   = 0000000F            SS$_CHANINTLK  = 0000004C            

PCB$V_PHDRES   = 00000012            PRV$V_VOLPRO   = 00000015            SS$_CLIFRCEXT  = 00000980            

PCB$V_PSWAPM   = 00000004            PRV$V_WORLD    = 00000010            SS$_CMODSUPR   = 0000041C            

PCB$V_PWRAST   = 00000016            PSL$C_EXEC     = 00000001            SS$_CMODUSER   = 00000424            

PCB$V_RES      = 00000000            PSL$C_KERNEL   = 00000000            SS$_COMPAT     = 0000042C            

PCB$V_RESPEN   = 00000005            PSL$C_SUPER    = 00000002            SS$_CONTINUE   = 00000001            

PCB$V_SSFEXC   = 00000006            PSL$C_USER     = 00000003            SS$_CONTROLC   = 00000651            

PCB$V_SSFEXCE  = 00000007            PSL$M_CM       = 80000000            SS$_CONTROLO   = 00000609            

PCB$V_SSFEXCS  = 00000008            PSL$M_CURMOD   = 03000000            SS$_CONTROLY   = 00000611            

PCB$V_SSFEXCU  = 00000009            PSL$M_DV       = 00000080            SS$_CREATED    = 00000619            

PCB$V_SSRWAIT  = 0000000A            PSL$M_FPD      = 08000000            SS$_CTRLERR    = 00000054            

PCB$V_SUSPEN   = 0000000B            PSL$M_FU       = 00000040            SS$_DATACHECK  = 0000005C            

PCB$V_SWPVBN   = 00000010            PSL$M_IPL      = 001F0000            SS$_DATAOVERUN = 00000838            

PCB$V_WAKEPEN  = 0000000C            PSL$M_IS       = 04000000            SS$_DEBUG      = 0000046C            

PCB$V_WALL     = 0000000D            PSL$M_IV       = 00000020            SS$_DECOVF     = 000004A4            

SYSSETMOD       - SYSTEM SERVICES TO SET PROCESS MODES           21-AUG-1978 20:43:14   VAX-11 MACRO X0.3-11               Page   6

SYMBOL TABLE                                                                                                                     (1)



SS$_DEVACTIVE  = 000002C4            SS$_INSFWSL    = 0000011C            SS$_OPINCOMPL  = 000002D4            

SS$_DEVALLOC   = 00000840            SS$_INTDIV     = 00000484            SS$_PAGOWNVIO  = 000001EC            

SS$_DEVALRALLOC= 00000641            SS$_INTOVF     = 0000047C            SS$_PAGRDERR   = 00000444            

SS$_DEVASSIGN  = 00000848            SS$_IVADDR     = 00000134            SS$_PARITY     = 000001F4            

SS$_DEVFOREIGN = 00000064            SS$_IVCHAN     = 0000013C            SS$_PARTESCAPE = 000001FC            

SS$_DEVICEFULL = 00000850            SS$_IVCHNLSEC  = 0000026C            SS$_PFMBSY     = 00000204            

SS$_DEVMOUNT   = 0000006C            SS$_IVDEVNAM   = 00000144            SS$_PLHLDR     = 00000404            

SS$_DEVNOTALLOC= 00000858            SS$_IVGSDNAM   = 0000014C            SS$_PSTFULL    = 0000020C            

SS$_DEVNOTMBX  = 00000074            SS$_IVLOGNAM   = 00000154            SS$_RADRMOD    = 0000044C            

SS$_DEVNOTMOUNT= 0000007C            SS$_IVLOGTAB   = 0000015C            SS$_REJECT     = 00000294            

SS$_DEVOFFLINE = 00000084            SS$_IVPROTECT  = 000002F4            SS$_REMOTE     = 00000649            

SS$_DIRFULL    = 00000860            SS$_IVQUOTAL   = 00000164            SS$_RESIGNAL   = 00000918            

SS$_DRVERR     = 0000008C            SS$_IVSECFLG   = 0000016C            SS$_RESULTOVF  = 00000214            

SS$_DUPFILENAME= 00000868            SS$_IVSECIDCTL = 000002E4            SS$_ROPRAND    = 00000454            

SS$_DUPLNAM    = 00000094            SS$_IVSSRQ     = 00000174            SS$_SECTBLFUL  = 0000021C            

SS$_ENDOFFILE  = 00000870            SS$_IVSTSFLG   = 0000017C            SS$_SSFAIL     = 0000045C            

SS$_ENDOFTAPE  = 00000878            SS$_IVTIME     = 00000184            SS$_SUBRNG     = 000004AC            

SS$_ENDOFUSRLBL= 00000970            SS$_LCKPAGFUL  = 000000D4            SS$_SUPERSEDE  = 00000631            

SS$_EXQUOTA    = 0000001C            SS$_LENVIO     = 0000018C            SS$_TAPEPOSLOST= 00000224            

SS$_EXTIDXFILE = 00000880            SS$_LKWSETFUL  = 00000194            SS$_TBIT       = 00000464            

SS$_FCPREADERR = 00000888            SS$_MBFULL     = 000008D8            SS$_TIMEOUT    = 0000022C            

SS$_FCPREPSTN  = 00000988            SS$_MBTOOSML   = 0000019C            SS$_TOOMANYVER = 00000990            

SS$_FCPREWNDERR= 00000890            SS$_MCHECK     = 000002BC            SS$_TOOMUCHDATA= 0000029C            

SS$_FCPSPACERR = 00000898            SS$_MEDOFL     = 000001A4            SS$_UNASEFC    = 00000234            

SS$_FCPWRITERR = 000008A0            SS$_MSGNOTFND  = 00000621            SS$_UNSAFE     = 0000023C            

SS$_FILACCERR  = 0000009C            SS$_MTLBLLONG  = 00000304            SS$_UNWIND     = 00000920            

SS$_FILALRACC  = 000000A4            SS$_MUSTCLOSEFL= 00000948            SS$_UNWINDING  = 00000928            

SS$_FILELOCKED = 000008A8            SS$_NOAQB      = 00000314            SS$_VASFULL    = 00000244            

SS$_FILENUMCHK = 000008B0            SS$_NODATA     = 000001AC            SS$_VECINUSE   = 0000024C            

SS$_FILESEQCHK = 000008B8            SS$_NOHANDLER  = 000008F8            SS$_VOLINV     = 00000254            

SS$_FILESTRUCT = 000008C0            SS$_NOHOMEBLK  = 000008E0            SS$_WAITUSRLBL = 00000950            

SS$_FILNOTACC  = 000000AC            SS$_NOIOCHAN   = 000001B4            SS$_WASCLR     = 00000001            

SS$_FILNOTCNTG = 000002AC            SS$_NOLINKS    = 0000027C            SS$_WASECC     = 00000639            

SS$_FILNOTEXP  = 000000B4            SS$_NOLOGNAM   = 000001BC            SS$_WASSET     = 00000009            

SS$_FLTDIV     = 00000494            SS$_NOMBX      = 00000274            SS$_WRITLCK    = 0000025C            

SS$_FLTOVF     = 0000048C            SS$_NOMOREFILES= 00000930            SS$_WRONGACP   = 0000031C            

SS$_FLTUND     = 0000049C            SS$_NONEXDRV   = 000001C4            SWPFLG         = 00000004            

SS$_FORMAT     = 000000BC            SS$_NONEXPR    = 000008E8            WATFLG         = 00000004            

SS$_GPTFULL    = 000000C4            SS$_NONLOCAL   = 000008F0            

SS$_GSDFULL    = 000000CC            SS$_NOPRIV     = 00000024            

SS$_HANGUP     = 000002CC            SS$_NORMAL     = 00000001            

SS$_HEADERFULL = 000008C8            SS$_NOSIGNAL   = 00000900            

SS$_IDXFILEFULL= 000008D0            SS$_NOSOLICIT  = 00000284            

SS$_ILLBLKNUM  = 000000DC            SS$_NOSUCHDEV  = 00000908            

SS$_ILLCNTRFUNC= 000000E4            SS$_NOSUCHFILE = 00000910            

SS$_ILLEFC     = 000000EC            SS$_NOSUCHNODE = 0000028C            

SS$_ILLIOFUNC  = 000000F4            SS$_NOSUCHSEC  = 00000978            

SS$_ILLLBLAST  = 00000968            SS$_NOTAPEOP   = 00000264            

SS$_ILLPAGCNT  = 000000FC            SS$_NOTFILEDEV = 000001CC            

SS$_ILLSEQOP   = 000002DC            SS$_NOTINTBLSZ = 000001D4            

SS$_ILLSER     = 00000104            SS$_NOTLABELMT = 000001DC            

SS$_ILLUSRLBLRD= 00000958            SS$_NOTMODIFIED= 00000659            

SS$_ILLUSRLBLWT= 00000960            SS$_NOTNETDEV  = 000002EC            

SS$_INCVOLLABEL= 0000010C            SS$_NOTRAN     = 00000629            

SS$_INSFARG    = 00000114            SS$_NOTSQDEV   = 000001E4            

SS$_INSFMEM    = 00000124            SS$_OPCCUS     = 00000434            

SS$_INSFRAME   = 0000012C            SS$_OPCDEC     = 0000043C            

SYSSETMOD       - SYSTEM SERVICES TO SET PROCESS MODES           21-AUG-1978 20:43:14   VAX-11 MACRO X0.3-11               Page   7

PROGRAM SECTION SYNOPSIS                                                                                                         (1)







PROGRAM SECTION SYNOPSIS



.  ABS  .        00000000      00     NOPIC   USR   CON   ABS   LCL NOSHR NOEXE NORD  NOWRT BYTE  

. BLANK .        00000000      01     NOPIC   USR   CON   REL   LCL NOSHR   EXE   RD    WRT BYTE  

$ABS$            0000007C      02     NOPIC   USR   CON   ABS   LCL NOSHR   EXE   RD    WRT BYTE  

Y$EXEPAGED       00000035      03     NOPIC   USR   CON   REL   LCL NOSHR   EXE   RD    WRT BYTE  





THERE WERE NO ERRORS OR WARNINGS.

15660. BYTES LEFT IN FREE MEMORY POOL.

3750. BYTES OF RECLAIMED MEMORY.

OBJ$:SYSSETMOD,LIS$:SYSSETMOD/-SP=EXECML$/ML,SRC$:SYSSETMOD

4 MLB DIR RDS - 529 GETS TO DEFINE 14 MACROS. 42 INTER. FILE WRITES. 

