RSXCRDRV        - VAX/VMS RSX11M AME CARD READER DRIVER          22-AUG-1978 05:13:49   VAX-11 MACRO X0.3-11               Page   0

TABLE OF CONTENTS   



   (2)      41  RSX$CR_DRV - RSX11M AME CARD READER DRIVER

   (3)      95  CR_RVB AND CR_RLB FUNCTIONS

RSXCRDRV        - VAX/VMS RSX11M AME CARD READER DRIVER          22-AUG-1978 05:13:49   VAX-11 MACRO X0.3-11               Page   1

V06.0                                                                                                                            (1)



                                     0000     1 	.TITLE	RSXCRDRV - VAX/VMS RSX11M AME CARD READER DRIVER

                                     0000     2 	.IDENT	/V06.0/		;

                                     0000     3 

                                     0000     4 ;

                                     0000     5 ; COPYRIGHT (C) 1978

                                     0000     6 ; DIGITAL EQUIPMENT CORPORATION, MAYNARD, MASSACHUSETTS 01754

                                     0000     7 ;

                                     0000     8 ; THIS SOFTWARE IS FURNISHED  UNDER A LICENSE FOR USE ONLY ON A SINGLE

                                     0000     9 ; COMPUTER  SYSTEM AND  MAY BE  COPIED ONLY WITH  THE INCLUSION OF THE

                                     0000    10 ; ABOVE COPYRIGHT NOTICE.  THIS SOFTWARE, OR ANY OTHER COPIES THEREOF,

                                     0000    11 ; MAY NOT BE PROVIDED OR  OTHERWISE MADE AVAILABLE TO ANY OTHER PERSON

                                     0000    12 ; EXCEPT FOR USE ON SUCH SYSTEM AND TO ONE WHO AGREES TO THESE LICENSE

                                     0000    13 ; TERMS.  TITLE TO AND  OWNERSHIP OF THE  SOFTWARE  SHALL AT ALL TIMES

                                     0000    14 ; REMAIN IN DEC.

                                     0000    15 ;

                                     0000    16 ; THE INFORMATION IN THIS SOFTWARE IS SUBJECT TO CHANGE WITHOUT NOTICE

                                     0000    17 ; AND SHOULD  NOT BE CONSTRUED  AS A COMMITMENT  BY DIGITAL  EQUIPMENT

                                     0000    18 ; CORPORATION.

                                     0000    19 ;

                                     0000    20 ; DEC ASSUMES  NO  RESPONSIBILITY  FOR  THE USE OR  RELIABILITY OF ITS

                                     0000    21 ; SOFTWARE ON EQUIPMENT WHICH IS NOT SUPPLIED BY DEC.

                                     0000    22 

                                     0000    23 ;++

                                     0000    24 ; FACILITY:

                                     0000    25 ;

                                     0000    26 ;	VAX/VMS RSX11M AME

                                     0000    27 ;

                                     0000    28 ; ABSTRACT:

                                     0000    29 ;

                                     0000    30 ;	CARD READER DRIVER

                                     0000    31 ;

                                     0000    32 ; AUTHOR: R.HEINEN 4-NOV-76

                                     0000    33 ;--

                                     0000    34 ;

                                     0000    35 ; EXTERNAL SYMBOLS

                                     0000    36 ;

                                     0000    37 	$RSXDEF			; DEFINE RSX SYMBOLS

                                     0000    38 	SPCIO$			; DEFINE SPECIAL I/O FUNCTIONS

                                     0000    39 	FILIO$			;

RSXCRDRV        - VAX/VMS RSX11M AME CARD READER DRIVER          22-AUG-1978 05:13:49   VAX-11 MACRO X0.3-11               Page   2

V06.0           RSX$CR_DRV - RSX11M AME CARD READER DRIVER                                                                       (2)



                                     0000    41 	.SBTTL	RSX$CR_DRV - RSX11M AME CARD READER DRIVER

                                     0000    42  

                                     0000    43 ;++

                                 00000000    44 	.PSECT	RSXCODE,NOWRT,SHR,PIC

                                     0000    45 ; RSX$CR_DRV - RSX11M AME CARD READER DRIVER 

                                     0000    46 ;

                                     0000    47 ; FUNCTIONAL DESCRIPTION:

                                     0000    48 ;

                                     0000    49 ; THIS ROUTINE PROCESSES I/O DIRECTED TO A CARD READER.

                                     0000    50 ;

                                     0000    51 ; INPUTS:

                                     0000    52 ;

                                     0000    53 ;	R2 = ADDRESS OF THE QIO CONTEXT BLOCK

                                     0000    54 ;	R3 = MAJOR FUNCTION CODE

                                     0000    55 ;	R5 = ADDRESS OF THE DPB AREA

                                     0000    56 ;	R6 = ADDRESS OF THE IMAGE STACK

                                     0000    57 ;	R8 = ADDRESS OF THE LUT

                                     0000    58 ;	R10 = ADDRESS OF THE IMAGE IMPURE SECTION

                                     0000    59 ;	R11 = ADDRESS OF THE IMAGE

                                     0000    60 ;

                                     0000    61 ; OUTPUTS:

                                     0000    62 ;

                                     0000    63 ;	R2,R6,R8,R10,R11 ARE PRESERVED

                                     0000    64 ;--

                                     0000    65 RSX$CR_DRV::				; CARD READER DRIVER

                                     0000    66 	CASE	R3,<-			;

                                     0000    67 		RSX$IOKILL,-		; I/O KILL

                                     0000    68 		RSX$IEIFC,-		; WRITE LOGICAL BLOCK

                                     0000    69 		CR_RLB,-		; READ LOGICAL BLOCK

                                     0000    70 		RSX$DLVRQIOAST,-	; ATTACH DEVICE

                                     0000    71 		RSX$DLVRQIOAST,-	; DETACH DEVICE

                                     0000    72 		RSX$IEIFC,-		; FUNCTION CODE 5

                                     0000    73 		RSX$IEIFC,-		; FUNCTION CODE 6

                                     0000    74 		RSX$IEIFC,-		; ILLEGAL

                                     0000    75 		RSX$IEIFC,-		; ILLEGAL

                                     0000    76 		RSX$DLVRQIOAST,-	; FUNCTION CODE 9

                                     0000    77 		RSX$IEIFC,-		; ILLEGAL

                                     0000    78 		RSX$DLVRQIOAST,-	; ACP FUNCTIONS

                                     0000    79 		RSX$DLVRQIOAST,-	; ACP FUNCTIONS

                                     0000    80 		RSX$DLVRQIOAST,-	; ACP FUNCTIONS

                                     0000    81 		RSX$DLVRQIOAST,-	; ACP FUNCTIONS

                                     0000    82 		RSX$DLVRQIOAST,-	; ACP FUNCTIONS

                                     0000    83 		RSX$DLVRQIOAST,-	; ACP FUNCTIONS

                                     0000    84 		CR_RLB,-		; READ VIRTUAL BLOCK

                                     0000    85 		RSX$IEIFC,-		; WRITE VIRTUAL BLOCK

                                     0000    86 		RSX$DLVRQIOAST,-	; ACP FUNCTIONS

                                     0000    87 		RSX$DLVRQIOAST,-	; ACP FUNCTIONS

                                     0000    88 		RSX$DLVRQIOAST,-	; ACP FUNCTIONS

                                     0000    89 		RSX$DLVRQIOAST,-	; ACP FUNCTIONS

                                     0000    90 		RSX$DLVRQIOAST,-	; ACP FUNCTIONS

                                     0000    91 		RSX$DLVRQIOAST,-	; ACP FUNCTIONS

                                     0000    92 		>

                          FFC7'  31  0036    93 	BRW	RSX$IEIFC		; ERROR EXIT

RSXCRDRV        - VAX/VMS RSX11M AME CARD READER DRIVER          22-AUG-1978 05:13:49   VAX-11 MACRO X0.3-11               Page   3

V06.0           CR_RVB AND CR_RLB FUNCTIONS                                                                                      (3)



                                     0039    95 	.SBTTL	CR_RVB AND CR_RLB FUNCTIONS

                                     0039    96 ;

                                     0039    97 ; READ VIRTUAL BLOCK

                                     0039    98 ;

                                     0039    99 CR_RVB:					; READ VIRTUAL BLOCK

         34 AA       0000'8F     3C  0039   100 	MOVZWL	#IO$_READVBLK,I_SCRATCH+12(R10); SET FUNCTION CODE

                          FFBE'  31  003F   101 	BRW	RSX$ISSUQIO		; PERFORM THE I/O

                                     0042   102 ;

                                     0042   103 ; READ LOGICAL BLOCK

                                     0042   104 ;

                                     0042   105 CR_RLB:					; READ LOGICAL BLOCK

         34 AA       0000'8F     3C  0042   106 	MOVZWL	#IO$_READLBLK,I_SCRATCH+12(R10); SET THE FUNCTION CODE

       0080 8F            57     B1  0048   107 	CMPW	R7,#<IO.RDB&^X0FF>	; IO.RDB?

                          06     12  004D   108 	BNEQ	10$			; IF NEQ THEN NO

         34 AA       0000'8F     A8  004F   109 	BISW	#IO$M_BINARY,I_SCRATCH+12(R10); SET READ BINARY

                          FFA8'  31  0055   110 10$:	BRW	RSX$ISSUQIO		; PERFORM THE FUNCTION

                                     0058   111 	.END

RSXCRDRV        - VAX/VMS RSX11M AME CARD READER DRIVER          22-AUG-1978 05:13:49   VAX-11 MACRO X0.3-11               Page   4

SYMBOL TABLE                                                                                                                     (3)



$$MSG          = 00000000            H.ISP            00000010            IE.ILL         = FFFFFFD6            

...GBL         = 00000000            H.LUN            0000003E            IE.ISQ         = FFFFFFC3            

ACBC_CTLRCAST  = 00000002            H.NLUN           0000003C            IE.LCK         = FFFFFFE5            

ACBC_FLOATAST  = 00000003            H.NML            00000031            IE.MOD         = FFFFFFEB            

ACBC_PWRAST    = 00000000            H.ODVA           00000012            IE.NBF         = FFFFFFD9            

ACBC_RCVAST    = 00000001            H.ODVL           00000014            IE.NBK         = FFFFFFD7            

ACBV_INPROG    = 00000001            H.OVLY           0000002C            IE.NDR         = FFFFFFB8            

ACBV_PERM      = 00000000            H.PFVA           0000001A            IE.NFI         = FFFFFFC4            

ACBV_TYPE      = 00000008            H.RCVA           0000001E            IE.NFW         = FFFFFFBB            

ACB_FLAGS        0000000C            H.RRVA           00000032            IE.NLK         = FFFFFFB1            

ACB_LINK         00000000            H.SPRI           00000030            IE.NLN         = FFFFFFDB            

ACB_UPC          0000000A            H.TKVA           00000016            IE.NNC         = FFFFFFB3            

ACB_UPRM         00000008            H.TKVL           00000018            IE.NNL         = FFFFFFB2            

ADR_HIGHLIM      00000004            H.VEXT           0000002E            IE.NNN         = FFFFFFBC            

ADR_LOWLIM       00000000            H.WND            00000024            IE.NOD         = FFFFFFE9            

ADR_SIZE         00000008            IE.2DV         = FFFFFFD0            IE.NSF         = FFFFFFE6            

AP_NAME          00000004            IE.ABO         = FFFFFFF1            IE.NST         = FFFFFFB0            

AST_PARAM        00000004            IE.ALC         = FFFFFFAC            IE.OFL         = FFFFFFBF            

AST_PC           00000010            IE.ALN         = FFFFFFDE            IE.ONP         = FFFFFFFB            

AST_PSL          00000014            IE.AST         = FFFFFFB0            IE.OVR         = FFFFFFEE            

AST_R0           00000008            IE.BAD         = FFFFFFFF            IE.PES         = FFFFFFAD            

AST_R1           0000000C            IE.BBE         = FFFFFFC8            IE.PRI         = FFFFFFF0            

BIT...         = 0006809C            IE.BCC         = FFFFFFBE            IE.RAC         = FFFFFFD4            

CR_RLB           00000042 R     05   IE.BDI         = FFFFFFCC            IE.RAT         = FFFFFFD3            

CR_RVB           00000039 R     05   IE.BDR         = FFFFFFCE            IE.RBG         = FFFFFFD8            

C_CANONPS      = 83C00000            IE.BDV         = FFFFFFC9            IE.RCN         = FFFFFFD2            

C_RCVDSTR      = 44564352            IE.BHD         = FFFFFFC0            IE.RER         = FFFFFFE0            

FCB_ATTRIBS      0000007C            IE.BLB         = FFFFFFBA            IE.RNM         = FFFFFFCD            

FCB_FIB          0000004C            IE.BLK         = FFFFFFEC            IE.RSU         = FFFFFFEF            

FCB_FID          00000000            IE.BNM         = FFFFFFCA            IE.SNC         = FFFFFFDD            

FCB_FNAME        00000014            IE.BTF         = FFFFFFB4            IE.SPC         = FFFFFFFA            

FCB_FNAMEDESC    0000000C            IE.BTP         = FFFFFFD5            IE.SQC         = FFFFFFDC            

FCB_FNB          00000002            IE.BVR         = FFFFFFC1            IE.SRE         = FFFFFFF2            

FCB_PC           00000078            IE.BYT         = FFFFFFED            IE.STK         = FFFFFFC6            

FCB_RESULT       00000030            IE.CKS         = FFFFFFE2            IE.TMM         = FFFFFFB9            

FCB_RESULTDESC   00000004            IE.CLO         = FFFFFFDA            IE.TMO         = FFFFFFB6            

FCB_SIZE         000000B4            IE.CNR         = FFFFFFB7            IE.ULK         = FFFFFFAB            

FP_AP            00000008            IE.CON         = FFFFFFEA            IE.VER         = FFFFFFFC            

FP_FP            0000000C            IE.DAA         = FFFFFFF8            IE.WAC         = FFFFFFE3            

FP_PC            00000010            IE.DAO         = FFFFFFF3            IE.WAT         = FFFFFFE1            

FP_PSL           00000004            IE.DFU         = FFFFFFE8            IE.WCK         = FFFFFFAA            

FP_REGISTERS     00000014            IE.DNA         = FFFFFFF9            IE.WER         = FFFFFFDF            

GBL...         = 00000000            IE.DNR         = FFFFFFFD            IE.WLK         = FFFFFFF4            

H.CSP            00000000            IE.DUN         = FFFFFFF7            IO$M_BINARY      ********   X   05   

H.CUIC           00000008            IE.DUP         = FFFFFFC7            IO$_READLBLK     ********   X   05   

H.DSW            00000026            IE.EOF         = FFFFFFF6            IO$_READVBLK     ********   X   05   

H.DUIC           0000000A            IE.EOT         = FFFFFFC2            IO.ACE         = 00000F00            

H.EFLM           00000004            IE.EOV         = FFFFFFF5            IO.ACR         = 00000D00            

H.EFSV           00000020            IE.EXP         = FFFFFFB5            IO.ACW         = 00000E00            

H.FCS            00000028            IE.FEX         = FFFFFFCF            IO.ADS         = 00001800            

H.FORT           0000002A            IE.FHE         = FFFFFFC5            IO.APC         = 00001800            

H.FPSA           00000022            IE.FLN         = FFFFFFAF            IO.APV         = 00001808            

H.FPVA           0000001C            IE.FOP         = FFFFFFCB            IO.ATA         = 00000308            

H.GARD           0000003A            IE.HFU         = FFFFFFE4            IO.ATT         = 00000300            

H.HDLN           00000002            IE.IES         = FFFFFFAE            IO.CAS         = 00001B10            

H.IPC            0000000E            IE.IFC         = FFFFFFFE            IO.CBO         = 00001B48            

H.IPS            0000000C            IE.IFU         = FFFFFFE7            IO.CCI         = 00001800            

RSXCRDRV        - VAX/VMS RSX11M AME CARD READER DRIVER          22-AUG-1978 05:13:49   VAX-11 MACRO X0.3-11               Page   5

SYMBOL TABLE                                                                                                                     (3)



IO.CCO         = 00000120            IO.MCS         = 00001700            IO.UEI         = 00001328            

IO.CIN         = 00001D40            IO.MDA         = 00001C00            IO.UER         = 00001320            

IO.CLK         = 00001A00            IO.MDI         = 00001900            IO.ULK         = 00000A00            

IO.CLN         = 00000700            IO.MDO         = 00001B00            IO.UNL         = 00000022            

IO.CNT         = 00001E00            IO.MLO         = 00000C00            IO.USI         = 00001330            

IO.CON         = 00001B00            IO.MOD         = 00000600            IO.UTI         = 00001310            

IO.CPR         = 00001B08            IO.MSO         = 00000A00            IO.UTY         = 00001318            

IO.CPW         = 00001D50            IO.NLB         = 00001D58            IO.WAL         = 00000108            

IO.CRC         = 00000220            IO.NLK         = 00001300            IO.WAT         = 00001700            

IO.CRE         = 00001400            IO.ONL         = 00001F00            IO.WBT         = 00000140            

IO.CRJ         = 00001B20            IO.R1C         = 00000500            IO.WDD         = 00000124            

IO.CSI         = 00001600            IO.RAD         = 00001100            IO.WLB         = 00000100            

IO.CSM         = 00001D38            IO.RAL         = 00000208            IO.WLC         = 00000110            

IO.CTI         = 00001B00            IO.RAT         = 00001600            IO.WLS         = 00000108            

IO.CTL         = 00001D00            IO.RBC         = 00000600            IO.WLT         = 00000108            

IO.CTR         = 00001B88            IO.RCI         = 00001A00            IO.WLV         = 00000140            

IO.CTY         = 00000700            IO.RCV         = 00001A00            IO.WMS         = 00000110            

IO.DAC         = 00001000            IO.RDB         = 00000280            IO.WNS         = 00000110            

IO.DCI         = 00001900            IO.RDD         = 00001008            IO.WPB         = 00000120            

IO.DEL         = 00001500            IO.RDN         = 00000012            IO.WVB         = 00001200            

IO.DET         = 00000400            IO.REL         = 00001700            IO.XMT         = 00001900            

IO.DIS         = 00001C00            IO.RHD         = 00000208            IO.XNA         = 00001908            

IO.DLB         = 00001D60            IO.RLB         = 00000200            IQ.Q           = 00000002            

IO.DSI         = 00001700            IO.RLV         = 00000240            IQ.S           = 00000004            

IO.DTI         = 00001C00            IO.RMT         = 00001010            IQ.UMD         = 00000004            

IO.DTY         = 00000D00            IO.RNA         = 00000B00            IQ.X           = 00000001            

IO.ENA         = 00000C00            IO.RNC         = 00000220            IS.BV          = 00000005            

IO.EOF         = 00000600            IO.RNE         = 00000210            IS.CC          = 00000301            

IO.EXT         = 00001300            IO.RNS         = 00000210            IS.CR          = 00000D01            

IO.FDX         = 00000610            IO.RPB         = 00000220            IS.EOT         = 00000401            

IO.FLN         = 00001500            IO.RPR         = 00000900            IS.ESC         = 00001B01            

IO.FNA         = 00000900            IO.RST         = 00000201            IS.ESQ         = 00009B01            

IO.GLC         = 00001D18            IO.RTC         = 00000700            IS.PES         = 00008001            

IO.GLI         = 00001D10            IO.RTI         = 00001D00            IS.PND         = 00000000            

IO.GNI         = 00001D08            IO.RTK         = 00000030            IS.RDD         = 00000002            

IO.GRC         = 00001D28            IO.RTM         = 00000280            IS.SUC         = 00000001            

IO.GRI         = 00001D20            IO.RVB         = 00001100            IS.TAB         = 00000901            

IO.GRN         = 00001D30            IO.RWD         = 00000500            IS.TMO         = 00000002            

IO.GTS         = 00000500            IO.RWU         = 00000560            I_ADR0           000000FC            

IO.HDX         = 00000608            IO.SAO         = 00000800            I_ASCIINAME      00000140            

IO.HIS         = 00001A00            IO.SCS         = 00001600            I_ASTPOOL        000000D0            

IO.HNG         = 00000600            IO.SDI         = 00001600            I_ASTQUEUE       000000C8            

IO.INI         = 00001900            IO.SDO         = 00001500            I_BAILOUTFP      00000188            

IO.INL         = 00000500            IO.SEC         = 00000550            I_CMDROUT        000000E8            

IO.ITI         = 00001E00            IO.SET         = 00000018            I_CURAST         00000198            

IO.KIL         = 0000000A            IO.SLO         = 00000B00            I_DEBVEC         00000190            

IO.LDI         = 00000E00            IO.SMO         = 00000570            I_DEBVECL        00000192            

IO.LED         = 00001400            IO.SPB         = 00000510            I_FCBPOOL        000000D8            

IO.LEI         = 00000F08            IO.SPF         = 00000520            I_FCC            000001B4            

IO.LKE         = 00001400            IO.SPW         = 00001D48            I_FLOATA0        000001C0            

IO.LOD         = 00001800            IO.SSO         = 00000900            I_FLOATA1        000001C8            

IO.LOV         = 00000208            IO.STA         = 00001B00            I_FLOATA2        000001D0            

IO.LSI         = 00001200            IO.STC         = 00000540            I_FLOATA3        000001D8            

IO.LTI         = 00000F00            IO.STP         = 00001D00            I_FLOATA4        000001E0            

IO.LTK         = 00000028            IO.SYN         = 00000620            I_FLOATA5        000001E8            

IO.LTY         = 00001000            IO.TRM         = 00000508            I_FLOATADR       000001B0            

IO.MAO         = 00000708            IO.UDI         = 00001308            I_FLOATAST       000001A4            

RSXCRDRV        - VAX/VMS RSX11M AME CARD READER DRIVER          22-AUG-1978 05:13:49   VAX-11 MACRO X0.3-11               Page   6

SYMBOL TABLE                                                                                                                     (3)



I_FLOATCSR       000001A8            PSL_CC         = 00000000            W.BLVR           00000002            

I_FLOATERR       000001AC            PSL_CM         = 0000001F            W.BNPD           0000000D            

I_FLOATTMP       000001B8            PSL_FPD        = 0000001B            W.BOFF           0000000A            

I_GARD           000000EC            PSL_FU         = 00000006            W.BPCB           00000000            

I_HIGHEFN        0000016C            PSL_TBIT       = 00000004            W.BSIZ           00000008            

I_HIGHSIZE       000000F4            QIOV_FILES     = 00000000            

I_IMAGEVBN       000000F8            QIO_FLAGS        0000001A            

I_INISIZE        000000F0            QIO_IOSB         0000000E            

I_LENGTH         000001F0            QIO_LUT          00000016            

I_LOGNAME        000000E0            QIO_SECONDBLK    0000001C            

I_LUT            00000168            QIO_SIZE         00000020            

I_NLUN           00000164            RSX$CR_DRV       00000000 RG    05   

I_PC             00000020            RSX$C_SUBSYSTEM= 00000006            

I_PPFINDEX       00000162            RSX$DLVRQIOAST   ********   X   05   

I_PROCNAME       0000014C            RSX$IEIFC        ********   X   05   

I_PS             00000024            RSX$IOKILL       ********   X   05   

I_PWRAST         000001A0            RSX$ISSUQIO      ********   X   05   

I_R0             00000000            RSX$_ACCVIO    = 00068044            

I_R1             00000004            RSX$_BADLIBREF = 0006806C            

I_R2             00000008            RSX$_BADSTACK  = 0006804C            

I_R3             0000000C            RSX$_BREAK     = 0006800C            

I_R4             00000010            RSX$_EXITSTATUS= 00068640            

I_R5             00000014            RSX$_EXTERNABRT= 0006805C            

I_R6             00000018            RSX$_ILLINST   = 0006802C            

I_RAD50NAME      00000148            RSX$_IMAGETERM = 00068084            

I_RCVAST         0000019C            RSX$_INSFDYNMEM= 00068054            

I_RCVMAIL        00000160            RSX$_IOT       = 00068014            

I_RUNFLAGS       0000018C            RSX$_LIBNOTFND = 00068074            

I_SCRATCH        00000028            RSX$_LOADERROR = 0006807C            

I_SSTVEC         00000194            RSX$_NOCOMM    = 00068094            

I_SSTVECL        00000196            RSX$_NONRSXEMT = 0006801C            

I_STATE          00000170            RSX$_NOPMD     = 00068332            

I_TYPE           0000001C            RSX$_NOSUCHDEV = 00068322            

I_UIC            0000013C            RSX$_NOTSKIMG  = 00068064            

I_WAIT           00000178            RSX$_ODDADDR   = 00068034            

I_WAITSAVE       00000180            RSX$_PMD       = 0006832A            

LUTC_CR        = 00000005            RSX$_RCVMBXSIZ = 0000012C            

LUTC_DISK      = 00000002            RSX$_REGMSG    = 0006808C            

LUTC_LP        = 00000004            RSX$_RESERVED  = 00068004            

LUTC_RMS       = 00000000            RSX$_TBIT      = 0006803C            

LUTC_TAPE      = 00000003            RSX$_TRAP      = 00068024            

LUTC_TRM       = 00000001            RSX$_VERIFYCMD = 00068648            

LUTV_CTRLC     = 00000002            SV_ASTLVL        00000004            

LUTV_CTRLO     = 00000000            SV_DCL           00000002            

LUTV_PRM       = 00000003            SV_FLOATAST      00000009            

LUT_CHAN         0000000C            SV_NOAST         00000003            

LUT_CHAR         00000012            SV_PENDWAIT      00000005            

LUT_CTRLC        00000032            SV_PWRAST        00000008            

LUT_FLAGS        0000000A            SV_RCVAST        00000007            

LUT_INFONAME     0000002E            SV_RESTORE       00000000            

LUT_INFOUNIT     00000030            SV_TRANSLATE     00000001            

LUT_LINK         00000000            SV_WAIT          00000006            

LUT_REALNAME     0000001E            W.BATT           00000006            

LUT_REF          00000008            W.BFPD           0000000C            

LUT_RSXNAME      00000010            W.BHVR           00000004            

LUT_SIZE         00000036            W.BLGH           00000010            

LUT_TYPE         00000016            W.BLPD           0000000E            

RSXCRDRV        - VAX/VMS RSX11M AME CARD READER DRIVER          22-AUG-1978 05:13:49   VAX-11 MACRO X0.3-11               Page   7

PROGRAM SECTION SYNOPSIS                                                                                                         (3)







PROGRAM SECTION SYNOPSIS



.  ABS  .        00000000      00     NOPIC   USR   CON   ABS   LCL NOSHR NOEXE NORD  NOWRT BYTE  

. BLANK .        00000000      01     NOPIC   USR   CON   REL   LCL NOSHR   EXE   RD    WRT BYTE  

..ABS.           00000042      02     NOPIC   USR   CON   ABS   LCL NOSHR   EXE   RD    WRT BYTE  

$ABS$            00000000      03     NOPIC   USR   CON   ABS   LCL NOSHR   EXE   RD    WRT BYTE  

RSXDEF           000001F4      04     NOPIC   USR   CON   ABS   LCL NOSHR   EXE   RD    WRT BYTE  

RSXCODE          00000058      05       PIC   USR   CON   REL   LCL   SHR   EXE   RD  NOWRT BYTE  





THERE WERE NO ERRORS OR WARNINGS.

12982. BYTES LEFT IN FREE MEMORY POOL.

3056. BYTES OF RECLAIMED MEMORY.

OBJ$:RSXCRDRV,LIS$:RSXCRDRV/-SP=EXECML$/ML,LIB$:R/ML,SRC$:RSXCRDRV

19 MLB DIR RDS - 589 GETS TO DEFINE 17 MACROS. 16 INTER. FILE WRITES. 

