IOPERFORM                                                        22-AUG-1978 00:13:43   VAX-11 MACRO X0.3-11               Page   0

TABLE OF CONTENTS   



   (1)      46  DECLARATIONS

   (1)      64  DUMMY ROUTINES FOR I/O PERFORMANCE MEASUREMENT

IOPERFORM                                                        22-AUG-1978 00:13:43   VAX-11 MACRO X0.3-11               Page   1

00                                                                                                                               (1)



                                     0000     1 	.TITLE	IOPERFORM

                                     0000     2 	.IDENT	/00/

                                     0000     3 

                                     0000     4 ;

                                     0000     5 ;			  COPYRIGHT (c) 1977 BY

                                     0000     6 ;	      DIGITAL EQUIPMENT CORPORATION, MAYNARD, MASS.

                                     0000     7 ;

                                     0000     8 ; THIS SOFTWARE IS FURNISHED UNDER A LICENSE AND MAY BE USED AND  COPIED

                                     0000     9 ; ONLY  IN  ACCORDANCE  WITH  THE  TERMS  OF  SUCH  LICENSE AND WITH THE

                                     0000    10 ; INCLUSION OF THE ABOVE COPYRIGHT NOTICE.  THIS SOFTWARE OR  ANY  OTHER

                                     0000    11 ; COPIES  THEREOF MAY NOT BE PROVIDED OR OTHERWISE MADE AVAILABLE TO ANY

                                     0000    12 ; OTHER PERSON.  NO TITLE TO AND OWNERSHIP OF  THE  SOFTWARE  IS  HEREBY

                                     0000    13 ; TRANSFERRED.

                                     0000    14 ;

                                     0000    15 ; THE INFORMATION IN THIS SOFTWARE IS SUBJECT TO CHANGE  WITHOUT  NOTICE

                                     0000    16 ; AND  SHOULD  NOT  BE  CONSTRUED  AS  A COMMITMENT BY DIGITAL EQUIPMENT

                                     0000    17 ; CORPORATION.

                                     0000    18 ;

                                     0000    19 ; DIGITAL ASSUMES NO RESPONSIBILITY FOR THE USE OR  RELIABILITY  OF  ITS

                                     0000    20 ; SOFTWARE ON EQUIPMENT WHICH IS NOT SUPPLIED BY DIGITAL.

                                     0000    21 ;

                                     0000    22 

                                     0000    23 ;++

                                     0000    24 ; FACILITY:

                                     0000    25 ;

                                     0000    26 ;	STAND-ALONE EXECUTIVE FOR THE DSC UTILITY

                                     0000    27 ;

                                     0000    28 ; ABSTRACT:

                                     0000    29 ;

                                     0000    30 ;	THESE DUMMY ROUTINES REPLACE THE I/O PERFORMANCE MEASUREMENT

                                     0000    31 ;	SUBROUTINES FOR THE STAND-ALONE SYSTEM

                                     0000    32 ;

                                     0000    33 ;

                                     0000    34 ; ENVIRONMENT:

                                     0000    35 ;

                                     0000    36 ;	STAND-ALONE EXECUTIVE KERNAL MODE

                                     0000    37 ;

                                     0000    38 ; AUTHOR: C. A. MONIA	, CREATION DATE: 24-JAN-1978

                                     0000    39 ;

                                     0000    40 ; MODIFIED BY:

                                     0000    41 ;

                                     0000    42 ;	, : VERSION

                                     0000    43 ; 01	- 

                                     0000    44 ;--

IOPERFORM                                                        22-AUG-1978 00:13:43   VAX-11 MACRO X0.3-11               Page   2

00              DECLARATIONS                                                                                                     (1)



                                     0000    46 	.SBTTL	DECLARATIONS

                                     0000    47 ;

                                     0000    48 ; INCLUDE FILES:

                                     0000    49 ;

                                     0000    50 

                                     0000    51 ;

                                     0000    52 ; MACROS:

                                     0000    53 ;

                                     0000    54 

                                     0000    55 ;

                                     0000    56 ; EQUATED SYMBOLS:

                                     0000    57 ;

                                     0000    58 

                                     0000    59 ;

                                     0000    60 ; OWN STORAGE:

                                     0000    61 ;

                                     0000    62 

IOPERFORM                                                        22-AUG-1978 00:13:43   VAX-11 MACRO X0.3-11               Page   3

00              DUMMY ROUTINES FOR I/O PERFORMANCE MEASUREMENT                                                                   (1)



                                     0000    64 	.SBTTL	DUMMY ROUTINES FOR I/O PERFORMANCE MEASUREMENT

                                     0000    65 ;++

                                     0000    66 ; FUNCTIONAL DESCRIPTION:

                                     0000    67 ;

                                     0000    68 ;	THE FOLLOWING ENTRY POINTS FOR PERFORMANCE MEASUREMENT ARE REPLACED:

                                     0000    69 ;

                                     0000    70 ;		PMS$END_IO

                                     0000    71 ;		PMS$END_RQ

                                     0000    72 ;		PMS$START_IO

                                     0000    73 ;		PMS$START_RQ

                                     0000    74 ;

                                     0000    75 ;

                                     0000    76 ; CALLING SEQUENCE:

                                     0000    77 ;

                                     0000    78 ;	BSBW	ENTRY

                                     0000    79 ;

                                     0000    80 ; INPUT PARAMETERS:

                                     0000    81 ;

                                     0000    82 ;	NONE

                                     0000    83 ;

                                     0000    84 ; IMPLICIT INPUTS:

                                     0000    85 ;

                                     0000    86 ;	NONE

                                     0000    87 ;

                                     0000    88 ; OUTPUT PARAMETERS:

                                     0000    89 ;

                                     0000    90 ;	NONE

                                     0000    91 ;

                                     0000    92 ; IMPLICIT OUTPUTS:

                                     0000    93 ;

                                     0000    94 ;	NONE

                                     0000    95 ;

                                     0000    96 ; COMPLETION CODES:

                                     0000    97 ;

                                     0000    98 ;	NONE

                                     0000    99 ;

                                     0000   100 ; SIDE EFFECTS:

                                     0000   101 ;

                                     0000   102 ;	NONE

                                     0000   103 ;

                                     0000   104 ;--

                                     0000   105  

                                 00000000   106 	.PSECT	$AEXENONPAGED

                                     0000   107  

                                     0000   108 PMS$END_IO::				; DUMMY ENTRY POINTS

                                     0000   109 PMS$END_RQ::				; ....

                                     0000   110 PMS$START_IO::				; ....

                                     0000   111 PMS$START_RQ::				; ....

                                 05  0000   112 	RSB

                                     0001   113 

                                     0001   114 	.END

IOPERFORM                                                        22-AUG-1978 00:13:43   VAX-11 MACRO X0.3-11               Page   4

SYMBOL TABLE                                                                                                                     (1)



PMS$END_IO       00000000 RG    02   

PMS$END_RQ       00000000 RG    02   

PMS$START_IO     00000000 RG    02   

PMS$START_RQ     00000000 RG    02   





PROGRAM SECTION SYNOPSIS



.  ABS  .        00000000      00     NOPIC   USR   CON   ABS   LCL NOSHR NOEXE NORD  NOWRT BYTE  

. BLANK .        00000000      01     NOPIC   USR   CON   REL   LCL NOSHR   EXE   RD    WRT BYTE  

$AEXENONPAGED    00000001      02     NOPIC   USR   CON   REL   LCL NOSHR   EXE   RD    WRT BYTE  





THERE WERE NO ERRORS OR WARNINGS.

28474. BYTES LEFT IN FREE MEMORY POOL.

OBJ$:IOPERFORM,LIS$:IOPERFORM/-SP=LIB$:LIB/ML,SRC$:IOPERFORM

0 MLB DIR RDS - 0 GETS TO DEFINE 0 MACROS. 1 INTER. FILE WRITES. 

