NETOPCOM        - OPERATOR COMMUNICATIONS                        22-AUG-1978 00:58:24   VAX-11 MACRO X0.3-11               Page   0

TABLE OF CONTENTS   



   (1)    3400  HISTORY

   (1)    4200  DECLARATIONS

   (1)   15500  NETWORK OPERATOR MESSAGE FORMATTING

NETOPCOM        - OPERATOR COMMUNICATIONS                        22-AUG-1978 00:58:24   VAX-11 MACRO X0.3-11               Page   1

X01                                                                                                                              (1)



                                     0000   100 

                                     0000   200 	.TITLE	NETOPCOM - OPERATOR COMMUNICATIONS

                                     0000   300 	.IDENT	/X01/

                                     0000   400 

                                     0000   500 ;

                                     0000   600 ; COPYRIGHT (C) 1978

                                     0000   700 ; DIGITAL EQUIPMENT CORPORATION, MAYNARD, MASSACHUSETTS 01754

                                     0000   800 ;

                                     0000   900 ; THIS SOFTWARE IS FURNISHED  UNDER A LICENSE FOR USE ONLY ON A SINGLE

                                     0000  1000 ; COMPUTER  SYSTEM AND  MAY BE  COPIED ONLY WITH  THE INCLUSION OF THE

                                     0000  1100 ; ABOVE COPYRIGHT NOTICE.  THIS SOFTWARE, OR ANY OTHER COPIES THEREOF,

                                     0000  1200 ; MAY NOT BE PROVIDED OR  OTHERWISE MADE AVAILABLE TO ANY OTHER PERSON

                                     0000  1300 ; EXCEPT FOR USE ON SUCH SYSTEM AND TO ONE WHO AGREES TO THESE LICENSE

                                     0000  1400 ; TERMS.  TITLE TO AND  OWNERSHIP OF THE  SOFTWARE  SHALL AT ALL TIMES

                                     0000  1500 ; REMAIN IN DEC.

                                     0000  1600 ;

                                     0000  1700 ; THE INFORMATION IN THIS SOFTWARE IS SUBJECT TO CHANGE WITHOUT NOTICE

                                     0000  1800 ; AND SHOULD  NOT BE CONSTRUED  AS A COMMITMENT  BY DIGITAL  EQUIPMENT

                                     0000  1900 ; CORPORATION.

                                     0000  2000 ;

                                     0000  2100 ; DEC ASSUMES  NO  RESPONSIBILITY  FOR  THE USE OR  RELIABILITY OF ITS

                                     0000  2200 ; SOFTWARE ON EQUIPMENT WHICH IS NOT SUPPLIED BY DEC.

                                     0000  2300 

                                     0000  2400 ;++

                                     0000  2500 ; FACILITY:	NETWORK ACP

                                     0000  2600 ;

                                     0000  2700 ; ABSTRACT:

                                     0000  2800 ;	THIS MODULE IS USED TO SEND INFORMATIONAL MESSAGES TO THE NETWORK OPERATOR

                                     0000  2900 ;

                                     0000  3000 ; ENVIRONMENT:

                                     0000  3100 ;	MODE = EXEC

                                     0000  3200 ;--

NETOPCOM        - OPERATOR COMMUNICATIONS                        22-AUG-1978 00:58:24   VAX-11 MACRO X0.3-11               Page   2

X01             HISTORY                                                                                                          (1)



                                     0000  3400 	.SBTTL	HISTORY

                                     0000  3500 ; AUTHOR:	SCOTT G. DAVIS, CREATION DATE: 13-APR-1978

                                     0000  3600 ;

                                     0000  3700 ; MODIFIED BY:

                                     0000  3800 ;

                                     0000  3900 ;	, : VERSION

                                     0000  4000 ; 01	- 

NETOPCOM        - OPERATOR COMMUNICATIONS                        22-AUG-1978 00:58:24   VAX-11 MACRO X0.3-11               Page   3

X01             DECLARATIONS                                                                                                     (1)



                                     0000  4200 	.SBTTL	DECLARATIONS

                                     0000  4300 ;

                                     0000  4400 ; INCLUDE FILES:

                                     0000  4500 ;

                                     0000  4600 	$MSGDEF

                                     0000  4700 	$NDBDEF

                                     0000  4800 	$OPCDEF

                                     0000  4900 

                                     0000  5000 ;

                                     0000  5100 ; MACROS:

                                     0000  5200 ;

                                     0000  5300 

                                     0000  5400 ;

                                     0000  5500 ; EQUATED SYMBOLS:

                                     0000  5600 ;

                           00000050  0000  5700 TEXT_LTH = 80

                                     0000  5800 

                                     0000  5900 ;

                                     0000  6000 ; OWN STORAGE:

                                     0000  6100 ;

                                 00000000  6200 	.PSECT	NET_PURE,NOWRT,NOEXE

                                     0000  6300 

                                     0000  6400 ;

                                     0000  6500 ; MESSAGES

                                     0000  6600 ;

         67 6E 69 74 72 61 74 73 00' 0000  6700 START_MSG:	.ASCIC	/starting/

                                 08  0000       

69 61 6D 20 64 65 72 65 74 6E 65 00' 0009  6800 MAINT_MSG:	.ASCIC	/entered maintenance mode/

64 6F 6D 20 65 63 6E 61 6E 65 74 6E  0015       

                                 65  0021       

                                 18  0009       

      6E 77 6F 64 20 74 6E 65 77 00' 0022  6900 DOWN_MSG:	.ASCIC	/went down/

                                 09  0022       

6E 61 20 64 65 76 69 65 63 65 72 00' 002C  7000 NGINI_MSG:	.ASCIC	/received an invalid node init/

64 6F 6E 20 64 69 6C 61 76 6E 69 20  0038       

                  74 69 6E 69 20 65  0044       

                                 1D  002C       

20 61 20 64 65 76 69 65 63 65 72 00' 004A  7100 OKINI_MSG:	.ASCIC	/received a valid node init/

69 20 65 64 6F 6E 20 64 69 6C 61 76  0056       

                           74 69 6E  0062       

                                 1A  004A       

6F 64 20 67 6E 69 74 74 75 68 73 00' 0065  7200 SHUT_MSG:	.ASCIC	/shutting down/

                              6E 77  0071       

                                 0D  0065       

6F 20 52 53 44 20 61 20 64 61 68 00' 0073  7300 DSRCH_MSG:	.ASCIC	/had a DSR on-to-off transition/

61 72 74 20 66 66 6F 2D 6F 74 2D 6E  007F       

               6E 6F 69 74 69 73 6E  008B       

                                 1E  0073       

79 6C 74 63 65 72 72 6F 63 6E 69 00' 0092  7400 LOOPB_MSG:	.ASCIC	/incorrectly looped back/

6B 63 61 62 20 64 65 70 6F 6F 6C 20  009E       

                                 17  0092       

72 65 20 64 65 64 65 65 63 78 65 00' 00AA  7500 DCHK_MSG:	.ASCIC	/exceeded error threshold/

6C 6F 68 73 65 72 68 74 20 72 6F 72  00B6       

                                 64  00C2       

                                 18  00AA       

                                     00C3  7600 

                                     00C3  7700 MSG_ARRAY:				; MESSAGE ADDRESSES

NETOPCOM        - OPERATOR COMMUNICATIONS                        22-AUG-1978 00:58:24   VAX-11 MACRO X0.3-11               Page   4

X01             DECLARATIONS                                                                                                     (1)



                           00000000' 00C3  7800 	.LONG	START_MSG

                           00000001  00C7  7900 MSGNUM=<.-MSG_ARRAY>/4

                                     00C7  8000 	ASSUME	MSGNUM EQ NDB$C_MSG_START

                                     00C7  8100 

                           00000009' 00C7  8200 	.LONG	MAINT_MSG

                           00000002  00CB  8300 MSGNUM=<.-MSG_ARRAY>/4

                                     00CB  8400 	ASSUME	MSGNUM EQ NDB$C_MSG_MAINT

                                     00CB  8500 

                           00000022' 00CB  8600 	.LONG	DOWN_MSG

                           00000003  00CF  8700 MSGNUM=<.-MSG_ARRAY>/4

                                     00CF  8800 	ASSUME	MSGNUM EQ NDB$C_MSG_DOWN

                                     00CF  8900 

                           0000002C' 00CF  9000 	.LONG	NGINI_MSG

                           00000004  00D3  9100 MSGNUM=<.-MSG_ARRAY>/4

                                     00D3  9200 	ASSUME	MSGNUM EQ NDB$C_MSG_NGINI

                                     00D3  9300 

                           0000004A' 00D3  9400 	.LONG	OKINI_MSG

                           00000005  00D7  9500 MSGNUM=<.-MSG_ARRAY>/4

                                     00D7  9600 	ASSUME	MSGNUM EQ NDB$C_MSG_OKINI

                                     00D7  9700 

                           00000065' 00D7  9800 	.LONG	SHUT_MSG

                           00000006  00DB  9900 MSGNUM=<.-MSG_ARRAY>/4

                                     00DB 10000 	ASSUME	MSGNUM EQ NDB$C_MSG_SHUT

                                     00DB 10100 

                           00000073' 00DB 10200 	.LONG	DSRCH_MSG

                           00000007  00DF 10300 MSGNUM=<.-MSG_ARRAY>/4

                                     00DF 10400 	ASSUME	MSGNUM EQ NDB$C_MSG_DSRCH

                                     00DF 10500 

                           00000092' 00DF 10600 	.LONG	LOOPB_MSG

                           00000008  00E3 10700 MSGNUM=<.-MSG_ARRAY>/4

                                     00E3 10800 	ASSUME	MSGNUM EQ NDB$C_MSG_LOOPB

                                     00E3 10900 

                                     00E3 11000 

                           000000AA' 00E3 11100 	.LONG	DCHK_MSG

                           00000009  00E7 11200 MSGNUM=<.-MSG_ARRAY>/4

                                     00E7 11300 	ASSUME	MSGNUM EQ NDB$C_MSG_DCHK

                                     00E7 11400 

                                 00000000 11500 	.PSECT	NET_IMPURE,WRT,NOEXE

                                     0000 11600 

                           00000008  0000 11700 MSG_DESC:	.BLKQ	1		; MESSAGE DESCRIPTOR FOR ERROR LOGGER

                                     0008 11800 MSG_BUFFER:

                           00000008  0008 11900 	.LONG	MSG$_OPRQST		; MSG TYPE + MAILBOX CHANNEL

                           FFFFFFFF  000C 12000 	.LONG	-1			; PRIVILEGES

                           FFFFFFFF  0010 12100 	.LONG	-1			; MORE PRIVILEGES

                           00000000  0014 12200 	.LONG	0			; UIC

20 20 20 20 20 20 50 43 41 54 45 4E  0018 12300 	.ASCII	/NETACP      /		; MY NAME

            20 20 20 20 20 20 20 20  0024 12400 	.ASCII	/        /		; ACCOUNT - NULL

                               0000  002C 12500 	.WORD	0			; PRIORITY + FILL BYTE

                           00004103  002E 12600 	.LONG	OPC$_RQ_RQST!-		; SET UP BUFFER HEADER

                                     0032 12700 	<<OPC$M_NM_NTWORK!OPC$M_NM_CENTRL>@8>

                           00000000  0032 12800 	.LONG	0			; NO MESSAGE NO. FOR REPLY

                                     0036 12900 

                                     0036 13000 TEXT:

                           00000086  0036 13100 	.BLKB	TEXT_LTH		; FOR REST OF TEXT

                           0000008A  0086 13200 TEXT_DESC:	.BLKL	1		; LTH OF TEXT BFR

                           00000036' 008A 13300 	.LONG	TEXT			; BFR ADDR

                                     008E 13400 

NETOPCOM        - OPERATOR COMMUNICATIONS                        22-AUG-1978 00:58:24   VAX-11 MACRO X0.3-11               Page   5

X01             DECLARATIONS                                                                                                     (1)



                           00000015' 008E 13500 LINE_DESC:	.LONG	LINE_LTH	; LINE MESSAGE DESCRIPTOR

                           00000096' 0092 13600 		.LONG	LINE_CTRSTR	;

20 65 6E 69 6C 20 74 65 6E 43 45 44  0096 13700 LINE_CTRSTR:	.ASCII	/DECnet line /

                           000000A6  00A2 13800 LINE_NAME:	.BLKL	1		; FOR JAMMING LINE NAME

                     43 41 21 20 3A  00A6 13900 		.ASCII	/: !AC/		; REST OF CONTROL STRING

                           00000015  00AB 14000 LINE_LTH=.-LINE_CTRSTR

                                     00AB 14100 

                           0000000A' 00AB 14200 NODE_DESC:	.LONG	NODE_LTH	; NODE MESSAGE DESCRIPTOR

                           000000B3' 00AF 14300 		.LONG	NODE_CTRSTR	;

      43 41 21 20 74 65 6E 43 45 44  00B3 14400 NODE_CTRSTR:	.ASCII	/DECnet !AC/	;

                           0000000A  00BD 14500 NODE_LTH=.-NODE_CTRSTR

                                     00BD 14600 

                           00000032' 00BD 14700 ERROR_DESC:	.LONG	ERROR_LTH	; ERROR MESSAGE DESCRIPTOR

                           000000C5' 00C1 14800 		.LONG	ERROR_CTRSTR	;

20 65 6E 69 6C 20 74 65 6E 43 45 44  00C5 14900 ERROR_CTRSTR:	.ASCII	/DECnet line /

                           000000D5  00D1 15000 LINE_NAME1:	.BLKL	1		; FOR STUFFING LINE NAME

20 6F 74 20 64 65 6C 69 61 66 20 3A  00D5 15100 		.ASCII	/: failed to start due to error !XW/

6F 74 20 65 75 64 20 74 72 61 74 73  00E1       

      57 58 21 20 72 6F 72 72 65 20  00ED       

                           00000032  00F7 15200 ERROR_LTH=.-ERROR_CTRSTR

NETOPCOM        - OPERATOR COMMUNICATIONS                        22-AUG-1978 00:58:24   VAX-11 MACRO X0.3-11               Page   6

X01             DECLARATIONS                                                                                                     (1)



                                 00000000 15400 	.PSECT	NET_CONTROL,NOWRT,EXE

                                     0000 15500 	.SBTTL	NETWORK OPERATOR MESSAGE FORMATTING

                                     0000 15600 ;++

                                     0000 15700 ; FUNCTIONAL DESCRIPTION:

                                     0000 15800 ;

                                     0000 15900 ; NET$OPCOM_ERROR - ERROR STARTING LINE

                                     0000 16000 ; NET$OPCOM_NODE - MESSAGE IS FOR LOCAL NODE, NOT A LINE

                                     0000 16100 ; NET$OPCOM - FORMAT AND SEND OPERATOR MESSAGE ABOUT A LINE

                                     0000 16200 ;

                                     0000 16300 ; CALLING SEQUENCE:

                                     0000 16400 ;

                                     0000 16500 ;	BSB	NET$OPCOM, ETC.

                                     0000 16600 ;

                                     0000 16700 ; INPUT PARAMETERS:

                                     0000 16800 ;

                                     0000 16900 ;	R0 - ERROR CODE (NET$OPCOM_ERROR)

                                     0000 17000 ;	R6 - MESSAGE CODE

                                     0000 17100 ;	R9 - NDB ADDRESS

                                     0000 17200 ;

                                     0000 17300 ; SIDE EFFECTS:

                                     0000 17400 ;

                                     0000 17500 ;	MESSAGE SENT TO NETWORK OPERATOR

                                     0000 17600 ;

                                     0000 17700 ;--

                                     0000 17800 

                                     0000 17900 NET$OPCOM_ERROR::

            51       00BD'CF     9E  0000 18000 	MOVAB	W^ERROR_DESC,R1		; GET ADDRESS OF CONTROL STRING

       00D1'CF         04 A9     D0  0005 18100 	MOVL	NDB$L_LINE_NAME(R9),W^LINE_NAME1 ; STUFF THE LINE NAME

                          18     11  000B 18200 	BRB	COMMON1			; GO TO COMMON CODE

                                     000D 18300 

                                     000D 18400 NET$OPCOM_NODE::

            51       00AB'CF     9E  000D 18500 	MOVAB	W^NODE_DESC,R1		; GET ADDRESS OF CONTROL STRING

                          0B     11  0012 18600 	BRB	COMMON			; GO TO COMMON CODE

                                     0014 18700 NET$OPCOM::

       00A2'CF         04 A9     D0  0014 18800 	MOVL	NDB$L_LINE_NAME(R9),W^LINE_NAME ; STUFF THE LINE NAME

            51       008E'CF     9E  001A 18900 	MOVAB	W^LINE_DESC,R1		; GET ADDRESS OF CONTROL STRING

                                     001F 19000 COMMON:

            50       00BF'CF46   D0  001F 19100 	MOVL	W^MSG_ARRAY-4[R6],R0	; GET 1-ORIGIN ADDRESS OF TEXT STRING

                                     0025 19200 COMMON1:

                          3C     BB  0025 19300 	PUSHR	#^M<R2,R3,R4,R5>	; SAVE REGS

       0086'CF         50 8F     90  0027 19400 	MOVB	#TEXT_LTH,W^TEXT_DESC	; RESET THE OUTPUT BFR LTH

                                     002D 19500 	$FAO_S	CTRSTR=(R1),-		; FORMAT THE BUFFER

                                     002D 19600 		OUTLEN=W^TEXT_DESC,-	; STUFF THE BUFFER DESCRIPTOR

                                     002D 19700 		OUTBUF=W^TEXT_DESC,-	;

                                     002D 19800 		P1=R0			; THIS IS THE PARAMETER

                     0086'CF     DF  0040 19900 	PUSHAL	W^TEXT_DESC		; SET UP FOR CALL

   00000000'EF            01     FB  0044 20000 	CALLS	#1,EXE$NETSNDERL	; SEND THE MSG TO THE ERROR LOGGER

            55   00000000'EF     9E  004B 20100 	MOVAB	L^SYS$GL_OPRMBX,R5	; GET MAILBOX UCB ADDRESS

       0086'CF            2E'    C1  0052 20200 	ADDL3	S^#TEXT-MSG_BUFFER,W^TEXT_DESC,R3 ; LTH OF MBX MSG

                          53         0057       

            54       0008'CF     9E  0058 20300 	MOVAB	W^MSG_BUFFER,R4		; BUFFER ADDRESS

                 00000000'EF     16  005D 20400 	JSB	L^EXE$WRTMAILBOX	; SEND THE MESSAGE

                          3C     BA  0063 20500 	POPR	#^M<R2,R3,R4,R5>	; RESTORE REGS

                                 05  0065 20600 	RSB				; DONE

                                     0066 20700 

                                     0066 20800 	.END

NETOPCOM        - OPERATOR COMMUNICATIONS                        22-AUG-1978 00:58:24   VAX-11 MACRO X0.3-11               Page   7

SYMBOL TABLE                                                                                                                     (1)



$$T2           = 00000004            MSG_BUFFER       00000008 R     04   NET$OPCOM_NODE   0000000D RG    05   

BIT...         = 00000000            MSG_DESC         00000000 R     04   NGINI_MSG        0000002C R     03   

COMMON           0000001F R     05   NDB$B_COMMVER    0000002B            NODE_CTRSTR      000000B3 R     04   

COMMON1          00000025 R     05   NDB$B_CONNTMO    0000004F            NODE_DESC        000000AB R     04   

DCHK_MSG         000000AA R     03   NDB$B_FUNC       00000021            NODE_LTH       = 0000000A            

DOWN_MSG         00000022 R     03   NDB$B_NONPRVACC  00000050            OKINI_MSG        0000004A R     03   

DSRCH_MSG        00000073 R     03   NDB$B_NUMBUF     0000000B            OPC$B_MS_ENAB    00000001            

ERROR_CTRSTR     000000C5 R     04   NDB$B_PRVACC     0000007C            OPC$B_MS_TARGET  00000001            

ERROR_DESC       000000BD R     04   NDB$B_RTEVER     00000028            OPC$B_MS_TYPE    00000000            

ERROR_LTH      = 00000032            NDB$B_STATE      00000016            OPC$L_MS_MASK    00000004            

EXE$NETSNDERL    ********   X   05   NDB$B_STATUS     00000017            OPC$L_MS_MAXSZ   0000009A            

EXE$WRTMAILBOX   ********   X   05   NDB$B_TYPE       0000000A            OPC$L_MS_OTEXT   0000001A            

GBL...         = 00000000            NDB$C_CTL_LOOP = 00000005            OPC$L_MS_RPLYID  00000004            

LINE_CTRSTR      00000096 R     04   NDB$C_LENGTH     000000BC            OPC$L_MS_RQSTID  00000004            

LINE_DESC        0000008E R     04   NDB$C_LOOP     = 00000003            OPC$L_MS_TEXT    00000008            

LINE_LTH       = 00000015            NDB$C_MAINT    = 00000004            OPC$M_NM_CARDS = 00000020            

LINE_NAME        000000A2 R     04   NDB$C_MSG_DCHK = 00000009            OPC$M_NM_CENTRL= 00000001            

LINE_NAME1       000000D1 R     04   NDB$C_MSG_DOWN = 00000003            OPC$M_NM_DEVICE= 00000010            

LOOPB_MSG        00000092 R     03   NDB$C_MSG_DSRCH= 00000007            OPC$M_NM_DISKS = 00000008            

MAINT_MSG        00000009 R     03   NDB$C_MSG_LOOPB= 00000008            OPC$M_NM_NTWORK= 00000040            

MSG$_ABOOPR    = 00000011            NDB$C_MSG_MAINT= 00000002            OPC$M_NM_OPER1 = 00001000            

MSG$_ABORT     = 00000030            NDB$C_MSG_NGINI= 00000004            OPC$M_NM_OPER10= 00200000            

MSG$_ACCRSP    = 00000021            NDB$C_MSG_OKINI= 00000005            OPC$M_NM_OPER11= 00400000            

MSG$_CONFIRM   = 00000031            NDB$C_MSG_SHUT = 00000006            OPC$M_NM_OPER12= 00800000            

MSG$_CONNECT   = 00000032            NDB$C_MSG_START= 00000001            OPC$M_NM_OPER2 = 00002000            

MSG$_CRUNSOLIC = 00000002            NDB$C_OFF      = 00000001            OPC$M_NM_OPER3 = 00004000            

MSG$_DELPROC   = 00000003            NDB$C_ON       = 00000000            OPC$M_NM_OPER4 = 00008000            

MSG$_DELSMB    = 00000014            NDB$C_SHUT     = 00000002            OPC$M_NM_OPER5 = 00010000            

MSG$_DEVOFFLIN = 00000005            NDB$K_LENGTH     000000BC            OPC$M_NM_OPER6 = 00020000            

MSG$_DEVONLIN  = 00000007            NDB$L_LINE_NAME  00000004            OPC$M_NM_OPER7 = 00040000            

MSG$_DISCON    = 00000033            NDB$L_NEXT       00000000            OPC$M_NM_OPER8 = 00080000            

MSG$_EXIT      = 00000034            NDB$M_CTL_LOOP = 00000008            OPC$M_NM_OPER9 = 00100000            

MSG$_INIOPR    = 00000010            NDB$M_LOOPBACK = 00000001            OPC$M_NM_PRINT = 00000002            

MSG$_INTMSG    = 00000035            NDB$M_OFF      = 00000002            OPC$M_NM_TAPES = 00000004            

MSG$_OPREPLY   = 00000009            NDB$M_SHUT     = 00000004            OPC$T_MS_ONAME   0000000A            

MSG$_OPRQST    = 00000008            NDB$Q_AST        0000000C            OPC$V_NM_CARDS = 00000005            

MSG$_PATHLOST  = 00000036            NDB$Q_ZEROTIME   000000AC            OPC$V_NM_CENTRL= 00000000            

MSG$_PROTOCOL  = 00000037            NDB$T_NAME       0000001A            OPC$V_NM_DEVICE= 00000004            

MSG$_REJECT    = 00000038            NDB$T_SYSVER     0000002E            OPC$V_NM_DISKS = 00000003            

MSG$_RESOPR    = 00000013            NDB$V_CTL_LOOP = 00000003            OPC$V_NM_NTWORK= 00000006            

MSG$_SCANBAD   = 00000028            NDB$V_LOOPBACK = 00000000            OPC$V_NM_OPER1 = 0000000C            

MSG$_SCANRSP   = 00000029            NDB$V_OFF      = 00000001            OPC$V_NM_OPER10= 00000015            

MSG$_SMBDON    = 00000009            NDB$V_SHUT     = 00000002            OPC$V_NM_OPER11= 00000016            

MSG$_SMBINI    = 00000008            NDB$W_BLKSIZE    00000022            OPC$V_NM_OPER12= 00000017            

MSG$_SMBRSP    = 00000020            NDB$W_BUFSIZE    000000A8            OPC$V_NM_OPER2 = 0000000D            

MSG$_SNDACC    = 0000000A            NDB$W_CHANNEL    00000014            OPC$V_NM_OPER3 = 0000000E            

MSG$_SNDSMB    = 00000004            NDB$W_CHAR       000000AA            OPC$V_NM_OPER4 = 0000000F            

MSG$_SUSOPR    = 00000012            NDB$W_HISBLKSIZ  000000B8            OPC$V_NM_OPER5 = 00000010            

MSG$_THIRDPARTY= 00000039            NDB$W_HISNSPSIZ  000000BA            OPC$V_NM_OPER6 = 00000011            

MSG$_TIMEOUT   = 0000003A            NDB$W_MAXLNK     00000026            OPC$V_NM_OPER7 = 00000012            

MSG$_TRMHANGUP = 00000006            NDB$W_NODEADDR   00000018            OPC$V_NM_OPER8 = 00000013            

MSG$_TRMUNSOLIC= 00000001            NDB$W_NSPSIZE    00000024            OPC$V_NM_OPER9 = 00000014            

MSG$_XM_ATTN   = 0000000D            NDB$W_RCVBLKS    000000B4            OPC$V_NM_PRINT = 00000001            

MSG$_XM_DATAVL = 0000000B            NDB$W_SIZE       00000008            OPC$V_NM_TAPES = 00000002            

MSG$_XM_SHUTDN = 0000000C            NDB$W_XMTBLKS    000000B6            OPC$W_MS_OUNIT   00000008            

MSGNUM         = 00000009            NET$OPCOM        00000014 RG    05   OPC$W_MS_STATUS  00000002            

MSG_ARRAY        000000C3 R     03   NET$OPCOM_ERROR  00000000 RG    05   OPC$_DEVNOTERM = 00058074            

NETOPCOM        - OPERATOR COMMUNICATIONS                        22-AUG-1978 00:58:24   VAX-11 MACRO X0.3-11               Page   8

SYMBOL TABLE                                                                                                                     (1)



OPC$_DEVOFFLINE= 0005804C            

OPC$_DEVONLINE = 00058054            

OPC$_ILLRQST   = 0005807C            

OPC$_LOGCLOS   = 000580A4            

OPC$_LOGFAIL   = 00058034            

OPC$_LOGINIT   = 00058009            

OPC$_LOGTIME   = 00058099            

OPC$_NOCLI     = 0005805C            

OPC$_NOPERATOR = 00058061            

OPC$_NOSUCHRQST= 00058044            

OPC$_OPREPLY   = 00058091            

OPC$_OPRNOTIF  = 00058089            

OPC$_RQSTABORT = 0005801C            

OPC$_RQSTCAN   = 00058084            

OPC$_RQSTCMPLTE= 00058029            

OPC$_RQSTPEND  = 00058021            

OPC$_RQ_CANCEL = 00000005            

OPC$_RQ_LOGI   = 00000002            

OPC$_RQ_REPLY  = 00000004            

OPC$_RQ_RQST   = 00000003            

OPC$_RQ_STATUS = 00000006            

OPC$_RQ_TERME  = 00000001            

OPC$_TERMDSBL  = 00058011            

OPC$_TERMENAB  = 00058001            

OPC$_TERMFAIL  = 0005803C            

OPC$_UNKNOPR   = 0005806C            

SHUT_MSG         00000065 R     03   

START_MSG        00000000 R     03   

SYS$FAO          ********   X   05   

SYS$GL_OPRMBX    ********   X   05   

TEXT             00000036 R     04   

TEXT_DESC        00000086 R     04   

TEXT_LTH       = 00000050            





PROGRAM SECTION SYNOPSIS



.  ABS  .        00000000      00     NOPIC   USR   CON   ABS   LCL NOSHR NOEXE NORD  NOWRT BYTE  

. BLANK .        00000000      01     NOPIC   USR   CON   REL   LCL NOSHR   EXE   RD    WRT BYTE  

$ABS$            000000BC      02     NOPIC   USR   CON   ABS   LCL NOSHR   EXE   RD    WRT BYTE  

NET_PURE         000000E7      03     NOPIC   USR   CON   REL   LCL NOSHR NOEXE   RD  NOWRT BYTE  

NET_IMPURE       000000F7      04     NOPIC   USR   CON   REL   LCL NOSHR NOEXE   RD    WRT BYTE  

NET_CONTROL      00000066      05     NOPIC   USR   CON   REL   LCL NOSHR   EXE   RD  NOWRT BYTE  





THERE WERE NO ERRORS OR WARNINGS.

20480. BYTES LEFT IN FREE MEMORY POOL.

768. BYTES OF RECLAIMED MEMORY.

OBJ$:NETOPCOM,LIS$:NETOPCOM/-SP=EXECML$/ML,M1/ML,M2/ML,SRC$:NETOPCOM

48 MLB DIR RDS - 336 GETS TO DEFINE 15 MACROS. 23 INTER. FILE WRITES. 

