SYSRUNDWN       IMAGE RUNDOWN SYSTEM SERVICE                     22-AUG-1978 00:21:23   VAX-11 MACRO X0.3-11               Page   0

TABLE OF CONTENTS   



   (1)      34  HISTORY			; DETAILED

   (1)      44  DECLARATIONS

   (1)      65  EXE$RUNDWN - IMAGE RUNDOWN SYSTEM SERVICE

SYSRUNDWN       IMAGE RUNDOWN SYSTEM SERVICE                     22-AUG-1978 00:21:23   VAX-11 MACRO X0.3-11               Page   1

01                                                                                                                               (1)



                                     0000     1 

                                     0000     2 	.TITLE	SYSRUNDWN IMAGE RUNDOWN SYSTEM SERVICE

                                     0000     3 	.IDENT	/01/

                                     0000     4 

                                     0000     5 ;

                                     0000     6 ; COPYRIGHT (C) 1977

                                     0000     7 ; DIGITAL EQUIPMENT CORPORATION, MAYNARD, MASSACHUSETTS 01754

                                     0000     8 ;

                                     0000     9 ; THIS SOFTWARE IS FURNISHED  UNDER A LICENSE FOR USE ONLY ON A SINGLE

                                     0000    10 ; COMPUTER  SYSTEM AND  MAY BE  COPIED ONLY WITH  THE INCLUSION OF THE

                                     0000    11 ; ABOVE COPYRIGHT NOTICE.  THIS SOFTWARE, OR ANY OTHER COPIES THEREOF,

                                     0000    12 ; MAY NOT BE PROVIDED OR  OTHERWISE MADE AVAILABLE TO ANY OTHER PERSON

                                     0000    13 ; EXCEPT FOR USE ON SUCH SYSTEM AND TO ONE WHO AGREES TO THESE LICENSE

                                     0000    14 ; TERMS.  TITLE TO AND  OWNERSHIP OF THE  SOFTWARE  SHALL AT ALL TIMES

                                     0000    15 ; REMAIN IN DEC.

                                     0000    16 ;

                                     0000    17 ; THE INFORMATION IN THIS SOFTWARE IS SUBJECT TO CHANGE WITHOUT NOTICE

                                     0000    18 ; AND SHOULD  NOT BE CONSTRUED  AS A COMMITMENT  BY DIGITAL  EQUIPMENT

                                     0000    19 ; CORPORATION.

                                     0000    20 ;

                                     0000    21 ; DEC ASSUMES  NO  RESPONSIBILITY  FOR  THE USE OR  RELIABILITY OF ITS

                                     0000    22 ; SOFTWARE ON EQUIPMENT WHICH IS NOT SUPPLIED BY DEC.

                                     0000    23 

                                     0000    24 ;++

                                     0000    25 ; FACILITY: EXECUTIVE, SYSTEM SERVICES

                                     0000    26 ;

                                     0000    27 ; ABSTRACT:

                                     0000    28 ;

                                     0000    29 ; ENVIRONMENT:

                                     0000    30 ;

                                     0000    31 ;--

                                     0000    32 ;

                                     0000    33 ;	.PAGE

                                     0000    34 	.SBTTL	HISTORY			; DETAILED

                                     0000    35 ;

                                     0000    36 ; AUTHOR:	R. HUSTVEDT	 CREATION DATE: 10-OCT-76

                                     0000    37 ;

                                     0000    38 ; MODIFIED BY:

                                     0000    39 ; C. MONIA, : VERSION 01

                                     0000    40 ; 01	 -	MODIFIED FOR STAND-ALONE DSC SYSTEM

                                     0000    41 ;

                                     0000    42 

SYSRUNDWN       IMAGE RUNDOWN SYSTEM SERVICE                     22-AUG-1978 00:21:23   VAX-11 MACRO X0.3-11               Page   2

01              DECLARATIONS                                                                                                     (1)



                                     0000    44 	.SBTTL	DECLARATIONS

                                     0000    45 

                                     0000    46 ;

                                     0000    47 ; INCLUDE FILES:

                                     0000    48 ;

                                     0000    49 

                                     0000    50 	$ACBDEF				; DEFINE AST CONTROL BLOCK

                                     0000    51 	$CCBDEF				; DEFINE CHANNEL CONTROL BLOCK

                                     0000    52 	$IPLDEF				; DEFINE INTERRUPT PRIORITIES

                                     0000    53 	$LOGDEF				; DEFINE LOGICAL NAME BLOCK

                                     0000    54 	$PCBDEF				; DEFINE PCB OFFSETS

                                     0000    55 	$PRDEF				; DEFINE PROCESSOR REGISTERS

                                     0000    56 	$SSDEF				; DEFINE STATUS CODES

                                     0000    57 

                                     0000    58 ;

                                     0000    59 ; EQUATED SYMBOLS:

                                     0000    60 ;

                           00000004  0000    61 ACMODE=4				; DISPLACEMENT TO ACCESS MODE ARGUMENT

                                     0000    62 

                                     0000    63 	.LIST	MEB			; LIST MACRO EXPANSIONS

SYSRUNDWN       IMAGE RUNDOWN SYSTEM SERVICE                     22-AUG-1978 00:21:23   VAX-11 MACRO X0.3-11               Page   3

01              EXE$RUNDWN - IMAGE RUNDOWN SYSTEM SERVICE                                                                        (1)



                                     0000    65 	.SBTTL	EXE$RUNDWN - IMAGE RUNDOWN SYSTEM SERVICE

                                     0000    66 

                                     0000    67 ;++

                                     0000    68 ; FUNCTIONAL DESCRIPTION:

                                     0000    69 ;	EXE$RUNDWN TERMINATES ALL PENDING ACTIVITY FOR THE SPECIFIED

                                     0000    70 ;	AND ALL LESS PRIVILEGED ACCESS MODES.  ALL RESOURCES ASSOCIATED 

                                     0000    71 ;	WITH THE PENDING ACTIVITY WILL BE RELEASED IF APPROPRIATE

                                     0000    72 ;

                                     0000    73 ; CALLING SEQUENCE:

                                     0000    74 ;	CALLG	ARGLIST,EXE$RUNDWN

                                     0000    75 ;

                                     0000    76 ; INPUT PARAMETERS:

                                     0000    77 ;	ACMODE(AP) - ACCESS MODE BOUNDARY FOR WHICH RUNDOWN IS TO BE PERFORMED

                                     0000    78 ;			(MAXIMIZED WITH THE ACCESS MODE OF THE CALLER)

                                     0000    79 ;

                                     0000    80 ; IMPLICIT INPUTS:

                                     0000    81 ;	R4 - POINTER TO CURRENT PCB

                                     0000    82 ;

                                     0000    83 ; OUTPUT PARAMETERS:

                                     0000    84 ;	NONE

                                     0000    85 ;

                                     0000    86 ; IMPLICIT OUTPUTS:

                                     0000    87 ;	ALL ACTIVITY INITIATED BUT NOT COMPLETED FOR ALL ACCESS MODES

                                     0000    88 ;	HAVING THE SAME OR LESSER PRIVILEGE THAN THAT SPECIFIED WILL

                                     0000    89 ;	BE TERMINATED.

                                     0000    90 ;

                                     0000    91 ; COMPLETION CODES:

                                     0000    92 ;	SS$_NORMAL  -  SUCCESSFUL COMPLETION

                                     0000    93 ;

                                     0000    94 ; SIDE EFFECTS:

                                     0000    95 ;	NONE

                                     0000    96 ;

                                     0000    97 ;--

                                     0000    98 

                               00FC' 0000    99 	.ENTRY	EXE$RUNDWN,^M<R2,R3,R4,R5,R6,R7>

            02            00     EF  0002   100 	EXTZV	#0,#2,ACMODE(AP),R0	; FETCH ACCESS MODE ARGUMENT

            50         04 AC         0005       

                          FFF5'  30  0008   101 	BSBW	EXE$MAXACMODE		; MAXIMIZE WITH PREVIOUS

            57            50     D0  000B   102 	MOVL	R0,R7			; SAVE IN R7 FOR REFERENCE

                                     000E   103 

                                     000E   104 ;-------------------------------------------------------------

                                     000E   105 ;

                                     000E   106 ;	RELEASE MEMORY

                                     000E   107 ;

                                     000E   108 ; NOT INVOKED IN THE CORE-ONLY SYSTEM

                                     000E   109 ;

                                     000E   110 ;

                                     000E   111 ;-------------------------------------------------------------

                                     000E   112 

                                     000E   113 ;	BSBW	MMG$IMGRESET		; RELEASE IMAGE PAGES

                                     000E   114 ;**************************************   NEED INTERFACE CHANGE FOR ACMODE

                                     000E   115 ;-------------------------------------------------------------

                                     000E   116 ;

                                     000E   117 ;	DEASSIGN CHANNELS

                                     000E   118 ;

                                     000E   119 ;-------------------------------------------------------------

                                     000E   120 

SYSRUNDWN       IMAGE RUNDOWN SYSTEM SERVICE                     22-AUG-1978 00:21:23   VAX-11 MACRO X0.3-11               Page   4

01              EXE$RUNDWN - IMAGE RUNDOWN SYSTEM SERVICE                                                                        (1)



                                     000E   121 IORUNDWN:				;

            56   00000000'9F     3C  000E   122 	MOVZWL	@#CTL$GW_NMIOCH,R6	; GET NUMBER OF I/O CHANNELS

            55   00000000'9F     3C  0015   123 	MOVZWL	@#CTL$GW_CHINDX,R5	; GET MAXIMUM INDEX + 16

            55            55     CE  001C   124 	MNEGL	R5,R5			; INVERT

            55            10     C0  001F   125 10$:	ADDL	#16,R5			; POINT AT NEXT CHANNEL

            53   00000000'FF45   9E  0022   126 	MOVAB	@CTL$GL_CCBBASE[R5],R3	; COMPUTE ADDRESS OF HIGHEST CHANNEL

            57         09 A3     91  002A   127 	CMPB	CCB$B_AMOD(R3),R7	; IS THIS CHANNEL DEASSIGNABLE?

                          0A     15  002E   128 	BLEQ	20$			; NO, ASSIGNED BY LOWER ACMODE

            7E            55     CE  0030   129 	MNEGL	R5,-(SP)		; CHANNEL NUMBER ARGUMENT

   00000000'9F            01     FB  0033   130 	CALLS	#1,@#SYS$DASSGN		; DE-ASSIGN CHANNEL

            E2            56     F4  003A   131 20$:	SOBGEQ	R6,10$			; NEXT CHANNEL

                                     003D   132 	$DALLOC_S	ACMODE=R7	; DE-ALLOCATE AT ACCESS MODE

                          57     DD  003D       		PUSHL	R7

                          00     DD  003F       		PUSHL	#0

   00000000'9F            02     FB  0041       		CALLS	#2,@#SYS$DALLOC

                                     0048   133 

                                     0048   134 ;-------------------------------------------------------------

                                     0048   135 ;

                                     0048   136 ;	CANCEL TIMER REQUESTS

                                     0048   137 ;

                                     0048   138 ;-------------------------------------------------------------

                                     0048   139 

                          57     DD  0048   140 	PUSHL	R7			; ACCESS MODE ARGUMENT

                          00     DD  004A   141 	PUSHL	#0			; CANCEL ALL INDICATOR

       0000'CF            02     FB  004C   142 	CALLS	#2,W^EXE$CANTIM		; CANCEL TIMER REQUESTS

                                     0051   143 

                                     0051   144 

                                     0051   145 ;-------------------------------------------------------------

                                     0051   146 ;

                                     0051   147 ;	DISASSOCIATE COMMON EVENT BLOCKS

                                     0051   148 ;

                                     0051   149 ;-------------------------------------------------------------

                                     0051   150 

            7E         40 8F     9A  0051   151 	MOVZBL	#64,-(SP)		; PUSHL EFN FOR GROUP #2

       0000'CF            01     FB  0055   152 	CALLS	#1,W^EXE$DACEFC		; DISASSOCIATE

            7E         60 8F     9A  005A   153 	MOVZBL	#96,-(SP)		; PUSH	EFN FOR GROUP #3

       0000'CF            01     FB  005E   154 	CALLS	#1,W^EXE$DACEFC		; DISASSOCIATE

                                     0063   155 ;-------------------------------------------------------------

                                     0063   156 ;

                                     0063   157 ;	PURGE PENDING UNDELIVERED AST CONTROL BLOCKS

                                     0063   158 ;

                                     0063   159 ;-------------------------------------------------------------

                                     0063   160 

                                     0063   161 ASTRUNDWN:				; 

            56         10 A4     DE  0063   162 	MOVAL	PCB$L_ASTQFL(R4),R6	; COMPUTE ADDRESS OF HEADER

                                     0067   163 	DSBINT	#IPL$_SYNCH		; BLOCK AST ARRIVAL

            7E            12     DB  0067       		MFPR	#PR$_IPL,-(SP)

            12            07     DA  006A       		MTPR	#IPL$_SYNCH,#PR$_IPL

         60 A4       0004'CF     D1  006D   164 	CMPL	W^EXE$GQ_ERLMBX+4,PCB$L_PID(R4)	; CHECK FOR ERROR LOG MAILBOX

                          04     12  0073   165 	BNEQ	10$			; BR IF NO

                     0000'CF     7C  0075   166 	CLRQ	W^EXE$GQ_ERLMBX		; YES, DEASSIGN IT

            50         14 A4     D0  0079   167 10$:	MOVL	PCB$L_ASTQBL(R4),R0	; GET TAIL OF AST QUEUE

            56            50     D1  007D   168 	CMPL	R0,R6			; CHECK FOR EMPTY QUEUE

                          1A     13  0080   169 	BEQL	20$			; YES, DONE WITH ASTS

            02            00     ED  0082   170 	CMPZV	#ACB$V_MODE,#ACB$S_MODE,ACB$B_RMOD(R0),R7 ; CHECK ACCESS MODE OF ACB

            57         0B A0         0085       

                          12     19  0088   171 	BLSS	20$			; REACHED THE END OF DELETABLE ASTS

SYSRUNDWN       IMAGE RUNDOWN SYSTEM SERVICE                     22-AUG-1978 00:21:23   VAX-11 MACRO X0.3-11               Page   5

01              EXE$RUNDWN - IMAGE RUNDOWN SYSTEM SERVICE                                                                        (1)



            50            60     0F  008A   172 	REMQUE	(R0),R0			; REMOVE IT FROM AST QUEUE

                          0D     1D  008D   173 	BVS	20$			; EXIT IF QUEUE EMPTY

         0B A0            06     E1  008F   174 	BBC	#ACB$V_QUOTA,ACB$B_RMOD(R0),15$	; SKIP IF NO QUOTA ACCOUNTING

                          03         0093       

                       3C A4     B6  0094   175 	INCW	PCB$W_ASTCNT(R4)	; ALLOW ANOTHER AST

                          FF66'  30  0097   176 15$:	BSBW	EXE$DEANONPAGED		; AND RELEASE ITS SPACE

                          DD     11  009A   177 	BRB	10$			; CONTINUE

                                     009C   178 

                                     009C   179 ;-------------------------------------------------------------

                                     009C   180 ;

                                     009C   181 ;	RESET AST ACTIVE AND AST ENABLE BITS

                                     009C   182 ;

                                     009C   183 ;-------------------------------------------------------------

                                     009C   184 

            55            57     D0  009C   185 20$:	MOVL	R7,R5			; INITIALIZE MODE INDEX

                          13     13  009F   186 	BEQL	40$			; SKIP TERMINATION HANDLER FOR KERNEL

                                     00A1   187 30$:	

            55            02     D1  00A1   188 	CMPL	#2,R5			; SUPERVISOR OR USER MODE?

                          07     19  00A4   189 	BLSS	35$			; BRANCH IF NOT

                 FFFFFFF8'9F45   D4  00A6   190 	CLRL	@#CTL$GL_CMSUPR-8[R5]	; CLEAR CHANGE MODE HANDLER

                 FFFFFFFC'9F45   D4  00AD   191 35$:	CLRL	@#CTL$GL_THEXEC-4[R5]	; CLEAR TERMINATION HANDLER

                 00000000'9F45   7C  00B4   192 40$:	CLRQ	@#CTL$AQ_EXCVEC[R5]	; CLEAR EXCEPTION HANDLER ENTRIES

                 00000000'9F45   D4  00BB   193 	CLRL	@#CTL$AL_FINALEXC[R5]	; CLEAR LAST CHANCE EXCEPTION HANDLER

         0D A4            55     E2  00C2   194 	BBSS	R5,PCB$B_ASTEN(R4),50$	; SET ENABLE BIT

                          00         00C6       

         0C A4            55     E5  00C7   195 50$:	BBCC	R5,PCB$B_ASTACT(R4),60$	; CLEAR AST ACTIVE

                          00         00CB       

            55            06     C1  00CC   196 60$:	ADDL3	#PCB$V_SSFEXC,R5,R0	; COMPUTE SSFAIL ENABLE BIT NUMBER

                          50         00CF       

         28 A4            50     E5  00D0   197 	BBCC	R0,PCB$L_STS(R4),70$	; AND CLEAR IT

                          00         00D4       

            55            04     F2  00D5   198 70$:	AOBLSS	#4,R5,30$		; DO ALL REQUESTED MODES

                          C8         00D8       

                 00000000'9F     D4  00D9   199 	CLRL	@#CTL$GL_CMHANDLR	; CLEAR COMPATIBILITY MODE HANDLER

                          FF1E'  30  00DF   200 	BSBW	SCH$NEWLVL		; COMPUTE NEW ASTLVL

         28 A4            02     E5  00E2   201 	BBCC	#PCB$V_FORCPEN,PCB$L_STS(R4),80$	; CLEAR FORCE EXIT PENDING

                          00         00E6       

                                     00E7   202 80$:					;

                                     00E7   203 	ENBINT				; ENABLE AGAIN

            12            8E     DA  00E7       		MTPR	(SP)+,#PR$_IPL

                                     00EA   204 ;-------------------------------------------------------------

                                     00EA   205 ;

                                     00EA   206 ;	DELETE IMAGE LOGICAL NAMES

                                     00EA   207 ;

                                     00EA   208 ;-------------------------------------------------------------

                                     00EA   209 

                                     00EA   210 LOGNRUNDWN:				; LOGICAL NAME RUNDOWN

                                     00EA   211 	$DELLOG_S	TBLFLG=#2,-	; DELETE PROCESS LOCAL

                                     00EA   212 			ACMODE=R7	; FOR RUNDOWN MODE

                          57     DD  00EA       		PUSHL	R7

                          00     DD  00EC       		PUSHL	#0

                          02     DD  00EE       		PUSHL	#2

   00000000'9F            03     FB  00F0       		CALLS	#3,@#SYS$DELLOG

                                     00F7   213 

                                     00F7   214 

            50            01     3C  00F7   215 	MOVZWL	#SS$_NORMAL,R0		; SET NORMAL COMPLETION STATUS

                                 04  00FA   216 	RET				; RETURN

SYSRUNDWN       IMAGE RUNDOWN SYSTEM SERVICE                     22-AUG-1978 00:21:23   VAX-11 MACRO X0.3-11               Page   6

01              EXE$RUNDWN - IMAGE RUNDOWN SYSTEM SERVICE                                                                        (1)



                                     00FB   217 

                                     00FB   218 	.END

SYSRUNDWN       IMAGE RUNDOWN SYSTEM SERVICE                     22-AUG-1978 00:21:23   VAX-11 MACRO X0.3-11               Page   7

SYMBOL TABLE                                                                                                                     (1)



ACB$B_RMOD       0000000B            LOG$C_SYSTEM   = 00000000            PCB$W_APTCNT     00000034            

ACB$B_TYPE       0000000A            LOG$K_LENGTH     00000014            PCB$W_ASTCNT     0000003C            

ACB$L_AST        00000010            LOG$L_LTBL       00000004            PCB$W_BIOCNT     0000003E            

ACB$L_ASTPRM     00000014            LOG$L_LTFL       00000000            PCB$W_BIOLM      00000040            

ACB$L_ASTQBL     00000004            LOG$L_MBXUCB     00000010            PCB$W_BYTCNT     00000042            

ACB$L_ASTQFL     00000000            LOG$T_NAME       00000014            PCB$W_BYTLM      00000068            

ACB$L_KAST       00000018            LOG$W_GROUP      0000000C            PCB$W_DIOCNT     00000044            

ACB$L_PID        0000000C            LOG$W_SIZE       00000008            PCB$W_DIOLM      00000046            

ACB$M_QUOTA    = 00000040            LOGNRUNDWN       000000EA R     01   PCB$W_FILCNT     00000048            

ACB$S_MODE     = 00000002            PCB$B_ASTACT     0000000C            PCB$W_GPGCNT     00000038            

ACB$V_KAST     = 00000007            PCB$B_ASTEN      0000000D            PCB$W_GRP        00000022            

ACB$V_MODE     = 00000000            PCB$B_PRI        0000000B            PCB$W_MEM        00000020            

ACB$V_QUOTA    = 00000006            PCB$B_PRIB       00000033            PCB$W_MTXCNT     0000000E            

ACB$W_SIZE       00000008            PCB$B_TYPE       0000000A            PCB$W_PPGCNT     0000003A            

ACMODE         = 00000004            PCB$B_WEFC       00000032            PCB$W_PRCCNT     0000006A            

ASTRUNDWN        00000063 R     01   PCB$C_LENGTH     0000007C            PCB$W_SIZE       00000008            

BIT...         = 00000000            PCB$K_LENGTH     0000007C            PCB$W_STATE      00000030            

CCB$B_AMOD       00000009            PCB$L_ASTQBL     00000014            PCB$W_TMBU       00000036            

CCB$B_STS        00000008            PCB$L_ASTQFL     00000010            PCB$W_TQCNT      0000004A            

CCB$C_LENGTH     00000010            PCB$L_EFC2P      00000058            PR$_ACCR       = 00000029            

CCB$K_LENGTH     00000010            PCB$L_EFC3P      0000005C            PR$_ACCS       = 00000028            

CCB$L_DIRP       0000000C            PCB$L_EFCS       00000050            PR$_ASTLVL     = 00000013            

CCB$L_UCB        00000000            PCB$L_EFCU       00000054            PR$_ESP        = 00000001            

CCB$L_WIND       00000004            PCB$L_EFWM       0000004C            PR$_ICCS       = 00000018            

CCB$W_IOC        0000000A            PCB$L_OWNER      0000001C            PR$_ICR        = 0000001A            

CTL$AL_FINALEXC  ********   X   01   PCB$L_PHD        00000064            PR$_IPL        = 00000012            

CTL$AQ_EXCVEC    ********   X   01   PCB$L_PHYPCB     00000018            PR$_ISP        = 00000004            

CTL$GL_CCBBASE   ********   X   01   PCB$L_PID        00000060            PR$_KSP        = 00000000            

CTL$GL_CMHANDLR  ********   X   01   PCB$L_PQB        0000004C            PR$_MAPEN      = 00000038            

CTL$GL_CMSUPR    ********   X   01   PCB$L_SQBL       00000004            PR$_NICR       = 00000019            

CTL$GL_THEXEC    ********   X   01   PCB$L_SQFL       00000000            PR$_P0BR       = 00000008            

CTL$GW_CHINDX    ********   X   01   PCB$L_STS        00000028            PR$_P0LR       = 00000009            

CTL$GW_NMIOCH    ********   X   01   PCB$L_UIC        00000020            PR$_P1BR       = 0000000A            

EXE$CANTIM       ********   X   01   PCB$L_WSSWP      00000024            PR$_P1LR       = 0000000B            

EXE$DACEFC       ********   X   01   PCB$L_WTIME      0000002C            PR$_PCBB       = 00000010            

EXE$DEANONPAGED  ********   X   01   PCB$T_LNAME      0000006C            PR$_RXCS       = 00000020            

EXE$GQ_ERLMBX    ********   X   01   PCB$V_ASTPEN   = 00000011            PR$_RXDB       = 00000021            

EXE$MAXACMODE    ********   X   01   PCB$V_BATCH    = 0000000E            PR$_SBIER      = 00000034            

EXE$RUNDWN       00000000 RG    01   PCB$V_DELPEN   = 00000001            PR$_SBIFS      = 00000030            

GBL...         = 00000000            PCB$V_FORCPEN  = 00000002            PR$_SBIMT      = 00000033            

IORUNDWN         0000000E R     01   PCB$V_HIBER    = 00000013            PR$_SBIQC      = 00000036            

IPL$_ASTDEL    = 00000002            PCB$V_INQUAN   = 00000003            PR$_SBIS       = 00000031            

IPL$_HWCLK     = 00000018            PCB$V_LOGIN    = 00000014            PR$_SBISC      = 00000032            

IPL$_IOPOST    = 00000004            PCB$V_NOACNT   = 0000000F            PR$_SBITA      = 00000035            

IPL$_MAILBOX   = 0000000B            PCB$V_PHDRES   = 00000012            PR$_SBR        = 0000000C            

IPL$_POWER     = 0000001F            PCB$V_PSWAPM   = 00000004            PR$_SCBB       = 00000011            

IPL$_QUEUEAST  = 00000006            PCB$V_RES      = 00000000            PR$_SID        = 0000003E            

IPL$_SCHED     = 00000003            PCB$V_RESPEN   = 00000005            PR$_SIRR       = 00000014            

IPL$_SYNCH     = 00000007            PCB$V_SSFEXC   = 00000006            PR$_SISR       = 00000015            

IPL$_TIMER     = 00000007            PCB$V_SSFEXCE  = 00000007            PR$_SLR        = 0000000D            

LOG$B_AMOD       0000000E            PCB$V_SSFEXCS  = 00000008            PR$_SSP        = 00000002            

LOG$B_TABLE      0000000B            PCB$V_SSFEXCU  = 00000009            PR$_TBIA       = 00000039            

LOG$B_TYPE       0000000A            PCB$V_SSRWAIT  = 0000000A            PR$_TBIS       = 0000003A            

LOG$C_GROUP    = 00000001            PCB$V_SUSPEN   = 0000000B            PR$_TODR       = 0000001B            

LOG$C_LENGTH     00000014            PCB$V_SWPVBN   = 00000010            PR$_TXCS       = 00000022            

LOG$C_NAMLENGTH= 00000040            PCB$V_WAKEPEN  = 0000000C            PR$_TXDB       = 00000023            

LOG$C_PROCESS  = 00000002            PCB$V_WALL     = 0000000D            PR$_USP        = 00000003            

SYSRUNDWN       IMAGE RUNDOWN SYSTEM SERVICE                     22-AUG-1978 00:21:23   VAX-11 MACRO X0.3-11               Page   8

SYMBOL TABLE                                                                                                                     (1)



PR$_WCSA       = 0000002C            SS$_EXTIDXFILE = 00000880            SS$_MSGNOTFND  = 00000621            

PR$_WCSD       = 0000002D            SS$_FCPREADERR = 00000888            SS$_MUSTCLOSEFL= 00000948            

SCH$NEWLVL       ********   X   01   SS$_FCPREPSTN  = 00000988            SS$_NODATA     = 000001AC            

SS$_ABORT      = 0000002C            SS$_FCPREWNDERR= 00000890            SS$_NOHANDLER  = 000008F8            

SS$_ACCONFLICT = 00000800            SS$_FCPSPACERR = 00000898            SS$_NOHOMEBLK  = 000008E0            

SS$_ACCVIO     = 0000000C            SS$_FCPWRITERR = 000008A0            SS$_NOIOCHAN   = 000001B4            

SS$_ARITH      = 00000404            SS$_FILACCERR  = 0000009C            SS$_NOLINKS    = 0000027C            

SS$_ASTFLT     = 0000040C            SS$_FILALRACC  = 000000A4            SS$_NOLOGNAM   = 000001BC            

SS$_BADATTRIB  = 00000034            SS$_FILELOCKED = 000008A8            SS$_NOMBX      = 00000274            

SS$_BADCHKSUM  = 00000808            SS$_FILENUMCHK = 000008B0            SS$_NOMOREFILES= 00000930            

SS$_BADESCAPE  = 0000003C            SS$_FILESEQCHK = 000008B8            SS$_NONEXDRV   = 000001C4            

SS$_BADFILEHDR = 00000810            SS$_FILESTRUCT = 000008C0            SS$_NONEXPR    = 000008E8            

SS$_BADFILENAME= 00000818            SS$_FILNOTACC  = 000000AC            SS$_NONLOCAL   = 000008F0            

SS$_BADFILEVER = 00000820            SS$_FILNOTCNTG = 000002AC            SS$_NOPRIV     = 00000024            

SS$_BADIMGHDR  = 00000044            SS$_FILNOTEXP  = 000000B4            SS$_NORMAL     = 00000001            

SS$_BADIRECTORY= 00000828            SS$_FORMAT     = 000000BC            SS$_NOSIGNAL   = 00000900            

SS$_BADPARAM   = 00000014            SS$_GPTFULL    = 000000C4            SS$_NOSOLICIT  = 00000284            

SS$_BADSTACK   = 000002B4            SS$_GSDFULL    = 000000CC            SS$_NOSUCHDEV  = 00000908            

SS$_BEGOFFILE  = 00000938            SS$_GSDNOTXXX  = 000000D4            SS$_NOSUCHFILE = 00000910            

SS$_BLOCKCNTERR= 00000940            SS$_HANGUP     = 000002CC            SS$_NOSUCHNODE = 0000028C            

SS$_BREAK      = 00000414            SS$_HEADERFULL = 000008C8            SS$_NOSUCHSEC  = 00000978            

SS$_BUFFEROVF  = 00000601            SS$_IDXFILEFULL= 000008D0            SS$_NOTAPEOP   = 00000264            

SS$_BUGCHECK   = 000002A4            SS$_ILLBLKNUM  = 000000DC            SS$_NOTFILEDEV = 000001CC            

SS$_CANCEL     = 00000830            SS$_ILLCNTRFUNC= 000000E4            SS$_NOTINTBLSZ = 000001D4            

SS$_CHANINTLK  = 0000004C            SS$_ILLEFC     = 000000EC            SS$_NOTLABELMT = 000001DC            

SS$_CLIFRCEXT  = 00000980            SS$_ILLIOFUNC  = 000000F4            SS$_NOTNETDEV  = 000002EC            

SS$_CMODSUPR   = 0000041C            SS$_ILLLBLAST  = 00000968            SS$_NOTRAN     = 00000629            

SS$_CMODUSER   = 00000424            SS$_ILLPAGCNT  = 000000FC            SS$_NOTSQDEV   = 000001E4            

SS$_COMPAT     = 0000042C            SS$_ILLSEQOP   = 000002DC            SS$_OPCCUS     = 00000434            

SS$_CONTINUE   = 00000001            SS$_ILLSER     = 00000104            SS$_OPCDEC     = 0000043C            

SS$_CONTROLC   = 00000651            SS$_ILLUSRLBLRD= 00000958            SS$_OPINCOMPL  = 000002D4            

SS$_CONTROLO   = 00000609            SS$_ILLUSRLBLWT= 00000960            SS$_PAGOWNVIO  = 000001EC            

SS$_CONTROLY   = 00000611            SS$_INCVOLLABEL= 0000010C            SS$_PAGRDERR   = 00000444            

SS$_CREATED    = 00000619            SS$_INSFARG    = 00000114            SS$_PARITY     = 000001F4            

SS$_CTRLERR    = 00000054            SS$_INSFMEM    = 00000124            SS$_PARTESCAPE = 000001FC            

SS$_DATACHECK  = 0000005C            SS$_INSFRAME   = 0000012C            SS$_PFMBSY     = 00000204            

SS$_DATAOVERUN = 00000838            SS$_INSFWSL    = 0000011C            SS$_PSTFULL    = 0000020C            

SS$_DEBUG      = 0000046C            SS$_IVADDR     = 00000134            SS$_RADRMOD    = 0000044C            

SS$_DEVACTIVE  = 000002C4            SS$_IVCHAN     = 0000013C            SS$_REJECT     = 00000294            

SS$_DEVALLOC   = 00000840            SS$_IVCHNLSEC  = 0000026C            SS$_REMOTE     = 00000649            

SS$_DEVALRALLOC= 00000641            SS$_IVDEVNAM   = 00000144            SS$_RESIGNAL   = 00000918            

SS$_DEVASSIGN  = 00000848            SS$_IVGSDNAM   = 0000014C            SS$_RESULTOVF  = 00000214            

SS$_DEVFOREIGN = 00000064            SS$_IVLOGNAM   = 00000154            SS$_ROPRAND    = 00000454            

SS$_DEVICEFULL = 00000850            SS$_IVLOGTAB   = 0000015C            SS$_SECTBLFUL  = 0000021C            

SS$_DEVMOUNT   = 0000006C            SS$_IVPROTECT  = 000002F4            SS$_SSFAIL     = 0000045C            

SS$_DEVNOTALLOC= 00000858            SS$_IVQUOTAL   = 00000164            SS$_SUPERSEDE  = 00000631            

SS$_DEVNOTMBX  = 00000074            SS$_IVSECFLG   = 0000016C            SS$_TAPEPOSLOST= 00000224            

SS$_DEVNOTMOUNT= 0000007C            SS$_IVSECIDCTL = 000002E4            SS$_TBIT       = 00000464            

SS$_DEVOFFLINE = 00000084            SS$_IVSSRQ     = 00000174            SS$_TIMEOUT    = 0000022C            

SS$_DIRFULL    = 00000860            SS$_IVSTSFLG   = 0000017C            SS$_TOOMANYVER = 00000990            

SS$_DRVERR     = 0000008C            SS$_IVTIME     = 00000184            SS$_TOOMUCHDATA= 0000029C            

SS$_DUPFILENAME= 00000868            SS$_LENVIO     = 0000018C            SS$_UNASEFC    = 00000234            

SS$_DUPLNAM    = 00000094            SS$_LKWSETFUL  = 00000194            SS$_UNSAFE     = 0000023C            

SS$_ENDOFFILE  = 00000870            SS$_MBFULL     = 000008D8            SS$_UNWIND     = 00000920            

SS$_ENDOFTAPE  = 00000878            SS$_MBTOOSML   = 0000019C            SS$_UNWINDING  = 00000928            

SS$_ENDOFUSRLBL= 00000970            SS$_MCHECK     = 000002BC            SS$_VASFULL    = 00000244            

SS$_EXQUOTA    = 0000001C            SS$_MEDOFL     = 000001A4            SS$_VECINUSE   = 0000024C            

SYSRUNDWN       IMAGE RUNDOWN SYSTEM SERVICE                     22-AUG-1978 00:21:23   VAX-11 MACRO X0.3-11               Page   9

SYMBOL TABLE                                                                                                                     (1)



SS$_VOLINV     = 00000254            

SS$_WAITUSRLBL = 00000950            

SS$_WASCLR     = 00000001            

SS$_WASECC     = 00000639            

SS$_WASSET     = 00000009            

SS$_WRITLCK    = 0000025C            

SYS$DALLOC       ********   X   01   

SYS$DASSGN       ********   X   01   

SYS$DELLOG       ********   X   01   





PROGRAM SECTION SYNOPSIS



.  ABS  .        00000000      00     NOPIC   USR   CON   ABS   LCL NOSHR NOEXE NORD  NOWRT BYTE  

. BLANK .        000000FB      01     NOPIC   USR   CON   REL   LCL NOSHR   EXE   RD    WRT BYTE  

$ABS$            0000007C      02     NOPIC   USR   CON   ABS   LCL NOSHR   EXE   RD    WRT BYTE  





THERE WERE NO ERRORS OR WARNINGS.

15220. BYTES LEFT IN FREE MEMORY POOL.

2958. BYTES OF RECLAIMED MEMORY.

OBJ$:SYSRUNDWN,LIS$:SYSRUNDWN/-SP=LIB$:LIB/ML,SRC$:SYSRUNDWN

4 MLB DIR RDS - 601 GETS TO DEFINE 21 MACROS. 40 INTER. FILE WRITES. 

