TTYDRVDAT       - TERMINAL DRIVER DATA BASE                      21-AUG-1978 21:01:39   VAX-11 MACRO X0.3-11               Page   0

TABLE OF CONTENTS   



   (2)     214  ESCAPE SYNTAX TABLE

   (3)     266  DRIVER DISPATCH TABLE AND FUNCTION DECISION TAB

   (4)     311  TERMINATOR BITMASK FOR STANDARD SET

   (5)     321  SPECIAL STRINGS

TTYDRVDAT       - TERMINAL DRIVER DATA BASE                      21-AUG-1978 21:01:39   VAX-11 MACRO X0.3-11               Page   1

V06                                                                                                                              (1)



                                     0000     1 	.TITLE	TTYDRVDAT - TERMINAL DRIVER DATA BASE

                                     0000     2 	.IDENT	/V06/

                                     0000     3 ;

                                     0000     4 ; COPYRIGHT (C) 1978

                                     0000     5 ; DIGITAL EQUIPMENT CORPORATION, MAYNARD, MASS.

                                     0000     6 ;

                                     0000     7 ; THIS SOFTWARE IS FURNISHED UNDER  A LICENSE FOR USE ONLY  ON  A

                                     0000     8 ; SINGLE COMPUTER SYSTEM AND MAY BE  COPIED ONLY WITH  THE INCLU-

                                     0000     9 ; SION OF  THE  ABOVE  COPYRIGHT NOTICE.  THIS SOFTWARE,  OR  ANY

                                     0000    10 ; OTHER COPIES THEREOF, MAY NOT BE  PROVIDED  OR  OTHERWISE  MADE

                                     0000    11 ; AVAILABLE TO ANY OTHER PERSON EXCEPT  FOR  USE  ON  SUCH SYSTEM

                                     0000    12 ; AND TO  ONE WHO AGREES  TO  THESE LICENSE  TERMS.  TITLE TO AND

                                     0000    13 ; OWNERSHIP OF THE SOFTWARE SHALL AT ALL TIMES REMAIN IN DEC.

                                     0000    14 ;

                                     0000    15 ; THE INFORMATION IN THIS SOFTWARE  IS  SUBJECT TO CHANGE WITHOUT

                                     0000    16 ; NOTICE AND SHOULD NOT BE CONSTRUED  AS  A COMMITMENT BY DIGITAL

                                     0000    17 ; EQUIPMENT CORPORATION.

                                     0000    18 ;

                                     0000    19 ; DEC ASSUMES NO RESPONSIBILITY FOR THE USE OR RELIABILITY OF ITS

                                     0000    20 ; SOFTWARE ON EQUIPMENT WHICH IS NOT SUPPLIED BY DEC.

                                     0000    21 

                                     0000    22 ;++

                                     0000    23 ; FACILITY:

                                     0000    24 ;

                                     0000    25 ;	VAX/VMS TERMINAL DRIVER

                                     0000    26 ;

                                     0000    27 ; ABSTRACT:

                                     0000    28 ;

                                     0000    29 ;	TERMINAL DRIVER DATA BASE

                                     0000    30 ;

                                     0000    31 ; AUTHOR:

                                     0000    32 ;	R.HEINEN 14-JUN-1977

                                     0000    33 ;--

                                     0000    34  

                                     0000    35 ;

                                     0000    36 ; EXTERNAL DEFINITIONS

                                     0000    37 ;

                                     0000    38 	$IODEF				; DEFINE I/O FUNCTION CODES

                                     0000    39 	$TTYDEF				; DEFINE TERMINAL DRIVER SYMBOLS

                                     0000    40 	$TTDEF				; DEFINE TERMINAL CHARACTERISTICS

                                     0000    41 	$UCBDEF				; DEFINE UCB

                                     0000    42 	$TTYUCBDEF			; DEFINE TERMINAL DRIVER SYMBOLS

                                     0000    43 ;

                                     0000    44 ; LOCAL DATA STORAGE

                                     0000    45 ;

                                     0000    46 	.MACRO	TYPE	TYP

                                     0000    47 	CHAR=CHAR+1

                                     0000    48 	Y=0

                                     0000    49 	.IF	NB	TYP

                                     0000    50 	Y=XY'TYP

                                     0000    51 	XY'TYP=1+XY'TYP

                                     0000    52 	.IF	IDN	CONTROL,TYP

                                     0000    53 	Y=Y!<TTY$M_CH_CTRL>

                                     0000    54 	.ENDC

                                     0000    55 	.IF	IDN	SPEC,TYP

                                     0000    56 	Y=Y!<TTY$M_CH_SPEC>

                                     0000    57 	.ENDC

TTYDRVDAT       - TERMINAL DRIVER DATA BASE                      21-AUG-1978 21:01:39   VAX-11 MACRO X0.3-11               Page   2

V06                                                                                                                              (1)



                                     0000    58 	.IF	IDN	CTRL2,TYP

                                     0000    59 	Y=Y!<TTY$M_CH_CTRL2>

                                     0000    60 	.ENDC

                                     0000    61 	.ENDC

                                     0000    62 	.IF	GE	CHAR-97

                                     0000    63 	.IF	LE	CHAR-97-26

                                     0000    64 	Y=Y!<TTY$M_CH_LOWER>

                                     0000    65 	.ENDC

                                     0000    66 	.ENDC

                                     0000    67 	.BYTE	Y

                                     0000    68 	.ENDM

                                     0000    69  

                                 00000000    70 	.PSECT	$$$115_DRIVER,LONG	; DEFINE I/O DRIVER NON PAGED 

                                     0000    71  

                                     0000    72 ;

                                     0000    73 ; CHARACTERISTICS FOR CHARACTER ECHO AND TERMINATION DETECTION

                                     0000    74 ;

                                     0000    75 ;

                           00000000  0000    76 CHAR=0

                           00000000  0000    77 XYSPEC=0

                           00000000  0000    78 XYCONTROL=0

                           00000000  0000    79 XYCTRL2=0

                                     0000    80 ;

                                     0000    81 TTY$A_TYPE::

                                     0000    82 	TYPE				; NULL

                                     0001    83 	TYPE				; CONTROL A

                                     0002    84 	TYPE				; CONTROL B

                                     0003    85 	TYPE	CONTROL			; CONTROL C

                                     0004    86 	TYPE				; CONTROL D

                                     0005    87 	TYPE				; CONTROL E

                                     0006    88 	TYPE				; CONTROL F

                                     0007    89 	TYPE				; BELL CONTROL G

                                     0008    90 	TYPE	SPEC			; BACKSPACE

                                     0009    91 	TYPE	SPEC			; TAB

                                     000A    92 	TYPE	SPEC			; LINE FEED

                                     000B    93 	TYPE	SPEC			; VERTICLE TAB

                                     000C    94 	TYPE	SPEC			; FORM FEED

                                     000D    95 	TYPE	SPEC			; CARRIAGE RETURN

                                     000E    96 	TYPE				; CONTROL N

                                     000F    97 	TYPE	CONTROL			; CONTROL O

                                     0010    98 	TYPE				; CONTROL P

                                     0011    99 	TYPE	CONTROL			; CONTROL Q

                                     0012   100 	TYPE	CTRL2			; CONTROL R

                                     0013   101 	TYPE	CONTROL			; CONTROL S

                                     0014   102 	TYPE				; CONTROL T

                                     0015   103 	TYPE	CTRL2			; CONTROL U

                                     0016   104 	TYPE				; CONTROL V

                                     0017   105 	TYPE				; CONTROL W

                                     0018   106 	TYPE	CONTROL			; CONTROL X

                                     0019   107 	TYPE	CONTROL			; CONTROL Y

                                     001A   108 	TYPE	SPEC			; CONTROL Z

                                     001B   109 	TYPE	SPEC			; ESCAPE

                                     001C   110 	TYPE				;

                                     001D   111 	TYPE				;

                                     001E   112 	TYPE				;

                                     001F   113 	TYPE				;

                                     0020   114 	TYPE				; SPACE

TTYDRVDAT       - TERMINAL DRIVER DATA BASE                      21-AUG-1978 21:01:39   VAX-11 MACRO X0.3-11               Page   3

V06                                                                                                                              (1)



                                     0021   115 	TYPE				; !

                                     0022   116 	TYPE				; "

                                     0023   117 	TYPE				; #

                                     0024   118 	TYPE				; $

                                     0025   119 	TYPE				; %

                                     0026   120 	TYPE				; &

                                     0027   121 	TYPE				; '

                                     0028   122 	TYPE				; (

                                     0029   123 	TYPE				; )

                                     002A   124 	TYPE				; *

                                     002B   125 	TYPE				; +

                                     002C   126 	TYPE				; ,

                                     002D   127 	TYPE				; -

                                     002E   128 	TYPE				; .

                                     002F   129 	TYPE				; /

                                     0030   130 	TYPE				; 0

                                     0031   131 	TYPE				; 1

                                     0032   132 	TYPE				; 2

                                     0033   133 	TYPE				; 3

                                     0034   134 	TYPE				; 4

                                     0035   135 	TYPE				; 5

                                     0036   136 	TYPE				; 6

                                     0037   137 	TYPE				; 7

                                     0038   138 	TYPE				; 8

                                     0039   139 	TYPE				; 9

                                     003A   140 	TYPE				; :

                                     003B   141 	TYPE				; ; 

                                     003C   142 	TYPE				; <

                                     003D   143  	TYPE				; =

                                     003E   144 	TYPE				; >

                                     003F   145 	TYPE				; ?

                                     0040   146 	TYPE				; @

                                     0041   147 	TYPE				; A

                                     0042   148 	TYPE				; B

                                     0043   149 	TYPE				; C

                                     0044   150 	TYPE				; D

                                     0045   151 	TYPE				; E

                                     0046   152 	TYPE				; F

                                     0047   153 	TYPE				; G

                                     0048   154 	TYPE				; H

                                     0049   155 	TYPE				; I

                                     004A   156 	TYPE				; J

                                     004B   157 	TYPE				; K

                                     004C   158 	TYPE				; L

                                     004D   159 	TYPE				; M

                                     004E   160 	TYPE				; N

                                     004F   161 	TYPE				; O

                                     0050   162 	TYPE				; P

                                     0051   163 	TYPE				; Q

                                     0052   164 	TYPE				; R

                                     0053   165 	TYPE				; S

                                     0054   166 	TYPE				; T

                                     0055   167 	TYPE				; U

                                     0056   168 	TYPE				; V

                                     0057   169 	TYPE				; W

                                     0058   170 	TYPE				; X

                                     0059   171 	TYPE				; Y

TTYDRVDAT       - TERMINAL DRIVER DATA BASE                      21-AUG-1978 21:01:39   VAX-11 MACRO X0.3-11               Page   4

V06                                                                                                                              (1)



                                     005A   172 	TYPE				; Z

                                     005B   173 	TYPE				; [

                                     005C   174 	TYPE				; \

                                     005D   175 	TYPE				; ]

                                     005E   176 	TYPE				; ^

                                     005F   177 	TYPE				; _

                                     0060   178 	TYPE				; ELISPE

                                     0061   179 	TYPE				; LOWER A

                                     0062   180 	TYPE				; LOWER B

                                     0063   181 	TYPE				; LOWER C

                                     0064   182 	TYPE				; LOWER D

                                     0065   183 	TYPE				; LOWER E

                                     0066   184 	TYPE				; LOWER F

                                     0067   185 	TYPE				; LOWER G

                                     0068   186 	TYPE				; LOWER H

                                     0069   187 	TYPE				; LOWER I

                                     006A   188 	TYPE				; LOWER J

                                     006B   189 	TYPE				; LOWER K

                                     006C   190 	TYPE				; LOWER L

                                     006D   191 	TYPE				; LOWER M

                                     006E   192 	TYPE				; LOWER N

                                     006F   193 	TYPE				; LOWER O

                                     0070   194 	TYPE				; LOWER P

                                     0071   195 	TYPE				; LOWER Q

                                     0072   196 	TYPE				; LOWER R

                                     0073   197 	TYPE				; LOWER S

                                     0074   198 	TYPE				; LOWER T

                                     0075   199 	TYPE				; LOWER U

                                     0076   200 	TYPE				; LOWER V

                                     0077   201 	TYPE				; LOWER W

                                     0078   202 	TYPE				; LOWER X

                                     0079   203 	TYPE				; LOWER Y

                                     007A   204 	TYPE				; LOWER Z

                                     007B   205 	TYPE				; CURRLY LEFT

                                     007C   206 	TYPE				; UP LINE

                                     007D   207 	TYPE				; CURRLY RIGHT

                                     007E   208 	TYPE	CTRL2			; WIGGLE

                                     007F   209 	TYPE	CTRL2			; DELETE

                                     0080   210 	.REPT	128

                                     0080   211 	TYPE

                                     0080   212 	.ENDR

TTYDRVDAT       - TERMINAL DRIVER DATA BASE                      21-AUG-1978 21:01:39   VAX-11 MACRO X0.3-11               Page   5

V06             ESCAPE SYNTAX TABLE                                                                                              (2)



                                     0100   214 	.SBTTL	ESCAPE SYNTAX TABLE

                                     0100   215 ;

                                     0100   216 ; ESCAPE SYNTAX TABLE

                                     0100   217 ;

                                     0100   218 TTY$A_ESCAPE::				; ESCAPE SYNTAX TABLE

                                     0100   219 ;

                                     0100   220 ; ESCAPE SEQUENCE <ESC><;><32:47>....<48:126>

                                     0100   221 ;

                              3B 3B  0100   222 	.ASCII	/;;/			; ";"

                                 0F' 0102   223 	.BYTE	10$-TTY$A_ESCAPE	;

                                     0103   224 ;

                                     0103   225 ; ESCAPE SEQUENCE <ESC><?><32:47>....<48:126>

                                     0103   226 ;

                              3F 3F  0103   227 	.ASCII	/??/			; "?"

                                 0F' 0105   228 	.BYTE	10$-TTY$A_ESCAPE	;

                                     0106   229 ;

                                     0106   230 ; ESCAPE SEQUENCE <ESC><O><32:47>....<64:126>

                                     0106   231 ;

                              4F 4F  0106   232 	.ASCII	/OO/			; "O"

                                 15' 0108   233 	.BYTE	20$-TTY$A_ESCAPE	;

                                     0109   234 ;

                                     0109   235 ; ESCAPE SEQUENCE <ESC><P><32:47>....<48:126>

                                     0109   236 ;

                              50 50  0109   237 	.ASCII	/PP/			; "P"

                                 0F' 010B   238 	.BYTE	10$-TTY$A_ESCAPE	;

                                     010C   239 ;

                                     010C   240 ; ESCAPE SEQUENCE <ESC><Y><32:126><32:126>

                                     010C   241 ;

                              59 59  010C   242 	.ASCII	/YY/			; "Y"

                                 1A' 010E   243 	.BYTE	30$-TTY$A_ESCAPE	;

                                     010F   244 ;

                                     010F   245 ; ESCAPE SEQUENCE <ESC><32:47>....<48:126>

                                     010F   246 ;

                              2F 20  010F   247 10$:	.ASCII	! /!			; SPACE TO "/"

                                 0F' 0111   248 	.BYTE	10$-TTY$A_ESCAPE	; INTERMEDIATE CHARACTER

                              7E 30  0112   249 	.ASCII	/0/<126>		; "0" TO END

                                 00  0114   250 	.BYTE	0			; FINAL

                              2F 20  0115   251 20$:	.ASCII	! /!			; SPACE TO "/"

                                 15' 0117   252 	.BYTE	20$-TTY$A_ESCAPE

                              7E 40  0118   253 	.ASCII	/@/<126>		; "@" TO END

                              7E 20  011A   254 30$:	.ASCII	! !<126>		; SPACE TO END

                                 1D' 011C   255 	.BYTE	40$-TTY$A_ESCAPE

                              7E 20  011D   256 40$:	.ASCII	! !<126>		;

                                 00  011F   257 	.BYTE	0			;

                                     0120   258 ;

                                     0120   259 ; ESCAPE SEQUENCES WITH MEANING FOR OUTPUT

                                     0120   260 ;

                                     0120   261 ; THERE IS A CORRELATION BETWEEN THIS TABLE AND CODE!

                                     0120   262 ;

                                     0120   263 TTY$A_ESC_OUT::

5A 4B 47 46 59 49 48 44 43 42 41 00' 0120   264 	.ASCIC	/ABCDHIYFGKZ>=\[/		;

                        5B 5C 3D 3E  012C       

                                 0F  0120       

TTYDRVDAT       - TERMINAL DRIVER DATA BASE                      21-AUG-1978 21:01:39   VAX-11 MACRO X0.3-11               Page   6

V06             DRIVER DISPATCH TABLE AND FUNCTION DECISION TAB                                                                  (3)



                                     0130   266 	.SBTTL	DRIVER DISPATCH TABLE AND FUNCTION DECISION TABLE

                                     0130   267 ;

                                     0130   268 ; DRIVER DISPATCH TABLE

                                     0130   269 ;

                                     0130   270 	DDTAB	TT,-			; DRIVER DISPATCH TABLE

                                     0130   271 		+TTY$STARTIO,-		; START IO OPERATION

                                     0130   272 		0,-			; UNEXPECTED INTERRUPT

                                     0130   273 		FUNCTION,-		; FUNCTION DECISION TABLE

                                     0130   274 		+TTY$CANCELIO,-		; CANCEL I/O

                                     0130   275 		0,-			; REGISTER DUMP ROUTINE

                                     0130   276 		0,-			; SIZE OF DIAGNOSTIC BUFFER

                                     0130   277 		0			; SIZE OF ERROR LOG BUFFER

                                     0148   278 ;

                                     0148   279 ; FUNCTION DECISION TABLE FOR ALL TERMINALS

                                     0148   280 ;

                                     0148   281 FUNCTION:

                                     0148   282 	FUNCTAB	,-			; LEGAL FUNCTIONS

                                     0148   283 		<READLBLK,-

                                     0148   284 		WRITELBLK,-

                                     0148   285 		READVBLK,-

                                     0148   286 		WRITEVBLK,-

                                     0148   287 		READPBLK,-

                                     0148   288 		WRITEPBLK,-

                                     0148   289 		READPROMPT,-

                                     0148   290 		SETMODE,-

                                     0148   291 		SETCHAR,-

                                     0148   292 		SENSEMODE,-

                                     0148   293 		SENSECHAR,-

                                     0148   294 		>

                                     0150   295 	FUNCTAB	,-			; BUFFERED I/O FUNCTIONS

                                     0150   296 		<READLBLK,-

                                     0150   297 		WRITELBLK,-

                                     0150   298 		READVBLK,-

                                     0150   299 		WRITEVBLK-

                                     0150   300 		READPBLK,-

                                     0150   301 		READPROMPT,-

                                     0150   302 		WRITEPBLK,-

                                     0150   303 		>

                                     0158   304 	FUNCTAB	+TTY$FDTREAD,<READLBLK,READVBLK,READPBLK,READPROMPT>

                                     0164   305 	FUNCTAB	+TTY$FDTWRITE,<WRITELBLK,WRITEVBLK,WRITEPBLK>

                                     0170   306 	FUNCTAB +TTY$FDTSETM,<SETMODE>

                                     017C   307 	FUNCTAB	+TTY$FDTSETC,<SETCHAR>

                                     0188   308 	FUNCTAB +TTY$FDTSENSEM,<SENSEMODE>

                                     0194   309 	FUNCTAB	+TTY$FDTSENSEC,<SENSECHAR>

TTYDRVDAT       - TERMINAL DRIVER DATA BASE                      21-AUG-1978 21:01:39   VAX-11 MACRO X0.3-11               Page   7

V06             TERMINATOR BITMASK FOR STANDARD SET                                                                              (4)



                                     01A0   311 	.SBTTL	TERMINATOR BITMASK FOR STANDARD SET

                                     01A0   312 ;

                                     01A0   313 ;

                                     01A0   314 ;

                                     01A0   315 TTY$A_STANDARD::				;

                           FFFFE0FF  01A0   316 		.LONG	^X0FFFFE0FF		; BS,TAB,LF,VT,FORM NOT TERMS

         80000000 00000000 00000000  01A4   317 		.LONG	0,0,^X80000000		; AND DELETE

                           FFFFE0FF  01B0   318 		.LONG	^X0FFFFE0FF		;

         80000000 00000000 00000000  01B4   319 		.LONG	0,0,^X80000000	

TTYDRVDAT       - TERMINAL DRIVER DATA BASE                      21-AUG-1978 21:01:39   VAX-11 MACRO X0.3-11               Page   8

V06             SPECIAL STRINGS                                                                                                  (5)



                                     01C0   321 	.SBTTL	SPECIAL STRINGS

                                     01C0   322 ;

                                     01C0   323 ; MULTI ECHO STRINGS

                                     01C0   324 ;

                                     01C0   325 ; TAB STRINGS

                                     01C0   326 ;

         00 20 20 20 20 20 20 20 20  01C0   327 TTY$A_TAB::		.ASCIZ	/        /

                                     01C9   328 ;

                                     01C9   329 ; BACKSPACE STRING

                                     01C9   330 ;

            00 08'08'08'08'08'08'08' 01C9   331 TTY$A_DELCRTTAB::	.BYTE	TTY$C_BS,TTY$C_BS,TTY$C_BS,TTY$C_BS,TTY$C_BS,TTY$C_BS,TTY$C_

                           08'20'08' 01D1   332 TTY$A_BACKSPACE::	.BYTE	TTY$C_BS,TTY$C_BLANK,TTY$C_BS

                                 00  01D4   333 		.BYTE	0

                                     01D5   334 ;

                                     01D5   335 ; UTILITY STRINGS

                                     01D5   336 ;

                                     01D5   337 ; THE ORGANIZATION OF THIS TABLE IS CRITICAL

                                     01D5   338 ;

                                     01D5   339 ;

                           00 5B 1B  01D5   340 TTY$A_HLDSCREEN::	.BYTE	^O033,^O0133,0

                           00 5C 1B  01D8   341 TTY$A_RLSCREEN::	.BYTE	^O033,^O0134,0

                           00 1B 60  01DB   342 TTY$A_SCRIPT::	.BYTE	^X060,^X01B,0	; ELIPSE-ESCAPE-END

                        00 0D'5A 5E  01DE   343 TTY$A_CTRLZ::	.ASCIZ	/^Z/<TTY$C_CR>

                        00 0D'55 5E  01E2   344 TTY$A_CTRLU::	.ASCIZ	/^U/<TTY$C_CR>

                        00 0D'52 5E  01E6   345 TTY$A_CTRLR::	.ASCIZ	/^R/<TTY$C_CR>

                              5C 1B  01EA   346 		.BYTE	^O033,^O0134

               00 0A 0D 59 5E 0A 0D  01EC   347 TTY$A_CTRLY::	.ASCIZ	<13><10>/^Y/<13><10>

                              5C 1B  01F3   348 		.BYTE	^O033,^O0134

               00 0A 0D 43 5E 0A 0D  01F5   349 TTY$A_CTRLC::	.ASCIZ	<13><10>/^C/<13><10>

                     00 0A 0D 4F 5E  01FC   350 TTY$A_CTRLO::	.ASCIZ	/^O/<13><10>

                                     0201   351 ;

                                     0201   352 ; VTAB AND FORM

                                     0201   353 ;

                        0A'0A'0A'0A' 0201   354 TTY$A_VTAB::		.BYTE	TTY$C_LF,TTY$C_LF,TTY$C_LF,TTY$C_LF

                                 00  0205   355 TTY$A_FORM::		.BYTE	0

                     0C'0A'0A'0A'0A' 0206   356 TTY$A_LONGFORM::	.BYTE	TTY$C_LF,TTY$C_LF,TTY$C_LF,TTY$C_LF,TTY$C_FF

                                     020B   357 ;

                                     020B   358 	.END

TTYDRVDAT       - TERMINAL DRIVER DATA BASE                      21-AUG-1978 21:01:39   VAX-11 MACRO X0.3-11               Page   9

SYMBOL TABLE                                                                                                                     (5)



BIT...         = 00000008            IO$V_DSABLMBX  = 0000000A            IO$_SETCHAR    = 0000001A            

CHAR           = 00000100            IO$V_ENABLMBX  = 00000007            IO$_SETMODE    = 00000023            

FUNCTION         00000148 R     03   IO$V_FCODE     = 00000000            IO$_SKIPFILE   = 00000025            

GBL...         = 00000000            IO$V_HANGUP    = 00000009            IO$_SKIPRECORD = 00000026            

IO$M_ABORT     = 00000100            IO$V_INHERLOG  = 0000000B            IO$_SPACEFILE  = 00000002            

IO$M_ACCESS    = 00000040            IO$V_INHEXTGAP = 0000000C            IO$_SPACERECORD= 00000009            

IO$M_ATTNAST   = 00000100            IO$V_INHRETRY  = 0000000F            IO$_STARTSPNDL = 00000019            

IO$M_BINARY    = 00000040            IO$V_INHSEEK   = 0000000C            IO$_UNLOAD     = 00000001            

IO$M_CANCTRLO  = 00000040            IO$V_INTERRUPT = 00000006            IO$_VIRTUAL    = 0000003F            

IO$M_COMMOD    = 00000040            IO$V_INTSKIP   = 00000008            IO$_WRITECHECK = 0000000A            

IO$M_CREATE    = 00000080            IO$V_MOUNT     = 00000009            IO$_WRITECHECKH= 00000018            

IO$M_CTRLCAST  = 00000100            IO$V_NOECHO    = 00000006            IO$_WRITEHEAD  = 0000000D            

IO$M_CTRLYAST  = 00000080            IO$V_NOFILTR   = 00000009            IO$_WRITELBLK  = 00000020            

IO$M_CVTLOW    = 00000100            IO$V_NOFORMAT  = 00000008            IO$_WRITEMARK  = 0000001C            

IO$M_DATACHECK = 00004000            IO$V_NOW       = 00000006            IO$_WRITEOF    = 00000028            

IO$M_DELETE    = 00000100            IO$V_NOWAIT    = 00000007            IO$_WRITEPBLK  = 0000000B            

IO$M_DMOUNT    = 00000400            IO$V_PACKED    = 00000007            IO$_WRITETRACKD= 0000000F            

IO$M_DSABLMBX  = 00000400            IO$V_PURGE     = 0000000B            IO$_WRITEVBLK  = 00000030            

IO$M_ENABLMBX  = 00000080            IO$V_READATTN  = 00000007            IOC$RETURN       ********   X   03   

IO$M_FCODE     = 0000003F            IO$V_REVERSE   = 00000006            MASKH          = 00000000            

IO$M_HANGUP    = 00000200            IO$V_SHUTDOWN  = 00000007            MASKL          = 08000000            

IO$M_INHERLOG  = 00000800            IO$V_STARTUP   = 00000006            TT$C_BAUD_110  = 00000003            

IO$M_INHEXTGAP = 00001000            IO$V_SYNCH     = 00000009            TT$C_BAUD_1200 = 00000008            

IO$M_INHRETRY  = 00008000            IO$V_TIMED     = 00000007            TT$C_BAUD_134  = 00000004            

IO$M_INHSEEK   = 00001000            IO$V_TRMNOECHO = 0000000C            TT$C_BAUD_150  = 00000005            

IO$M_INTERRUPT = 00000040            IO$V_WRTATTN   = 00000008            TT$C_BAUD_1800 = 00000009            

IO$M_INTSKIP   = 00000100            IO$_ACCESS     = 00000032            TT$C_BAUD_2000 = 0000000A            

IO$M_MOUNT     = 00000200            IO$_ACPCONTROL = 00000038            TT$C_BAUD_2400 = 0000000B            

IO$M_NOECHO    = 00000040            IO$_CREATE     = 00000033            TT$C_BAUD_300  = 00000006            

IO$M_NOFILTR   = 00000200            IO$_DEACCESS   = 00000034            TT$C_BAUD_3600 = 0000000C            

IO$M_NOFORMAT  = 00000100            IO$_DELETE     = 00000035            TT$C_BAUD_4800 = 0000000D            

IO$M_NOW       = 00000040            IO$_DIAGNOSE   = 0000001D            TT$C_BAUD_50   = 00000001            

IO$M_NOWAIT    = 00000080            IO$_DRVCLR     = 00000004            TT$C_BAUD_600  = 00000007            

IO$M_PACKED    = 00000080            IO$_ERASETAPE  = 00000006            TT$C_BAUD_7200 = 0000000E            

IO$M_PURGE     = 00000800            IO$_LOGICAL    = 0000002F            TT$C_BAUD_75   = 00000002            

IO$M_READATTN  = 00000080            IO$_MODIFY     = 00000036            TT$C_BAUD_9600 = 0000000F            

IO$M_REVERSE   = 00000040            IO$_MOUNT      = 00000039            TT$DDT           00000130 RG    03   

IO$M_SHUTDOWN  = 00000080            IO$_NOP        = 00000000            TT$M_ALTRPAR   = 00000020            

IO$M_STARTUP   = 00000040            IO$_OFFSET     = 00000006            TT$M_CRFILL    = 00000400            

IO$M_SYNCH     = 00000200            IO$_PACKACK    = 00000008            TT$M_EIGHTBIT  = 00008000            

IO$M_TIMED     = 00000080            IO$_PHYSICAL   = 0000001F            TT$M_ESCAPE    = 00000008            

IO$M_TRMNOECHO = 00001000            IO$_READHEAD   = 0000000E            TT$M_HOLDSCREEN= 00004000            

IO$M_WRTATTN   = 00000100            IO$_READLBLK   = 00000021            TT$M_HOSTSYNC  = 00000010            

IO$S_FCODE     = 00000006            IO$_READPBLK   = 0000000C            TT$M_LFFILL    = 00000800            

IO$V_ABORT     = 00000008            IO$_READPRESET = 00000019            TT$M_LOWER     = 00000080            

IO$V_ACCESS    = 00000006            IO$_READPROMPT = 00000037            TT$M_MBXDSABL  = 00010000            

IO$V_ATTNAST   = 00000008            IO$_READTRACKD = 00000010            TT$M_MECHTAB   = 00000100            

IO$V_BINARY    = 00000006            IO$_READVBLK   = 00000031            TT$M_NOBRDCST  = 00020000            

IO$V_CANCTRLO  = 00000006            IO$_RECAL      = 00000003            TT$M_NOECHO    = 00000002            

IO$V_COMMOD    = 00000006            IO$_RELEASE    = 00000005            TT$M_NOTYPEAHD = 00000004            

IO$V_CREATE    = 00000007            IO$_RETCENTER  = 00000007            TT$M_ODD       = 00000080            

IO$V_CTRLCAST  = 00000008            IO$_REWIND     = 00000024            TT$M_PAGE      = FE000000            

IO$V_CTRLYAST  = 00000007            IO$_REWINDOFF  = 00000022            TT$M_PARITY    = 00000040            

IO$V_CVTLOW    = 00000008            IO$_SEARCH     = 00000009            TT$M_PASSALL   = 00000001            

IO$V_DATACHECK = 0000000E            IO$_SEEK       = 00000002            TT$M_READSYNC  = 00040000            

IO$V_DELETE    = 00000008            IO$_SENSECHAR  = 0000001B            TT$M_REMOTE    = 00002000            

IO$V_DMOUNT    = 0000000A            IO$_SENSEMODE  = 00000027            TT$M_SCOPE     = 00001000            

TTYDRVDAT       - TERMINAL DRIVER DATA BASE                      21-AUG-1978 21:01:39   VAX-11 MACRO X0.3-11               Page  10

SYMBOL TABLE                                                                                                                     (5)



TT$M_SCRIPT    = 00000040            TTY$B_BD_WHO     00000014            TTY$L_RB_UVA     00000004            

TT$M_TTSYNC    = 00000020            TTY$B_TA_TYPE    0000000A            TTY$L_TA_DATA    00000010            

TT$M_WRAP      = 00000200            TTY$CANCELIO     ********   X   03   TTY$L_TA_END     0000000C            

TT$S_PAGE      = 00000008            TTY$C_BELL     = 00000007            TTY$L_TA_GET     00000004            

TT$V_ALTRPAR   = 00000005            TTY$C_BLANK    = 00000020            TTY$L_TA_PUT     00000000            

TT$V_CRFILL    = 0000000A            TTY$C_BS       = 00000008            TTY$L_WB_DATA    0000000C            

TT$V_EIGHTBIT  = 0000000F            TTY$C_CR       = 0000000D            TTY$L_WB_END     00000004            

TT$V_ESCAPE    = 00000003            TTY$C_CTRLC    = 00000003            TTY$L_WB_NXT     00000000            

TT$V_HOLDSCREEN= 0000000E            TTY$C_CTRLO    = 0000000F            TTY$M_A        = 00003FFF            

TT$V_HOSTSYNC  = 00000004            TTY$C_CTRLQ    = 00000011            TTY$M_CH_CTRL  = 00000020            

TT$V_LFFILL    = 0000000B            TTY$C_CTRLR    = 00000012            TTY$M_CH_CTRL2 = 00000080            

TT$V_LOWER     = 00000007            TTY$C_CTRLS    = 00000013            TTY$M_CH_LOWER = 00000040            

TT$V_MBXDSABL  = 00000010            TTY$C_CTRLU    = 00000015            TTY$M_CH_SPEC  = 00000010            

TT$V_MECHTAB   = 00000008            TTY$C_CTRLX    = 00000018            TTY$M_ST_BADESC= 00100000            

TT$V_NOBRDCST  = 00000011            TTY$C_CTRLY    = 00000019            TTY$M_ST_BRDCST= 00000080            

TT$V_NOECHO    = 00000001            TTY$C_CTRLZ    = 0000001A            TTY$M_ST_CTRLO = 00001000            

TT$V_NOTYPEAHD = 00000002            TTY$C_DELETE   = 0000007F            TTY$M_ST_CTRLR = 00000400            

TT$V_ODD       = 00000007            TTY$C_DOLLAR   = 00000024            TTY$M_ST_CTRLS = 00000004            

TT$V_PAGE      = 00000019            TTY$C_DS_ACTIVE= 00000001            TTY$M_ST_CURSOR= 00000010            

TT$V_PARITY    = 00000006            TTY$C_DS_ATTN1 = 00000002            TTY$M_ST_DEL   = 00002000            

TT$V_PASSALL   = 00000000            TTY$C_DS_ATTN3 = 00000009            TTY$M_ST_EOL   = 00000200            

TT$V_READSYNC  = 00000012            TTY$C_DS_HANG  = 0000000A            TTY$M_ST_ESC   = 00080000            

TT$V_REMOTE    = 0000000D            TTY$C_DS_IDLE  = 00000000            TTY$M_ST_ESC_O = 04000000            

TT$V_SCOPE     = 0000000C            TTY$C_DS_RESET = 0000000B            TTY$M_ST_FILL  = 00000008            

TT$V_SCRIPT    = 00000006            TTY$C_ESCAPE   = 0000001B            TTY$M_ST_GETAHD= 01000000            

TT$V_TTSYNC    = 00000005            TTY$C_FC_N_SET = 00000004            TTY$M_ST_MULTI = 00000040            

TT$V_WRAP      = 00000009            TTY$C_FC_READ  = 00000000            TTY$M_ST_NL    = 00200000            

TT$_LA36       = 00000020            TTY$C_FC_SETC  = 00000003            TTY$M_ST_NOECHO= 00008000            

TT$_LAX        = 00000020            TTY$C_FC_SETM  = 00000002            TTY$M_ST_NOFLTR= 00040000            

TT$_UNKNOWN    = 00000000            TTY$C_FC_WRITE = 00000001            TTY$M_ST_PASALL= 00004000            

TT$_VT05       = 00000001            TTY$C_FF       = 0000000C            TTY$M_ST_PROMPT= 00020000            

TT$_VT52       = 00000040            TTY$C_HIGHIPL  = 00000016            TTY$M_ST_READ  = 00000800            

TT$_VT55       = 00000041            TTY$C_LF       = 0000000A            TTY$M_ST_SENDLF= 00000020            

TT$_VT5X       = 00000040            TTY$C_LOWA     = 00000061            TTY$M_ST_SKIPLF= 00800000            

TTY$A_BACKSPACE  000001D1 RG    03   TTY$C_LOWZ     = 0000007B            TTY$M_ST_TYPFUL= 00400000            

TTY$A_CTRLC      000001F5 RG    03   TTY$C_NL       = 00000080            TTY$M_ST_UNSOL = 02000000            

TTY$A_CTRLO      000001FC RG    03   TTY$C_ONE      = 00000031            TTY$M_ST_WRITE = 00000100            

TTY$A_CTRLR      000001E6 RG    03   TTY$C_PLUS     = 0000002B            TTY$M_ST_WRTALL= 00010000            

TTY$A_CTRLU      000001E2 RG    03   TTY$C_SCRIPT   = 00000060            TTY$M_ST_XOFF  = 00000002            

TTY$A_CTRLY      000001EC RG    03   TTY$C_TAB      = 00000009            TTY$M_ST_XON   = 00000001            

TTY$A_CTRLZ      000001DE RG    03   TTY$C_TYPAHDSIZ= 0000004E            TTY$Q_BD_LINK    00000000            

TTY$A_DELCRTTAB  000001C9 RG    03   TTY$C_VT       = 0000000B            TTY$STARTIO      ********   X   03   

TTY$A_ESCAPE     00000100 RG    03   TTY$C_XOFF     = 00000013            TTY$S_A        = 0000000E            

TTY$A_ESC_OUT    00000120 RG    03   TTY$C_XON      = 00000011            TTY$V_A        = 00000000            

TTY$A_FORM       00000205 RG    03   TTY$C_ZERO     = 00000030            TTY$V_CH_CTRL  = 00000005            

TTY$A_HLDSCREEN  000001D5 RG    03   TTY$FDTREAD      ********   X   03   TTY$V_CH_CTRL2 = 00000007            

TTY$A_LONGFORM   00000206 RG    03   TTY$FDTSENSEC    ********   X   03   TTY$V_CH_LOWER = 00000006            

TTY$A_RLSCREEN   000001D8 RG    03   TTY$FDTSENSEM    ********   X   03   TTY$V_CH_SPEC  = 00000004            

TTY$A_SCRIPT     000001DB RG    03   TTY$FDTSETC      ********   X   03   TTY$V_ST_BADESC= 00000014            

TTY$A_STANDARD   000001A0 RG    03   TTY$FDTSETM      ********   X   03   TTY$V_ST_BRDCST= 00000007            

TTY$A_TAB        000001C0 RG    03   TTY$FDTWRITE     ********   X   03   TTY$V_ST_CTRLO = 0000000C            

TTY$A_TYPE       00000000 RG    03   TTY$L_BD_DATA    00000018            TTY$V_ST_CTRLR = 0000000A            

TTY$A_VTAB       00000201 RG    03   TTY$L_BD_FORK    0000000C            TTY$V_ST_CTRLS = 00000002            

TTY$B_BD_CNT     00000015            TTY$L_BD_MIN     00000028            TTY$V_ST_CURSOR= 00000004            

TTY$B_BD_IPL     00000017            TTY$L_BD_UCB     00000010            TTY$V_ST_DEL   = 0000000D            

TTY$B_BD_REFC    00000016            TTY$L_RB_DATA    00000010            TTY$V_ST_EOL   = 00000009            

TTY$B_BD_TYPE    0000000A            TTY$L_RB_NXT     00000000            TTY$V_ST_ESC   = 00000013            

TTYDRVDAT       - TERMINAL DRIVER DATA BASE                      21-AUG-1978 21:01:39   VAX-11 MACRO X0.3-11               Page  11

SYMBOL TABLE                                                                                                                     (5)



TTY$V_ST_ESC_O = 0000001A            UCB$B_TT_LINE    00000094            UCB$M_DELMBX   = 00000002            

TTY$V_ST_FILL  = 00000003            UCB$B_TT_SPEED   0000009C            UCB$M_DIAGBUF  = 00000002            

TTY$V_ST_GETAHD= 00000018            UCB$B_TYPE       0000000A            UCB$M_DX_WRITE = 00000008            

TTY$V_ST_MULTI = 00000006            UCB$B_VERTSZ     0000003F            UCB$M_ECC      = 00000001            

TTY$V_ST_NL    = 00000015            UCB$C_LENGTH     00000074            UCB$M_ERLOGIP  = 00000004            

TTY$V_ST_NOECHO= 0000000F            UCB$C_LOGLNK   = 00000001            UCB$M_INT      = 00000002            

TTY$V_ST_NOFLTR= 00000012            UCB$K_LENGTH     00000074            UCB$M_INTTYPE  = 00000080            

TTY$V_ST_PASALL= 0000000E            UCB$L_AMB        00000054            UCB$M_JOB      = 00000001            

TTY$V_ST_PROMPT= 00000011            UCB$L_ASTQBL     00000010            UCB$M_MOUNTING = 00000200            

TTY$V_ST_READ  = 0000000B            UCB$L_ASTQFL     0000000C            UCB$M_NOCNVRT  = 00000004            

TTY$V_ST_SENDLF= 00000005            UCB$L_CPID       0000005C            UCB$M_NT_BFROVF= 00000004            

TTY$V_ST_SKIPLF= 00000017            UCB$L_CRB        00000020            UCB$M_NT_BREAK = 00000020            

TTY$V_ST_TYPFUL= 00000016            UCB$L_DDB        00000024            UCB$M_NT_NAME  = 00000010            

TTY$V_ST_UNSOL = 00000019            UCB$L_DEVCHAR    00000034            UCB$M_ONLINE   = 00000010            

TTY$V_ST_WRITE = 00000008            UCB$L_DEVDEPEND  0000003C            UCB$M_POWER    = 00000020            

TTY$V_ST_WRTALL= 00000010            UCB$L_DPC        00000080            UCB$M_PRMMBX   = 00000001            

TTY$V_ST_XOFF  = 00000001            UCB$L_DUETIM     0000005C            UCB$M_TIM      = 00000001            

TTY$V_ST_XON   = 00000000            UCB$L_DX_BFPNT   0000009C            UCB$M_TIMOUT   = 00000040            

TTY$W_BD_SIZE    00000008            UCB$L_DX_BUF     00000098            UCB$M_TT_NOTIF = 00000004            

TTY$W_RB_ORGHOR  0000000C            UCB$L_DX_RXDB    000000A0            UCB$M_TT_ODD   = 00000080            

TTY$W_RB_SIZE    00000008            UCB$L_EMB        00000078            UCB$M_TT_PARTY = 00000040            

TTY$W_RB_TIMOS   0000000E            UCB$L_FIRST      00000014            UCB$M_TT_SPEED = 0000003F            

TTY$W_TA_SIZE    00000008            UCB$L_FPC        0000000C            UCB$M_TT_TIMO  = 00000002            

TTY$W_WB_SIZE    00000008            UCB$L_FQBL       00000004            UCB$M_UNLOAD   = 00001000            

UCB$B_AMOD       00000053            UCB$L_FQFL       00000000            UCB$M_VALID    = 00000800            

UCB$B_CEX        00000077            UCB$L_FR3        00000010            UCB$S_LNKPRI   = 00000002            

UCB$B_CM1        0000004A            UCB$L_FR4        00000014            UCB$S_LTYPE    = 00000002            

UCB$B_CM2        0000004B            UCB$L_IOQBL      00000044            UCB$S_TT_ODD   = 00000001            

UCB$B_DEVCLASS   00000038            UCB$L_IOQFL      00000040            UCB$S_TT_PARTY = 00000001            

UCB$B_DEVTYPE    00000039            UCB$L_IRP        0000004C            UCB$S_TT_SPEED = 00000006            

UCB$B_DIPL       00000052            UCB$L_LINK       0000002C            UCB$T_PARTNER    0000000C            

UCB$B_DX_SCTCNT  000000A6            UCB$L_LOGADR     00000064            UCB$V_BACKP    = 00000005            

UCB$B_ERTCNT     00000070            UCB$L_MAXBLOCK   00000084            UCB$V_BSY      = 00000008            

UCB$B_ERTMAX     00000071            UCB$L_MEDIA      0000008C            UCB$V_CANCEL   = 00000003            

UCB$B_ESCAPE     0000004B            UCB$L_NT_DATSSB  00000074            UCB$V_DEADMO   = 0000000A            

UCB$B_FEX        00000076            UCB$L_NT_INTSSB  00000078            UCB$V_DELMBX   = 00000001            

UCB$B_FIPL       0000000B            UCB$L_OPCNT      00000060            UCB$V_DIAGBUF  = 00000001            

UCB$B_LOCSRV     0000003C            UCB$L_OWNUIC     0000001C            UCB$V_DX_WRITE = 00000003            

UCB$B_OFFNDX     00000094            UCB$L_PID        00000028            UCB$V_ECC      = 00000000            

UCB$B_OFFRTC     00000095            UCB$L_RQBL       00000004            UCB$V_ERLOGIP  = 00000002            

UCB$B_REMSRV     0000003D            UCB$L_RQFL       00000000            UCB$V_INT      = 00000001            

UCB$B_SECTORS    0000003C            UCB$L_SVAPTE     00000068            UCB$V_INTTYPE  = 00000007            

UCB$B_SLAVE      00000074            UCB$L_SVPN       00000064            UCB$V_JOB      = 00000000            

UCB$B_SPR        00000075            UCB$L_TTCHAR     0000003C            UCB$V_LNKPRI   = 00000006            

UCB$B_STATE      00000052            UCB$L_TT_BRDCST  00000084            UCB$V_LTYPE    = 00000000            

UCB$B_TRACKS     0000003D            UCB$L_TT_CTRLC   00000080            UCB$V_MOUNTING = 00000009            

UCB$B_TT_BRDPT   00000098            UCB$L_TT_CTRLY   0000007C            UCB$V_MSGACK   = 00000004            

UCB$B_TT_CRFILL  0000009D            UCB$L_TT_DECHAR  000000A8            UCB$V_MSGFLO   = 00000003            

UCB$B_TT_DECRF   000000A1            UCB$L_TT_MULTI   00000078            UCB$V_NOCNVRT  = 00000002            

UCB$B_TT_DELFF   000000A2            UCB$L_TT_RDUE    0000008C            UCB$V_NT_BFROVF= 00000002            

UCB$B_TT_DESPEE  000000A0            UCB$L_TT_STATE   00000074            UCB$V_NT_BREAK = 00000005            

UCB$B_TT_DETYPE  000000A4            UCB$L_TT_TYPAHD  00000088            UCB$V_NT_NAME  = 00000004            

UCB$B_TT_DIAL    00000096            UCB$L_VCB        00000030            UCB$V_ONLINE   = 00000004            

UCB$B_TT_ESC     00000095            UCB$M_BACKP    = 00000020            UCB$V_POWER    = 00000005            

UCB$B_TT_ESC_O   00000099            UCB$M_BSY      = 00000100            UCB$V_PRMMBX   = 00000000            

UCB$B_TT_FILL    00000097            UCB$M_CANCEL   = 00000008            UCB$V_SEGFLO   = 00000002            

UCB$B_TT_LFFILL  0000009E            UCB$M_DEADMO   = 00000400            UCB$V_TIM      = 00000000            

TTYDRVDAT       - TERMINAL DRIVER DATA BASE                      21-AUG-1978 21:01:39   VAX-11 MACRO X0.3-11               Page  12

SYMBOL TABLE                                                                                                                     (5)



UCB$V_TIMOUT   = 00000006            

UCB$V_TT_NOTIF = 00000002            

UCB$V_TT_ODD   = 00000007            

UCB$V_TT_PARTY = 00000006            

UCB$V_TT_SPEED = 00000000            

UCB$V_TT_TIMO  = 00000001            

UCB$V_UNLOAD   = 0000000C            

UCB$V_VALID    = 0000000B            

UCB$W_BCNT       0000006E            

UCB$W_BCR        00000096            

UCB$W_BOFF       0000006C            

UCB$W_BUFQUO     00000018            

UCB$W_BYTESTOGO  0000003E            

UCB$W_CHARGE     0000004A            

UCB$W_CYLINDERS  0000003E            

UCB$W_DA         0000008C            

UCB$W_DC         0000008E            

UCB$W_DEVBUFSIZ  0000003A            

UCB$W_DEVSTS     0000005A            

UCB$W_DIRSEQ     00000088            

UCB$W_DSTADDR    00000018            

UCB$W_DX_BCR     000000A4            

UCB$W_EC1        00000090            

UCB$W_EC2        00000092            

UCB$W_ERRCNT     00000072            

UCB$W_FUNC       0000007E            

UCB$W_MB_SEED    FFFFFFFC            

UCB$W_MSGCNT     00000016            

UCB$W_MSGMAX     00000014            

UCB$W_NT_CHAN    0000007C            

UCB$W_OFFSET     0000008A            

UCB$W_REFC       00000050            

UCB$W_SIZE       00000008            

UCB$W_SRCADDR    0000001A            

UCB$W_STS        00000058            

UCB$W_TT_CURSOR  0000009A            

UCB$W_TT_DESIZE  000000A5            

UCB$W_TT_HOLD    00000090            

UCB$W_TT_INAHD   00000092            

UCB$W_UNIT       00000048            

UCB$W_VPROT      0000001A            

XYCONTROL      = 00000006            

XYCTRL2        = 00000004            

XYSPEC         = 00000008            

Y              = 00000000            





PROGRAM SECTION SYNOPSIS



.  ABS  .        00000000      00     NOPIC   USR   CON   ABS   LCL NOSHR NOEXE NORD  NOWRT BYTE  

. BLANK .        00000000      01     NOPIC   USR   CON   REL   LCL NOSHR   EXE   RD    WRT BYTE  

$ABS$            FFFFFFFE      02     NOPIC   USR   CON   ABS   LCL NOSHR   EXE   RD    WRT BYTE  

$$$115_DRIVER    0000020B      03     NOPIC   USR   CON   REL   LCL NOSHR   EXE   RD    WRT LONG  





THERE WERE NO ERRORS OR WARNINGS.

9718. BYTES LEFT IN FREE MEMORY POOL.

TTYDRVDAT       - TERMINAL DRIVER DATA BASE                      21-AUG-1978 21:01:39   VAX-11 MACRO X0.3-11               Page  13

PROGRAM SECTION SYNOPSIS                                                                                                         (5)



3250. BYTES OF RECLAIMED MEMORY.

OBJ$:TTYDRVDAT,LIS$:TTYDRVDAT/-SP=EXECML$/ML,SRC$:TTYDRVDAT

9 MLB DIR RDS - 786 GETS TO DEFINE 17 MACROS. 108 INTER. FILE WRITES. 

