Product:  TOPDRAWER
Version:  5.12       ( SSC/Rice )
Document: PP0005.1
Author:   CLEMENT@RIPHYS
Guru:     KREYMER
Date:     8-JUL-1993
Support:  5 (full)

TOPDRAWER is a keyword-driven interface to the SLAC Unified Graphics
system, designed specifically to generate physics graphs with minimal
specifications.  Reasonable defaults are assumed for axis scales,
tic locations, label locations and size, etc.  

Topdrawer originated at the Stanford Linear Accelerator Center. The manual
for this modified version is online in TOPDRAWER_ROOT:[DOC]TOPDRAWER.DOC,
and via HELP, both at the VMS level and within the Topdrawer program.
The original SLAC document number is  CTGM 178.

Usage:    $ SETUP TOPDRAWER  ! Set up TD using its SETUP.COM procedure

          $ TD  filename  device   ! For noninteractive TD, default Tektronix
     or   $ TD                     ! For interactive TD

Many devices are supported, including the following common ones.
Hardcopy output file names match input file names, and have extensions
appropriate to the selected devices.

XWINDOW    remember to first SET DISPLAY/CREATE=node for remote windows

POSTSCR    supports color, has correct BoundingBox comment
           $ TD input "POSTSCR,ORI=3" ! For use with TeX/DVIPS

TEKTRONIX  with special modes CIT467,RADM3A,RVT100,RVT100A,SEL100XL,VIS102,
                              TAL1590,KERMIT,LSI7107,TEK4207,VT240

EXCL       for Talaris EXCL printers like the 1590

QMS1200    for Talaris and QMS printers like the 800 and 1200
