                   QLogic iSCSI Offload Driver

           Copyright (c) 2020 Marvell Semiconductor Inc.
                      All rights reserved.



Table of Contents

1. Change History
2. Known Issues
3. Notices
4. Contacting Support


1. Change History

Version 8.50.1.0a (Mar 13, 2020)
 * [CQXXXX]   : Updated OEM device ids and adapter friendly name
   Scope      : 45000/41000 Series Adapters	

Version 8.50.1.0 (Jan 15, 2020)
 * [CQXXXX]   : Updated copyright date information 
   Scope      : 45000/41000 Series Adapters	

Version 8.42.2.0 (Aug 26, 2019)
 * [CQ106397] : iSCSI Crash dump collection failed in Secure Boot enabled.
   Resolution : Renamed crash dump driver to qeiscdo.sys, and included it as part of the miniport driver bundle
   Scope      : 45000/41000 Series Adapter 

Version 8.42.1.0 (Aug 12, 2019)
 * [CQ106878] : CNA unable to create Multi-path with PowerPath while in iSCSI Offload mode.
   Resolution : Fixed residual flag parsing issue
   Scope      : 45000/41000 Series Adapter 

Version 8.40.6.0a (July 5, 2019)
 * [CQ106535] : Incorrect iSCSI device name present for Dell Tucson-D/Tucson-BTD adapters in Device manager.
   Resolution : Added ids for OEM adapter
   Scope      : 45000/41000 Series Adapter 

Version 8.40.6.0 (June 14, 2019)
 * [CQ103886] : Throughput is not higher with iSCSI offload in Win2016
   Resolution : Adjusted TCP and iSCSI parameters 
   Scope      : 45000/41000 Series Adapter 
 * [CQ105827] : Nimble DSM can't claim LUNs  
   Resolution : Modified handling of commands that complete with firmware reported underrun 
   Scope      : 45000/41000 Series Adapter 

Version 8.40.5.0a (June 14, 2019)
 * [CQ106188] : ISCSI INF not updated for Tuscon device
   Resolution : Added supported device ids
   Scope      : 45000/41000 Series Adapter 
 * [CQXXXXX]  : Added ids for OEM adapter 
   Scope      : 45000/41000 Series Adapter 

Version 8.40.5.0 (Mar 28, 2019)
 * [CQXXXXXX] : Update to the latest HSI
   Scope      : 45000/41000 Series Adapter 

Version 8.40.4.0 (Feb 6, 2019)
 * [CQXXXXXX] : Added checks for boot mode before consuming NVRAM data
   Scope      : 45000/41000 Series Adapter 
 * [CQ105017] : HLK: Verifier assertion while running BDE WLK Test
   Resolution : Fixed SQ buffer leaking issue
   Scope      : 45000/41000 Series Adapter 

Version 8.40.3.0 (Jan 17, 2019)
 * [CQ104701] : MS iSCSI Initiator target connection not re-established after perturbation
   Resolution : Modified handling of target connection recovery
   Scope      : 45000/41000 Series Adapters

 * [CQ104569] : ISCSI-AH: Not able to assign static IP to iSCSI initiator in Windows OS.
 * [CQ104621] : CN1300R iSCSI IPv4 portal unusable with Snap3 and Snap4 drivers/FW for WS2016
   Resolution : Changed the NVM BFS parameters valid checking
   Scope      : 45000/41000 Series Adapters
   
 * [CQ104635] : System fails to boot into OS using Secondary target params when Primary target IQN is blank.
   Resolution : Handle scenarios involving incorrect target parameters 
   Scope      : 45000/41000 Series Adapters
   

Version 8.40.2.0 (Dec 7, 2018)
 * [CQ104462] : Updated OEM id from .inf file 
   Scope      : 45000/41000 Series Adapters

 * [CQ102629] : Proton-8S won't boot with iSCSI Offload enabled 
   Resolution : Increased max supported processor number to 512
   Scope      : 45000/41000 Series Adapters

 * [CQ102918] : One time system crash seen while disable-enable vbd device with iSCSI driver installed 
 * [CQ102938] : DRIVER_IRQL_NOT_LESS_OR_EQUAL (d1) BSOD with load unload driver
   Resolution : Wait for bus driver interface to be fully operational before handling asynchronous events.
                Added functionality to notify bus driver once iSCSI driver's initialization is complete.
   Scope      : 45000/41000 Series Adapters

 * [CQ102128] : Unable to find disk drives during OS installation 
   Resolution : Updated handling of CHAP configuration
   Scope      : 45000/41000 Series Adapters

 * [CQ103163] : Second iSCSI path does not recover with enablement of downlink port after server reboot 
 * [CQ103128] : HWiSCSI failed path is not restored in Win2016 after the path is reconnected
   Resolution : Modified driver handling of target that is unavailable during boot.
   Scope      : 45000/41000 Series Adapters

 * [CQXXXXX]  : Add support for OEM adapter in Windows driver
   Resolution : Added OEM device ids
   Scope      : 45000/41000 Series Adapters

 * [CQ103140] : Fatal error during hibernate
   Resolution : Modified iSNS code to handle hibernate code flow
   Scope	  : 45000/41000 Series Adapters

 * [CQ102992] : Mismatch of Adapter name in OS level in Device manager
   Resolution : Corrected Adapter name
   Scope	  : 45000/41000 Series Adapters

 * [CQ101872] : qeois driver asserted when changing the lun on the target and adapter interfaces
   Resolution : Addressed the handling of incorrect target name
   Scope	  : 45000/41000 Series Adapters

 * [CQXXXXXX] : Added changes for being compatible with Universal driver requirements
   Scope	  : 45000/41000 Series Adapters

 * [CQ102557] : System crash while running traffic with iSNS configured
   Resolution : Addressed the incorrect ramrod sent down to fw
   Scope	  : 45000/41000 Series Adapters

 * [CQXXXXXX] : Added SmartSAN support
   Scope	  : 45000/41000 Series Adapters

 * [CQXXXXXX] : Added support for /Qspectre compiler option 
   Scope      : 45000/41000 Series Adapters	
 * [CQXXXXXX] : Optimized SGL handling when forwarding to I/O requests to firmware.
   Scope	  : 45000/41000 Series Adapters

Version 8.40.1.0 (May 18, 2018)
 * [CQXXXXXX] : Updated for HSI changes to support 8.40.x.x HSI
   Scope	  : 45000/41000 Series Adapters

Version 8.37.2.0 (Apr 03, 2018)
 * [CQ100100] : System crash while running multiprotocol data integrity traffic overnight
   Resolution : Fixed IO timeout handing issue
   Scope	  : 45000/41000 Series Adapters

 * [CQ99539]  : HP 12.30:Quack: Windows: iSCSI device shows incorrect link speed
   Resolution : Addressed the issue with adding support for the speed value coming from evbd
   Scope	  : 45000/41000 Series Adapters

 * [CQXXXXX]  : Added support for firmware debug flag via registry
   Scope      : 45000/41000 Series Adapters
   
Version 8.37.1.0 (Feb 09, 2018)
 * [CQXXXXX]  : Added ids for OEM adapter 
   Scope      : 45000/41000 Series Adapters

Version 8.33.2.0 (Jan 29, 2018)
 * [CQ99204]  : Observed stop code 0x7B during iSCSI BFS reboot test 
   Resolution : Addressed the issue with incorrect login parameters being used due to uninitialized memory
   Scope      : 45000/41000 Series Adapters

Version 8.33.1.0 (Jan 23, 2018)
 * [CQ99015]  : Storage functions (iSCSI + FCoE) showing incorrect Inf names in DM
   Resolution : Added device ids
   Scope      : 45000/41000 Series Adapters
 * [CQXXXXX]  : Added ids for OEM adapter
   Scope      : 45000/41000 Series Adapters
 * [CQXXXXX]  : Updated Copyright string
   Scope      : 45000/41000 Series Adapters

Version 8.30.10.0 (Nov 14, 2017)
 * [CQXXXXX]  : Update link speed parameters for SmartSAN
   Scope      : 45000/41000 Series Adapters

 * [CQ97873]  : Unable to get iSCSI DHCP on Port 1
   Resolution : Added NVM BFS parameters validation
   Scope      : 45000/41000 Series Adapters

Version 8.30.9.0 (Oct 17, 2017)
 * [CQ97528]  : SUT freezes for 80 seconds and resumes with one of MPIO switch port shut
   Resolution : Updated the port down detection logic
   Scope      : 45000/41000 Series Adapters

 * [CQ97074]  : System assert while running multiprotocol traffic
 * [CQ97374]  : Assertion while running read I/O and Qeois driver is on stack
   Resolution : Fixed a synchronization issue
   Scope      : 45000/41000 Series Adapters

Version 8.30.8.0 (Sep 29, 2017)
 * [CQXXXXX]  : Update OCBB Statistics
   Scope      : 45000/41000 Series Adapters

Version 8.30.7.0 (Sep 19, 2017)
 * [CQXXXXX]  : Link error stats support in smart SAN
   Resolution : Add Link error stats support in smart SAN
   Scope      : 45000/41000 Series Adapters

Version 8.30.6.0 (Sep 12, 2017)
 * [CQ96320]  : Driver installer hangs in channel2017E to Channel2017U1E upgrade scenario
   Resolution : Modified flow for handling PnP StopDevice
   Scope      : 45000/41000 Series Adapters

Version 8.30.5.0 (Aug 31, 2017)
 * [CQXXXXX]  : Add SmartSAN support
   Resolution : Added SmartSAN support
   Scope      : 45000/41000 Series Adapters

 * [CQ96387]  : Missing device ids for OEM adapter
   Resolution : Add ids for OEM adapter
   Scope      : 45000/41000 Series Adapters

Version 8.30.4.0a (Aug 21, 2017)
 * [CQXXXXX]  : Add support for OEM adapter in Windows driver
   Resolution : Added OEM device ids
   Scope      : 45000/41000 Series Adapters

Version 8.30.4.0 (Aug 07, 2017)
 * [CQXXXXX]  : Added OCBB support
   Scope      : 45000/41000 Series Adapters

Version 8.30.3.0 (Jul 27, 2017)
 * [CQ95253]  : iSCSI LUN is not showing after loading driver for Windows 2016
   Resolution : Synced with fw RQ HSI change
   Scope      : 45000/41000 Series Adapters

 * [CQXXXXX]  : Added Property Sheet Change for SCSI Bus and SCSI Target number
              : Added support for I/O timeout handling
   Scope      : 45000/41000 Series Adapters 

 * [CQXXXXX]  : Updated OEM adapter ids 
   Scope      : 45000/41000 Series Adapters

Version 8.30.2.0 (Jul 05, 2017)
 * [CQ94912]  : iSCSI L4 BFS fails even though VLAN mode is disabled with VLAN ID set
   Resolution : Corrected the way to access NVM VLAN field
   Scope      : 45000/41000 Series Adapters

Version 8.30.1.0 (May 11, 2017)
 * [CQXXXXX]  : Add support for OEM adapter in Windows driver
   Resolution : HSI sync with firmware 8.30.4.0 (qevbda v8.30.1.0)
   Scope      : 45000/41000 Series Adapters

Version 8.20.1.0 (May 11, 2017)
 * [CQ93596]  : Inconsistent storage device (FCoE/iSCSI) friendlyname
   Resolution : Modified the inf to reflect new friendly names for OEM adapters
   Scope      : 45000/41000 Series Adapters

 * [CQXXXXX]  : Added driver trace buffer support
   Resolution : Add Link Status in property menu
   Scope      : 45000/41000 Series Adapters

Version 8.18.7.0 (Apr 05, 2017)
 * [CQ92984]  : System crash observed with port1 and 2 configured for L4 boot
   Resolution : Fixed a memory overwrite issue when both ports are enabled for boot 
   Scope      : 45000/41000 Series Adapters

Version 8.18.6.0 (Mar 29, 2017)
 * [CQ92839]  : iSCSI session device points to one of Equallogic array NIC member port IP addresses
   Resolution : Provide group IP address for target portal group as part of handling MSiSCSI_InitiatorSessionInfo WMI class 
   Scope      : 45000/41000 Series Adapters

 * [CQ92796]  : QEOIS Incorrect Device Naming String
   Resolution : Corrected 4-part id in the INF file
   Scope      : 41000 Series Adapters

Version 8.18.5.0 (Mar 15, 2017)
 * [CQ92210]  : iSCSI L4 Win2016 BFS crashes when Port1/Port2 are configured with same IQN/Target
   Resolution : Assign unique ID for each boot target when booting across multiple ports 
   Scope      : 45000/41000 Series Adapters

Version 8.18.4.0 (Feb 24, 2017)
   CQXXXXX	 : Handle cancelling work item threads when moving to D3 state
   Scope    : 45000/41000 Series Adapters

Version 8.18.3.0 (Feb 06, 2017)
*  Fixed a bug that may pass a incorrect device number to crash dump driver
   Scope     : 45000 Series Adapters      

Version 8.18.2.0 (Jan 11, 2017)
* [CQ90085]  : iSCSI BFS LUN Detection Failure when we load driver with SCHAP,MCHAP Enabled
   Scope     : 45000 Series Adapters      

Version 8.18.1.0 (January 3, 2017)
 * Added Hibernate support
 * Added crash dump driver support

Version 8.18.0.0 (November 22, 2016)
 * [CQ89939] : Windows:System breaks @ qeois!PeriodicWorkitem+1618 while passing iscsi traffic
   Resolution: Fixed a synchronization issue between cleanup and command submission paths can lead to pending I/Os while destroying connection, causing the assert

 * [CQ90085] : iSCSI BFS LUN Detection Failure when we load driver with SCHAP,MCHAP Enabled
   Resolution: Fixed a CHAP ID size issue 

Version 8.14.4.0 (October 20, 2016)
 * [CQ89340] : L4 iSCSI IPv4 BFS failure when we load QEOIS
   [CQ89341] : BSOD after iSCSI boot configuration parameters changes from HII option
   Resolution: Added handling of incomplete/incorrect boot parameters in NVRAM
			 : Fixed target id mapping for more than one boot target
 * Added new IDs in INF file
   Scope     : 8500 Series Adapters

Version 8.14.3.0 (September 26, 2016)
 * [CQ88827] : Fail to login target disk while installing Win2012R2 using iSCSI IPv6 L4
   Resolution: Supported stateful address configuration (without depending on RA alone)
   Scope     : 8500 Series Adapters

Version 8.14.2.0 (August 16, 2016)
 * HSI sync with firmware 8.14.3.0 (qevbda v8.14.1.0)
 * Updated to Windows10 WDK toolset
 * Included "opt-in" feature for NonPagedPoolNx pool type

Version 8.14.1.0 (August 05, 2016)
 * Boot from SAN using NVRAM support added
   Resolution: Remove iBFT reference and add NVRAM boot support
   Scope     : 8500 Series Adapters

Version 8.14.0.0 (August 01, 2016)
 * HSI sync with firmware 8.14.1.0 (qevbda v8.14.0.0)
 * [CQ87483] : System crash while running iSCSI traffic on 100 LUN's
   Resolution: fixed a multi processors sync issue in miniport driver
   Scope     : 8500 Series Adapters

Version 8.10.7.0 (July 07, 2016)
 * HSI sync with firmware 8.10.8.0 (qevbda v8.10.13.0)

Version 8.10.6.0 (June 16, 2016)
 * [CQ86894] : System crash while adding 512 targets from sanblaze
   Resolution: Increased the session ID mask from 9 bits to 11 bits
   Scope     : 8500 Series Adapters
 * HSI sync with firmware 8.10.7.0 (qevbda v8.10.9.0)
 * Added AH IDs

Version 8.10.5.0 (May 26, 2016)
 * [CQ86695] : WS2016 doesn't show Advanced tab for iSCSI interface
   Resolution: rebuilt the dll with correct toolset
   Scope     : 8500 Series Adapters
 * HSI sync with firmware 8.10.5.0 (qevbda v8.10.6.0)

Version 8.10.4.0 (May 10, 2016)
 * HSI sync with firmware 8.10.4.0 (qevbda v8.10.5.0)

Version 8.10.3.0 (April 18, 2016)
 * [CQ86206] : System crash after installing iSCSI driver – one time
 * [CQ86222] : System crash after shut no-shut on switch ports
 * [CQ86223] : System crash during system reboot when all protocols driver loaded
   Resolution: added a fix for LL2 local buffer double free issue
   Scope     : 8500 Series Adapters

Version 8.10.2.0 (April 12, 2016)
 * [CQ85442] : E4-iSCSI: WS2016-E4-40G- System Crash while installing iSCSI Driver
   Resolution: work with matching bus driver (qevbda 8.10.3.0)
   Scope     : 8500 Series Adapters

 * [CQ85165] : Assertion while shutdown the system after running iscsi, roce and l2 traffic test
   Resolution: Fixed the buffer leak in LL2 rx path
   Scope     : 8500 Series Adapters

 * HSI sync with firmware 8.10.3.0 (qevbda v8.10.3.0)
 * Added BDQ-RQ support
 * Fixes added for WS2016 build

Version 8.10.1.0 (February 29, 2016)
 * [CQ85064] : E4-iSCSI: iSCSI driver doesn't install on 4X25G adapter
   Resolution: added support QLogic 4X25G iSCSI Adapter device
   Scope     : 8500 Series Adapters
 * HSI sync with firmware 8.10.1.0 (qevbda v8.10.1.0)
 * added device error recovery support

Version 8.7.4.0a (February 18, 2016)
 * added another QLogic 25 Gigabit iSCSI Adapter device

Version 8.7.4.0 (February 11, 2016)
 * added support QLogic 25 Gigabit iSCSI Adapter

Version 8.7.3.0 (January 14, 2016)

 * HSI sync with firmware 8.7.5.0 (qevbda v8.7.10.0)
 * Added ncsi supporting
 * removed extended resources set supporting

Version 8.7.2.0 (January 5, 2016)

 * HSI sync with firmware 8.7.5.0 (qevbda v8.7.10.0)
 * supporting extended resources set

Version 8.7.1.0 (December 16, 2015)

 * HSI sync with firmware 8.7.4.0
 * Changed BD build logic
 * [CQ83950] : E4-iSCSI: System crash during disable enable iscsi driver with verifier on
   Resolution: decrease connection reference number in unsolicited CQE processing
   Scope     : 8500 Series Adapters

Version 8.7.0.0 (November 10, 2015)

 * HSI sync with firmware 8.7.0.0
 * clear R and W bits when expect data length is 0

Version 8.6.0.0 (October 15, 2015)

 * HSI sync with firmware 8.6.0.0
 * defaultCq set for connection group

Version 8.5.3.0 (September 02, 2015)

 * [CQ81141] : E4-iSCSI: system crash while uninstalling iscsi driver
   Resolution: Hold to produce new events when waiting Ramrod be completed
   Scope     : 8500 Series Adapters

 * [CQ81476] : E4-iSCSI: assertion seen during system reboot when iSCSI targets are mapped
   Resolution: Hold to produce new events when waiting Ramrod be completed
   Scope     : 8500 Series Adapters

 * [CQ81889] : E4-iSCSI: Assertion during MCS click
   Resolution: Fixed in wmi LBpolicy
   Scope     : 8500 Series Adapters

Version 8.5.2.0 (August 25, 2015)

 * [CQ81141] : E4-iSCSI: system crash while uninstalling iscsi driver
   Resolution: Fixed in connection closing flow
   Scope     : 8500 Series Adapters

 * [CQ81440] : E4-iSCSI: system crash while running performance traffic for iSCSI
   Resolution: Fixed in connection closing flow
   Scope     : 8500 Series Adapters

 * [CQ81476] : E4-iSCSI: assertion seen during system reboot when iSCSI targets are mapped
   Resolution: Fixed in connection closing flow
   Scope     : 8500 Series Adapters

Version 8.5.1.0 (July 17, 2015)

 * changed values of srtt and rtt_var

Version 8.5.0.0 (July 07, 2015)

 * HSI sync with firmware 8.5.0.0

Version 8.4.1.0 (July 01, 2015)

 * code cleanup

Version 8.4.0.0 (June 29, 2015)

 * [CQ80267] : E4 ISCSI: "No response for NOP-OUT" result in assertion since the target doesn't response with NOP-IN
   Resolution: Adjust TCP parameters cwnd and ssthresh
   Scope     : 8500 Series Adapters

 * Increase QR to 8 pages
 * HSI sync with firmware 8.4.2.0
 * driver name field for NC-SI feature 

Version 8.3.3.0 (June 9, 2015)

 * [CQ79575] : E4-iSCSI: Observed assertion on QEOIS while running medusa traffic to iSCSI LUN over SMB share
   Resolution: Fixed BD list build logic
   Scope     : 8500 Series Adapters

 * [CQ79680] : Assertion while running RoCE traffic on iSCSI luns
   Resolution: Fixed BD list build logic
   Scope     : 8500 Series Adapters

Version 8.3.2.0 (May 19, 2015)

 * [CQ79672] : E4 ISCSI:Disconnect the target from Microsoft Initiator results in assertion
   Resolution: Fixed IO pending check flow
   Scope     : 8500 Series Adapters

 * [CQ79728] : E4-iSCSI: Observed assertion on QEOIS while running medusa traffic to iSCSI LUN over SMB share
   Resolution: Fixed IO pending check flow
   Scope     : 8500 Series Adapters

Version 8.3.1.0 (April 23, 2015)
 * Added TxDrain
 * HSI sync with firmware 8.3.6.0
 
Version 8.3.0.0 (April 13, 2015)
 * Sample 4 Base
 * HSI sync with firmware 8.3.4.0
 
Version 8.2.7.0 (March 31, 2015)
 * CQ 78868 Add device to inf files

Version 8.2.6.0 (March 12, 2015)
 * Support NOP-OUT Reply

Version 8.2.5.0 (March 11, 2015)
 * Set ISCSI_WQE_PTU_INVALIDATE for a scsi command with a itt reuse count wrapped by 12 bits.
 * Set the tcp send window, tcp window and congestion window from right edge to absolute value for connection upload.

Version 8.2.4.0 (March 3, 2015)
 * HSI sync with firmware 8.2.9.0
 * Set ISCSI_WQE_PTU_INVALIDATE for a scsi command with a itt reuse count wrapped by 16 bits
Version 8.2.3.0 (February 27, 2015) Special version ONLY works with 8.2.6.25 !ONLY!

 * HSI sync with firmware 8.2.6.21
 * CQ 78109 - E4 ISCSI connecting to target with Data Digest during discovery failed.
 * Set the tcp send window, tcp window and congestion window from right edge to absolute value for connection offload.
 
Version 8.2.2.2 (February 23, 2015)

 * Fixed CQ78109

Version 8.2.1.0 (February 17, 2015)

 * HSI re-sync with firmware 8.2.4.0
 * Added clear SQ command
 * Fixed CQ78089
 
Version 8.2.0.0 (February 11, 2015)

 * HSI sync with firmware 8.2.4.0
 * Fixed Cont00076145 "No Persistent Target"
 
Version 8.0.2.0 (January 30, 2015)

 * HSI sync with firmware 8.2.2.0

Version 8.0.1.0 (January 6, 2015)

 * HSI sync with firmware 8.1.8.0

Version 8.0.0.7 (December 2, 2014)

 * HSI sync with firmware 8.1.3.0

 * Fixed some Recovery issues

Version 8.0.0.6 (November 12, 2014)

 * [CQ76119] : E4:Brussels: initiator traffic stopped for 2M writing test
   Resolution: Fixed
   Scope     : 8500 Series Adapters

 * HSI sync with firmware 8.1.3.0

 * Added CleanUp logic before Recovery

Version 8.0.0.5 (October 01, 2014)

 * Version number update

Version 8.0.0.4c (September 30, 2014)

 * [CQ75897] : E4:Brussels: Iscsi device gets yellow bang on Win12R2 and Win2k8sp2
   Resolution: Added QLogic vendor id
   Scope     : 8500 Series Adapters

 * HSI sync with firmware 8.0.2.0

Version 8.0.0.4b (September 17, 2014)

 * added QLogic 57980S device IDs


Version 8.0.0.4a (September 10, 2014)

 * added QLogic 57940S device IDs


Version 8.0.0.4 (September 05, 2014)

 * HSI sync with firmware 8.0.0.7

Version 8.0.0.3 (August 18, 2014)

 * Task Management Support


Version 8.0.0.2 (August 6, 2014)

 * new HSI sync up


Version 8.0.0.1 (July 23, 2014)

 Initial Release.

2. Known Issues 

 *           : Get assert when running I/O meter LUN queue depth set to 128
 *           : Get assert when running I/O meter with block size 2M 

3. Notices

Information furnished in this document is believed to be accurate and
reliable. However, QLogic Corporation assumes no responsibility for
its use, nor for any infringements of patents or other rights of
third parties which may result from its use. QLogic Corporation
reserves the right to change product specifications at any time
without notice. Applications described in this document for any of
these products are only for illustrative purposes. QLogic Corporation
makes no representation nor warranty that such applications are
suitable for the specified use without further testing or
modification. QLogic Corporation assumes no responsibility for any
errors that may appear in this document.


4. Contacting Support

   For further assistance, contact QLogic Technical Support at:
   http://support.qlogic.com


(c) Copyright 2015. All rights reserved worldwide. QLogic and the 
QLogic logo are registered trademarks of QLogic Corporation. 
All other brand and product names are trademarks or registered
trademarks of their respective owners.

- Initial Release.
