                  ============================
                   R E L E A S E    N O T E S
                  ============================

				QLogic iSCSI Crash-dump Driver

              Copyright (c) 2019 Cavium, Inc.
                      All rights reserved.



1. Change History

Version 8.42.1.0 (Aug 15, 2019)
    CQ106397    : iSCSI Crash dump collection failed in Secure Boot enabled
    Resolution  : Renamed driver to qeiscdo.sys, and included as part of the miniport driver bundle
	Scope		: 45000/41000 Series Adapters

Version 8.38.1.0 (Feb 7, 2019)
	CQ105033	: Crash dump not generated with BSOD
	Resolution	: Set driver state as ACTIVE with MFW
	Scope		: 45000/41000 Series Adapters

Version 8.30.6.0 (October 8, 2018)
	CQ103872	: E3/E4 Driver Installer not updating Crash Dump (iSCSI/FCoE) driver from inbox to out of box on Fresh installed WS_2019 OS
	Resolution	: Update driver version to allow installer to update drivers
	Scope		: 45000/41000 Series Adapters

Version 8.30.5.0 (March 19, 2018)
	CQ100380	: iSCSI Crash Dump does not generate dump in OEM MF mode
	Resolution	: Fixed incorrect handling of check condition, request sense and NOP-OUT request 
	Scope		: 45000/41000 Series Adapters

Version 8.30.4.0 (December 8, 2017)
	CQ97784		: iSCSI crash dump driver taking long time to collect crashed dump on iSCSI BFS system
	Resolution	: Fine tuned layer 2 transmit path to reduce overheads  
	Scope		: 45000/41000 Series Adapters

Version 8.30.3.0 (October 3, 2017)
	CQ97029		: Crashdump driver fails to generate memory dump
	Resolution	: Fixed incorrect LUN field setting for iSCSI PDU  
	Scope		: 45000/41000 Series Adapters

Version 8.30.2.0 (September 15, 2017)
	CQ95802		: Memory dump created with PARTIALLY CORRUPT during iSCSI crash dump test
	Resolution	: Fixed incorrect handling of multiple iSCSI PDUs in a single TCP segment
	Scope		: 45000/41000 Series Adapters

Version 8.30.1.0 (August 31, 2017)
	CQ95802		: Memory dump created with PARTIALLY CORRUPT during iSCSI crash dump test
	Resolution	: Fixed incorrect handling of multiple R2T and NOP_IN request from target for a write command
	Scope		: 45000/41000 Series Adapters
	
Version 8.18.3.0 (March 6, 2017)
	Changes : Added support for L2 crash-dump functionality
	Scope   : 45000/41000 Series Adapters
	
Version 8.18.2.0 (Feb 21, 2017)
   CQ91769 : Crashdump driver fails to generate memory dump
   Resolution : Fixed the incorrect receive filter definitions 
   Scope      : 45000/41000 Series Adapters		  

Version 8.18.1.0 (Feb 07, 2017)
 * Initial Release
   Scope      : 45000 Series Adapters		  