UCHHJRZ0162> ?

160621-18:31:06 169.254.1.1 16.0a RBS_NODE_MODEL_U_4_95 stopfile=/tmp/7880
$ ?
Command         Description
                default shell command
.               execute commands from file
?               print description of commands
EtHostMo_getPmCounters Get PM counters for a specified host
EtHostMo_startPing
GtpShDump       Command syntax:
GtpShPrintProc  Command syntax:
Ippmlh          Umbrella function for internal COLI commands
IppsrhInfo                 The IppsrhInfo command has several subcommands;
MacHsTest_2     Warning: Only for internal development use. Do not abuse. Command has severe impact on subscriber traffic execution.
PmrColi         Umbrella function for internal COLI commands
UdpShDump       Command syntax:
UdpShPrintProc  Command syntax:
aaconfig        Sets TTL timeout for DNS lookups
aal2ap          Prints AAL2 AP program data.
aal2cpsrc       Prints AAL2 CPS RC program data
aal2ncc         Prints AAL2 NCC program data
aal2nccadm      Prints AAL2 NCC ADM program data
aal5apterm      Prints static connection data of AAL5 AP TERM
aal5debug       Collects and prints out AAL5 CBM data
aal5eph         Prints out AAL5 EP Handler data
aal5etterm      Print static connection data in AAL5 ET TERM
aatest          Diagnostics for AA server(s), -h for more help
acpapi          ACP34DR ACP34API status and control
acparp          ACP34DR ARP status and control
acpbasicbh      ACP34 Basic BH status and control
acpbasiccmn     ACP34BASIC CMN status and control
acpbasicproc    ACP34 Basic PROC status and control
acpbh           ACP34DR BH status and control
acpcmn          ACP34DR CMN status and control
acpdscp         ACP34DR DSCP
acpflc          ACP34DR FLC status and control
acpfpc          ACP34DR FPC
acpfsm          ACP34DR FSM status and control
acpiac          ACP34DR IAC
acpicmp         ACP34DR ICMP status and control
acpix           ACP34BASIC IX
acplaid         ACP34DR LAID
acplh           ACP34DR LH status and control
acppath         ACP34DR PATH
acppd           ACP34DR PD
acpph           ACP34DR PH status and control
acppol          ACP34DR POL Policies and counters
acpsa           ACP34DR SA and counters
acpsh           ACP34DR SH status and control
acpsync         ACP34DR SYNC status and control
acptm           ACP34DR TM status and counters
aet_aal2bp      Status info for the AET AAL2 BP program
aet_aal2mp      Status info for the AET AAL2 MP program
aet_atmbp       status info for AET ATM BP program
aet_atmmp       status info for AET ATM MP program
aet_imabp       Provides object status information for the AET IMA BP program
aet_imamp       Provides object status information for the AET IMA MP program
aetlss          Lists service registrations in the LSS
arm             print LLP armament info
arp             Display ARP cache entries
arplist         Display ARP table entries
atfConnect      Connect an AU via ATFI
autodds         Set error check level and/or default trace
banner
bbRdbtMeas_3    Starts or stops RDBT measurements
bbRdbtMeas_4    Starts or stops RDBT measurements
bbRdbtMeas_5    Starts or stops RDBT measurements
bbRdbtMeas_6    Starts or stops RDBT measurements
bbRdbtMeas_7    Starts or stops RDBT measurements
bbRdbtMeas_8    Starts or stops RDBT measurements
bbRdbtTrace_2   Starts or stops RDBT tracing
bbRdbtTrace_3   Starts or stops RDBT tracing
bbRdbtTrace_4   Starts or stops RDBT tracing
bbRdbtTrace_5   Starts or stops RDBT tracing
bbRdbtTrace_6   Starts or stops RDBT tracing
bbRdbtTrace_7   Starts or stops RDBT tracing
bbRdbtTrace_8   Starts or stops RDBT tracing
bcm             Accessing and setup the internal ethernet switch
bh              CommandName:
biosls          List installed bios modules
bl              list blocks
bmlmdata        List loaded modules data
bmpgmconfig     Management of Board Manager configuration
bmrdump
boardtemp       Read and display values from all configured board temp sensors.
bootmgr         bootmgr command
bs              Execute a number of commands and print result
buffel          Display buffel configuration and usage
bvlq            Get value from BVL. BVL_AREA default name if no area-name
bvlquery        Get value from BVL. BVL_AREA default name if no area-name
capi
cat             copy files to stdout
cd              change the working directory
cease           cease ...
cedchTraceRx_3  Activate tracing for all CEDCH users in the UE selective framework
cedchTraceRx_4  Activate tracing for all CEDCH users in the UE selective framework
cedchTraceRx_5  Activate tracing for all CEDCH users in the UE selective framework
cedchTraceRx_6  Activate tracing for all CEDCH users in the UE selective framework
cedchTraceRx_7  Activate tracing for all CEDCH users in the UE selective framework
cedchTraceRx_8  Activate tracing for all CEDCH users in the UE selective framework
chcmeasfwtrace  Selective Tracing for measurements in ChcMeasFwBlu
chkdsk          Request a checkdisk on given volume
chmod           change access mode of files
cls             clear screen (using ANSI codes)
connfss         This command has been disabled
coremgr         coremgr command
cp              copy files. If multiple names are given, the last name must be a directory. Option -R means recursive. Option --bufsize sets the size of the internal heap buffer to be used.
cpridump        Dumps CPRI related info
crashec         kill EC process(only for SVO test)
crashncc        Kill a NCC program Instance.
crashscc        kill SCC process(only for SVO test)
createObj       Creates an object.
csti            CSTI SERVER TOPOLOGY INFORMATION
cv              Configuration version command
dbvl
dda             Send DDA command
deleteObj       Delete an object.
devinfo         Display real and virtual device info
dhcctl          DHCP client and wrapper control and debug
dhcpclientrh    DHCPRH SWB debug
dhcpinfo        DHCP client internal state transition history and message counter info
dicm            dicm commands
dicminfo        Prints event history and internal structures in DICM
dig             DNS lookup utility
disableBPAIrestart_1 Disables the Restart Board Procedure (No dumps,no stopping of DPs and no board restart)
disableBPAIrestart_2 Disables the Restart Board Procedure (No dumps,no stopping of DPs and no board restart)
disableBPAIrestart_3 Disables the Restart Board Procedure (No dumps,no stopping of DPs and no board restart)
disableBPAIrestart_4 Disables the Restart Board Procedure (No dumps,no stopping of DPs and no board restart)
disableBPAIrestart_5 Disables the Restart Board Procedure (No dumps,no stopping of DPs and no board restart)
disableBPAIrestart_6 Disables the Restart Board Procedure (No dumps,no stopping of DPs and no board restart)
disableBPAIrestart_7 Disables the Restart Board Procedure (No dumps,no stopping of DPs and no board restart)
disableBPAIrestart_8 Disables the Restart Board Procedure (No dumps,no stopping of DPs and no board restart)
disableCBCIrestart_1 Disables the Restart Board Procedure (Dump, stop and no board restart)
disableCBCIrestart_2 Disables the Restart Board Procedure (Dump, stop and no board restart)
disableCBCIrestart_3 Disables the Restart Board Procedure (Dump, stop and no board restart)
disableCBCIrestart_4 Disables the Restart Board Procedure (Dump, stop and no board restart)
disableCBCIrestart_5 Disables the Restart Board Procedure (Dump, stop and no board restart)
disableCBCIrestart_6 Disables the Restart Board Procedure (Dump, stop and no board restart)
disableCBCIrestart_7 Disables the Restart Board Procedure (Dump, stop and no board restart)
disableCBCIrestart_8 Disables the Restart Board Procedure (Dump, stop and no board restart)
diskcredit      Disk credit command
dnsresolver3pp  display internal debug information
dnsresolverfh   DNSRESOLVERFH SWB debug
dnsrinfo        display DNS resolver information or reset counters
domlist         list all regions in one/all domain(s), optionally showing used physical memory fragments.
dpSetMemDumpAreas Set user memory area to be dumped for <snid>
dpcmd_1         Executes a list of commands
dpcmd_2         Executes a list of commands
dpcmd_3         Executes a list of commands
dpcmd_4         Executes a list of commands
dpcmd_5         Executes a list of commands
dpcmd_6         Executes a list of commands
dpcmd_7         Executes a list of commands
dpcmd_8         Executes a list of commands
drl             Read DSP ramlog
dscpgfh         DSCPGFH SWB debug
dscpgrh         DSCPGROUPRH SWB RO information
dspMemChange    Write DSP Memory
dspMemDump      Read DSP Memory
dsp_nmi         trigger NMI for DSP with given snid number
dspload         Load is presented as: mean [min, max], ...
dspmem          Memory is presented as: Pool1, Pool2, ...
dspstat         This command prints statistics counters and states from the DSP.
dsvl
duilFaultInject Injects a fault to SRIO-I BC
duilOpenTestPort Activates SRIO test ports
dump            Print a post mortem dump.See dump -h for more options.
dumpcap         dumps OAM IP-communication in pcap format on file
dumpecncr       Dumping EcNcrNodeConfigurationRepository(NCR) component residing at MPSW-EQC level
dumpelg         Prints HW log entries.
ecdevjsinfo     Dumping EcDevDeviceResMgrC(DEV) component residing at MPSW-EQC level
echo            echo arguments (-n no newline)
ecodes          List the entries in the error code log.
efcdump         filter = anp|gdl|gul|oil|rfc|sub|txm|all
efhreset        resetLeakyBucket component residing at MPSW-EQC level
erasehwlog      Erase HW log entries.
errinfo         List the entries in the error info area.
errno           print description of errno number
errorlist       Print all registrered error codes.
etcmd           Type etcmd help for detailed help.
ethadapter      Get registered clients and statistics for Ethernet Adapter Device.
ethernet        ethernet shell command
ethmode         Ethernet speed/duplex control cmd's
ethoamfh        ETHOAMFH SWB FRO information
ethoamrh        ETHOAMRH SWB RO information
eulmc           Enable or disable activation of secondary carrier for eulmc
exit            exit the current shell
fault           fault ...
faultdump       Dumps all configured faults.
faultind        Enables/disables sending of CPRI High Bit error rate Fault indications.
flash           Provides commands to manipulate the data in the flash.
flashstat       Flash statistics
forever         execute command forever
format          This command has been disabled
formathd        Format the Hard Disk
fpm             Interface to Flash Partition Manager
freerunning     Force regulator to enter freerunning state. No synchronization reference should be selected when this command is used.
fssls           list fss objects
fullDumpMode    creat DUWv2 dumps for all DPs or not
gdbtp           Command for handling trace point experiment
genann          Modify received Announce messages
gengpssstatus   Change GpssStatus received in GPppr message
genhptsisource  Change Hptsi clock source
genpdv          Introduce pdv to current packet reference
gentimestandard Change time standard received in GPtps message
genwander       Introduce wander to current frequency
getAttrObj      Get attributes for an object.
getDiskDataObj  Get attributes for disk for an object.
getProcessorLoad Get processor load for a PIU.
getpri          This command has been disabled
gps01reset      Reset GPS01 receiver and clear positioning data
gps02reset      Command used to clear and/or reset GPS02 receiver
gpscapture      Capture NMEA messages to and from GPS receivers
gpsprot         Change protocol between Furuno and Ericsson Combined
gpsreset        initiate reset of GRU or GRM FW on GPS receiver
gpssend         Send message to the GPS receiver
gpsstatus       Print the status of GPS receiver
gulm_reset      Assert reset for GULM with given snid number
gz              Compress/decompress file(s)
hdinfo          Hard disk parameter information
hdpartition     checks or harmonizes the disk partitions as per table
hdreadtest      Hard disk read test of HD
hdstat          Hard disk statistics printout
heapinfo        Heap information (for proc/seg)
help            print description of commands
hili            Hardware Inventory Log Handling commands
hooks           Print all registered error, dump and reset hooks.
hostname        show or set hostname
hwdi            Display HW distribution for the processor.
hwpid           Read hardware pid from specified target
iacrh           IACRH debug and utilities
idl2dump        Dumps related info on all IDL2 links.
idl2test        Start idl2 cpri link.
idux            IDUX_DRV
iexsCt          Usage:
iexsrm          Displays IEXS resource manager specific info.
ifconfig        Print IP address
ifmcstat        Dump multicast group management statistics per interface
iked            IKE debug commands
ikepeerfh       IKEPEERFH SWB debug
ikerh           IKERH SWB debug
ikev2           IKEv2 debug commands
inopcnt         Read or clear counter for inop on a given port nr.
inrsidump       Dump INRSI related information.
ipac_blockHostRegi Command for blocking of IPHOSTREGI
ipac_blockSyncRegi Command for blocking of IPSYNCREGI
ipac_ipadm      Status info for the IPAC IP Adm administrator program
ipac_ipsyncref  Status info for the IPAC IP Sync Ref administrator program
ipcp_bh         Status info for the IPCP board handler administrator program
ipcp_dh         Status info for the distribution handler administrator program
ipcp_lh         Status info the IPCP link handler administrator program
ipflowmonfh     IPFLOWMONFH SWB debug
ipflowmonrh     IPFLOWMONRH SWB RO information
iphoststatus    Status info for the hosts
ipiffh          IPIFFH SWB debug
iplicensingfh   IPLICENSINGFH SWB debug
ipsecfh         IPSECFH SWB debug
ipsectunnelfh   IPSECTUNNELFH SWB debug
iptransmode     information about ip transport settings
ixrh            IEXS::IXRH Topology
jdumpthreads    Dump the stack trace of Java threads
jfindjar        Find the Jar file that contains the Java class
jheapdump       Dump the heap statistics of Java classes
jheapinfo       Java heap information
jsinfo          Prints MultiCarrier info for Joint Scheduling.
keys            configure/display terminal key settings
lbim            Display information and manage images on flash
lhconfig        Config of link handlers
lhsh            Execute command on remote processor
license         License server command (license <cmd>)
linkstat        HDLC state and statistics for MP-ATF.
linkstat2       HDLC state and statistics for ATF in BPP.
linxeth         Tool for getting information about LINX ethernet connections
linxtrace       Enable or Disable LINX dc_disconnect trace
listObj         List an object.
list_filterobj  Print filter data
list_traceobj   Print trace data
listenv         list environment variables for <processes> and their corresponding block.
listloaded      List Loaded Modules
lkmcfg          View/create/delete Linx Ethernet links
llog            Read error log
ln              make a link from one file to another
load_zone       Command to display LoadZone information
loadbalance     Automatic load balancing for SMP
log             Log server command
logAll          Runs logDbcc,logDbch,logHsdbch,logEdbch and logEsc
logDbcc         Logs Dbcc resources
logDbch         Logs Dbch resources
logEdbch        Logs E-Dbch resources
logEsc          Logs E-Sc resources
logHsdbch       Logs Hs-Dbch resources
logMacHs_2      Logs all setup DBCC devices with its dbccId:s. If a cell is HS capable, macHs SNID will be a figure between 1 and 6
logUbch_3       Logs Ubch resources
logUbch_4       Logs Ubch resources
logUbch_5       Logs Ubch resources
logUbch_6       Logs Ubch resources
logUbch_7       Logs Ubch resources
logUbch_8       Logs Ubch resources
logattributes   List the attributes for a log
logclock        Start or stop logging of the system clock.
logdelete       Delete a log
login           login command is not supported
loglevel        Set loglevel for OSENET.
loglist         Lists all available logs
ls              list files
lsdtb           Display the contents of the Device Tree Blob
lsproc          List the most recently swaped in processes
maciDumpSession Dump session related information
mailboxLetterTrace Print the mailbox letter combination
man             man command
mch             MCH info
md5             prints MD5 checksum for a file
mdio            read registers from devices connected to mdio bus
memrd           Read CPU Memory
memwr           Write CPU Memory
migrate         Migrate a program to a core
mirror          Prints the status of the mirror driver
mkdir           create directories
mm              Display MM run-time state information
mount           mount a volume
mpcmd           Type mpcmd help for detailed help.
mpld            Print MP Load Sharing distribution info.
msi_list        Print region data for MSI
mv              rename/move files
namelookup      List registered services and pending lookups
nattstatus      Show NAT-T status
nbs             NBS
ncaeth          ncaeth shell command, use ethernet instead
ncli            ncli: start NCLI session to access CS.
ncpAlarmGet     This command displays the NCP device's alarms.
ncpAnd          This command is used to read a register and bit-wise AND the value with the value provided
ncpApiTraceDump This command displays the API trace buffer.
ncpBcastFill    Usage: ncpBcastFill [-a addr_stride] [ -c count ] [-D|-P|-T]
ncpBcastScatter Usage: ncpBcastScatter [-D|-P|-T] <devNum>.<node>.<target>.<offset>
ncpBcastWrite   Usage: ncpBcastWrite [-D|-P|-T] <devNum>.<node>.<target>.<offset>
ncpCatDecode      Take an incoming hex data stream (stdin or file), figure out the original
ncpCatRead      Use NCP RTE CAT utilities to take critical register data written to system memory, and output to stdout or a flat file.
ncpCatWrite     Use NCP RTE CAT utilities to capture important state to system memory.
ncpCeScriptLoad Usage: ncpCeScriptLoad [-i <devNum>] [-m <moduleNumber>] [-n <numScripts>]
ncpCeScriptUnload Usage: ncpCeScriptUnload [-i <devNum>] [-m <moduleNumber>] [-n <numScripts>]
ncpCfgTool      Usage: ncpCfgTool -h
ncpChanLoopbackSet This command displays MAC port Loopback configuration.
ncpCoherentRead Usage: ncpCoherentRead [-i <devNum>] [-w 8|16|32] [-D|P]
ncpCoherentWrite Usage: ncpCoherentWrite [-i <devNum>] [-w 8|16|32] [-D|-P|-T]
ncpCompare      Usage: ncpCompare [-c <count>] [-w 8|16|32|64] [-D|P]
ncpDecode       This command is used to decode the register values into meaningful fields.
ncpDevStats     This command displays the RTE device statistics.
ncpDeviceInfo   This command displays the device information.
ncpDomainCfg    This command allows the user to examine and/or modify the AMP Domain memory configuration
ncpDpiLoad      This command a loads compiled ruleset binary file.
ncpEioaSlotOvrclkGet This command displays overclocking information
ncpEioaSlotOvrclkSet This command forces overclocking for EIOA slot
ncpEioaSwitchStatistics This command displays the EIOA Switch Statistics.
ncpEioaTSPollRead This command reads the timestamp for a MAC channel.
ncpEioaTSRead   This command reads the timestamp for a MAC channel.
ncpEioaVPidRead This command Reads Virtual Pipeline Name and ID
ncpEioaVPidWrite This command sets Virtual Pipeline Name and Priority
ncpEngineSeqShow This command displays engine sequence details given
ncpExtMemBist   Perform tests on external BIST memory of a configured ACP.
ncpFill         This command fills the region identified by <devNum>.<node>.<target>.<offset>
ncpI2CRead      Exercise ACP I2C HW interface to read from devices (registers, EEPROM)
ncpI2CWrite     Exercise ACP I2C HW interface to write from devices (registers, EEPROM)
ncpIoPerf       Measures the CPU read/write performance of the specified device address space.
ncpIpDiag       This command executes an internal communications diagnostic test.
ncpLbiCfg       Configure chip selects and GPIO pins for devices on the ACP2500 LBI interface
ncpLinkStatus   This command displays the EIOA link status.
ncpLinkStatusBlock This command blocks on a Link State Change.
ncpMacAddrRead  This command displays MAC Address.
ncpMacAddrWrite This command sets the MAC Address
ncpMacAutoNegGet This command displays the state of the port Auto Negotiation enable flag
ncpMacAutoNegSet This command Enables/Disable Auto Negotiation for a port.
ncpMacMtuRead   This command displays MAC port Pause configuration.
ncpMacMtuWrite  This command sets MAC port MTU configuration.
ncpMacPauseRead This command displays MAC port Pause configuration.
ncpMacPauseWrite This command modifies MAC port Pause configuration.
ncpMacPhyRegRead This command displays the content of a PHY register.
ncpMacPhyRegWrite This command writes to a PHY register.
ncpMacStatistics This command displays the contents of the MAC statistics registers.
ncpMacStatus    This command displays MAC port status.
ncpMdioRead     This command displays the contents of a Clause 22 or Clause 45 PHY register.
ncpMdioWrite    This command writes Clause 22 or Clause 45 MDIO Phy registers.
ncpModify       This CLI will perform one or more 32-bit Read-Modify-Write
ncpMtmGlobalStats This command reads and prints the MTM global statistics counters.
ncpMtmNodeShow  This command reads and prints MTM node entries .
ncpNsEntryRead  CLI to display the table entries referenced by the Engine Tables
ncpNvmStatsGet  This command displays Non-volatile memory statistics.
ncpOr           This command reads the register(s) and bitwise ORs it with the value(s) provided.
ncpPkaTest      This command executes a set of pre-defined test vectors on the PKA engine
ncpPllInit      This command initializes the PLL clocks with default settings.
ncpPoll         This command is used to poll a register for specific value, mask and compare its value.
ncpRamTest      This utility will perform a simple memory test on the memory
ncpRead         This command displays the <count> number of values reading from
ncpRegister     Reads a single 32-bit word (register) from the specified
ncpReset        Perform a hardware/software reset of the NCP driver
ncpScatter      Provides a 64-bit scatter write to the specified node+target vector.
ncpSeFemEventsGet
ncpShell        Utility that provides a limited command interpreter on top of other CLIs.
ncpSmonInit
ncpSmonQuery
ncpSmonStop
ncpSpeedDuplexGet This command displays the contents of the MAC statistics registers.
ncpSpeedDuplexSet This command forces the speed and duplex settings on a Copper port.
ncpStatusPrint  Print the symbolic name of the specified ncp_st_t enumeration constant value (status code).
ncpSysClock     ncpSysClock is used to set the frequency or retrieve the current frequency of the system clock.
ncpSysmemPhyStatusShow Display SYSMEM PHY Status registers.
ncpTaskRecv
ncpTaskSend
ncpTaskShutdown
ncpTaskTraceDisable This command disables task tracing for the specified engine.
ncpTaskTraceEnable This command enables task tracing for the specified engine.
ncpTaskTraceLogShow This command provides the capability to inspect the NTF trace buffer for a given engine.
ncpTaskTraceTriggerDisable This command disables triggering for task tracing for the specified engine.
ncpTaskTraceTriggerEnable This command enables triggering for task tracing for the specified engine.
ncpTaskTraceTriggerSet This command sets trigger parameters for task tracing for the specified engine.
ncpTemplateShow This command displays the input and output templates for a given engine.
ncpTrngTest     This command uses the builtin TRNG module to provide random numbers.
ncpTvSense      This command displays the ACP tvsense statistics.
ncpUnicastAddrRead This command displays Unicast Filter Addresses.
ncpUnicastAddrWrite This command sets Unicast Addresses
ncpUsleep       This command is used to introduce micro-second sleep.
ncpVersion      This command displays the version of RTE being used.
ncpVirtualPipelineShow This command displays the Virtual Pipeline information.
ncpVoltage        Set the NCP chip's value (volts or vid) based upon an incoming file
ncpWrite        This command writes data to a register(s) of an ACP device.
ncpXrt73Cfg     This command programs the LBI+GPIO pins needed to perform I/O to XRT73 devices.
ncpXrt73Read    This command displays the <count> number of values reading from
ncpXrt73Write   This command writes data to an XRT73 GPIO device.
ndp             Display NDP cache entries
nehgammadata    Dumping EcNeh gamma data
nehidcptable    Dumping EcNeh IDCP Table
netstat         Display net statistics
node_id         node identity commands
notresocnt      Read or clear counter for not resolved problems on a given port nr.
notresoracnt    Read or clear counter for not resolved radio problems on a given port nr.
nsdbg           nsdbg enable
nsinfo          Nameserver information commands
nssconfigtimeacc Send the desired time accuracy to SCSPI clients
nssdegraderef   Simulate reference degradation
nssfixfrequency Force regulator to enter fix frequency mode. Synchronization reference should be selected when this command is used, clock should be in locked mode. Fix frequency mode will automatically end when frequency becomes good enough.
nsshist         Get NSS history information
nssholdoverthr  Set holdover threshold in minutes
nssinfo         Get NSS status information
nssmpinfo       Get NSS MP status information
nsspdvthr       Set pdv-threshold for a packet reference
nssprodtest     Access memory in DUXI to enable/disable LA_TEST_BUS or PROD_TEST_CLK_MUX in CCR register
nssreadhist     Reads current hist data from msi and flash disk
nssrefchangeinfo Get 20 latest reference switches
nssremovetime   Reset time state while in Time Holdover
nssscspiinfo    Get all client and subscriber info
nssselectregref Set the specified reference type as selectedreference in tureg and tuhwif.
nsssetcallimit  Set calibration expiration days limit
nsssetfastlock  Setting the jitter/wander tolerance level (R) for EXT REF which changes needed time for clock to become locked to the EXT REF.
nsssetfsyncreg  Set FSYNC transmit interval, pattern and phase alignment.
nsssysclkinfo   Get 20 latest SystemClock changes
nsstableinfo    Get NSS MP table information
nsstupktsync    Print useful information for troubleshooting
nsswritehist    Forces writing of hist data to flash disk or msi
ntp             NTP handling commands.
ntpconfig       get ntp info
ntprecover      ceases an NTP alarm and adjusts the node system time to the external NTP reference time
ospi_CXC1321315 Prints ospi status
overloadmon     Overload protection monitor to create load and collect statistics.
partition       Create, delete and list disk partitions.
passwd          Changing password for all users
pboot           Access of boot parameters in FLASH
pcapexplorer    Lists dumpcap traces. Traces can be deleted with the -d option
pci             PCI configuration read/write utility.
pgmUpgradeObj   Soft program upgrade
pgrun           Load and run a program from a load module
phySetRo_status Gets current status of SET RO object for one piuId
phy_eqmtbp      Lists equipment and driver data
phy_eqmtmp      Lists all objects on MP
phyhp_status    Gets current status of specified HP object
phyhp_status_all Gets current status of all specified HP objects
phylp_state     Gets current status of all specified lp objects
phylp_status    Gets current status of specified lp object
phylpdh_state   Gets current status of all specified lpdh objects
phylpdh_status  Gets current status of specified lpdh object
phyos155_status Gets current status of specified os155 object
phyos155_status_all Gets current status of all os155 objects
ping            The command verifies the IP connectivity to a host.
ping6           Verify the IPv6 connectivity to another IPv6 system
pm_create       Create a program.
pm_ff           Print all file formats supported.
pm_install      install a load module
pm_kill         Kill program
pm_lmconf       Print configuration for a load module image.
pm_lminfo       Print information for a/all load module image(s).
pm_pgconf       Print configuration for a program.
pm_pginfo       Print information for a/all program(s).
pm_pt           Print all program types supported.
pm_start        Start a program.
pm_uninstall    Uninstall a load module image
poolinfo        List information about pools
ppcpm           Processor performance monitoring
preload         Loads the flash with the specified programs
printf          ,redirect printf or end redirections
ps              list processes
pwd             print the working directory
qfDrvCmd        <qfDrvCmd ?> for description
qs              List signals in a process signal queue
raxlFaultInject_3 Injects a fault
raxlFaultInject_4 Injects a fault
raxlFaultInject_5 Injects a fault
raxlFaultInject_6 Injects a fault
raxlFaultInject_7 Injects a fault
raxlFaultInject_8 Injects a fault
rcmd            remote command execution
rcp             Copy files or directory to remote local volumes
rdfpga          Reads registers from the FPGA.
rdm             Read DSP Memory - alias for dspMemDump
rdsfp           Reads info related to given SFP.
readDsOffset_3  Prints FS-INFO/Ds Offset values for all cells
readDsOffset_4  Prints FS-INFO/Ds Offset values for all cells
readDsOffset_5  Prints FS-INFO/Ds Offset values for all cells
readDsOffset_6  Prints FS-INFO/Ds Offset values for all cells
readDsOffset_7  Prints FS-INFO/Ds Offset values for all cells
readDsOffset_8  Prints FS-INFO/Ds Offset values for all cells
readPower       Read the power consumption and temperature sensors.
readclock       Read system clock [unix date format]
readdspeventlog Read event log from DSP
reload          Restart the board (default warm)
resocnt         Read or clear counter for inop on a given port nr.
resoracnt       Read or clear counter for resolved radio problems on a given port nr.
restartObj      restarts an object.
restartntp      Restarts NTP Kernel
ricm            Print selected debug info. Call without args for help.
ricmfilter      Get the fault indication delay filter time in ms.
ricminfo        Prints history of events in RICM
riportglitch    Introduce link glitch on a <RI port> by disabling TX&RX for <glitch duration> ms.
rlc             Clear the ramlog
rld             Display ramlog
rlw             Write a string to the ramlog
rm              remove files
rmdir           remove (empty) directories
rollback        Rollback a transaction
route           Display or modify route table
rpmm            ram pmm commands
rrh             rrh help
rrt             Type 'rrt help' to display RoseRT debugger commands
rrt-CXC1735792%4_R14A Type 'rrt-CXC1735792%4_R14A help' to display RoseRT debugger commands
rrt-CXC1735793%4_R14B_1000 Type 'rrt-CXC1735793%4_R14B_1000 help' to display RoseRT debugger commands
rrt-CXC1735793%4_R14B_1001 Type 'rrt-CXC1735793%4_R14B_1001 help' to display RoseRT debugger commands
rrt-CXC1735793%4_R14B_1002 Type 'rrt-CXC1735793%4_R14B_1002 help' to display RoseRT debugger commands
rrt-CXC1735793%4_R14B_1003 Type 'rrt-CXC1735793%4_R14B_1003 help' to display RoseRT debugger commands
rrt-CXC1735793%4_R14B_1004 Type 'rrt-CXC1735793%4_R14B_1004 help' to display RoseRT debugger commands
rrt-CXC1735793%4_R14B_1005 Type 'rrt-CXC1735793%4_R14B_1005 help' to display RoseRT debugger commands
rrt-CXC1735793%4_R14B_1006 Type 'rrt-CXC1735793%4_R14B_1006 help' to display RoseRT debugger commands
rrt-CXC1735793%4_R14B_1007 Type 'rrt-CXC1735793%4_R14B_1007 help' to display RoseRT debugger commands
rrt-CXC1735893%4_R14A Type 'rrt-CXC1735893%4_R14A help' to display RoseRT debugger commands
rrt-CXC1735895%4_R14N Type 'rrt-CXC1735895%4_R14N help' to display RoseRT debugger commands
rrt_1000        Type 'rrt_1000 help' to display RoseRT debugger commands
rrt_1001        Type 'rrt_1001 help' to display RoseRT debugger commands
rrt_1002        Type 'rrt_1002 help' to display RoseRT debugger commands
rrt_1003        Type 'rrt_1003 help' to display RoseRT debugger commands
rrt_1004        Type 'rrt_1004 help' to display RoseRT debugger commands
rrt_1005        Type 'rrt_1005 help' to display RoseRT debugger commands
rrt_1006        Type 'rrt_1006 help' to display RoseRT debugger commands
rrt_1007        Type 'rrt_1007 help' to display RoseRT debugger commands
rsock           Configure/query rsock deamon.
run             Runs all intercepted processes
sadprint        Printout of the Security Association Database (SAD)
scc             scc help
sccrcinfo       sector = 1..6 carrier = 1..4 object = a string
scrub           scrubber commands
sctp_config     prints some SCTP-ROF configuration data
sctpadm         cmd sctpadm lists info about all Sctp Associations in SCTP ADM
sctpadm_config  cmd sctpadm_config lists some configuration data in SCTP ADM.
sctpadm_info    cmd sctpadm_info lists all process info in SCTP ADM
sctpadmrofcmd   cmd sctpadmrofcmd send trace settings to user plane.
sctphost        Prints some SCTP-ROF configuration data, statistical information and lists association or endpoint info in SCTP Host.
sctphost_info   cmd sctphost_info lists association or endpoint info in SCTP HOST
sctphost_stat   cmd sctphost_stat prints some statistical information
sctphosttrace   Configure log filtering and dumping internal log.
secmode
serialport      UART device driver settings
setAssuredMode  kindOfResource = 0..2 established = 0..1
setAttrObj      sets an attribute value for an object.
setGracePeriod  kindOfResource = 0..2 decreaseTimer = 1..1000
setGtpEchoOriginatorState WARNING
setboardtemp    Override read tempvalues with given tempvalue on given board temp sensor.
setclock        Set Clock
setenv          set/list environment variable [for block] [for process]
sethighsp       Set terminal speed to 115200 baud
setkey          Configure manual SAs and SPs
setlowsp        Set terminal speed to 9600 baud
setpri          This command has been disabled
sfftime         Set the fault indication delay filter time in ms.
sfp             Reads info related to given SFP.
shell           invoke shell
sigs            List information about signals
sleep           This command has been disabled
slowprh         SLOWPRH status and control
sma             Prints SMA status and container data
snapshot        Creates rmd snapshot of the system
sockstat        List open sockets
socprireadsfc   Read eSFC and SFC registers
socpritogreg    Toggle regulation for SoCpri reference
spdel           Delete a system parameter.
spdprint        Printout of the Security Policy Database (SPD)
spedit          Edit system parameters interactively
splitethcdbg    Returns debug information fetched from split eth client.
splitethevent   controls logging frequency for eventID 5
splitethsdbg    Returns debug information fetched from ose_split_server.
splitethstat    Shows/clears statistics of split ethernet server/client.
spmod           Stepwise view and modify system parameters.
spr             Read a system parameter.
spray
spw             Write a system parameter.
srio            SrioDriver shell command
srioconf        Read/write srio device registers
srt             SRIOMSG test utility.
ss              Show maximum process stack usage
ssw
stacks          list stacks
stat            report information about file/directory
statheapchc     static heap manager
supervision     enables/disables supervision of DSP's
swcon           Set or print srio switch congestion stats
swdump          Print srio switch registers
swi             Software installation commands
switchObj       Switch an object.
swperf          Enable/Disable or print srio switch performance stats
swport          Enable/Disable port on srio switch
sync            synchronize volume with disk
syncinfo        Get general Synchronization information
syspar          Get or set system parameters
te              Trace & Error Handling commands
tempsensorfault Generate temp sensor fault on given board temp sensor.
term            display info about terminal
tetxt           Adds INFO trace to CPP T&E log.
timers          Information about timers
tm              target monitor command
touch           Create an empty file.
traceSettingsRx_3 Sets general trace configuration on RX
traceSettingsRx_4 Sets general trace configuration on RX
traceSettingsRx_5 Sets general trace configuration on RX
traceSettingsRx_6 Sets general trace configuration on RX
traceSettingsRx_7 Sets general trace configuration on RX
traceSettingsRx_8 Sets general trace configuration on RX
traceSettingsTx_2 Sets general trace configuration on TX
tracejbdelay    Traces out the jitter buffer delay in the T&E log at certain intervals
traceroute      The command finds the routing path to a certain host.
traceroute6     Verify IPv6 routing to another IPv6 system
trce            prints information on TRCE container in flash
txlFaultInject_2 Injects a fault
uart            UART device driver statistics and settings
uetrace         Selective UE Tracing
uetraceRx_3     Configure number of UE's for trace settings
uetraceRx_4     Configure number of UE's for trace settings
uetraceRx_5     Configure number of UE's for trace settings
uetraceRx_6     Configure number of UE's for trace settings
uetraceRx_7     Configure number of UE's for trace settings
uetraceRx_8     Configure number of UE's for trace settings
uetraceTx_2     Configure number of UE's for trace settings on Tx
umask           display/set the current file system mask
unmount         unmount a volume
unsetenv        remove environment variables [from block] [from process]
uptime          display system uptime
usaaladm        information about usaaladm
usaalserver     information about usaalserver
uselmc_1        Selects an LMC
uselmc_2        Selects an LMC
uselmc_3        Selects an LMC
uselmc_4        Selects an LMC
uselmc_5        Selects an LMC
uselmc_6        Selects an LMC
uselmc_7        Selects an LMC
uselmc_8        Selects an LMC
vii             VII info
viilist         VII state list
vlandev         Create or remove VLAN device
vols            report volume statistics
wdm             Write DSP Memory - alias for dspMemChange
who             list who is logged on
winAal2Cmd      Use winAal2Cmd ? for description.
winAtcCmd       Use winAtcCmd ? for description.
winAtmCmd       Use winAtmCmd ? for description.
winCmd          Use winCmd ? for description.
winImaCmd       Use winImaCmd ? for description.
wrfpga          Writes to a register in the FPGA.
zzosvarp        Show the address of the OSE kernel data handle.
$

UCHHJRZ0162>
