The following commands are available:
 ?                               Displays all available commands
 abortsessionoperation           Interrupts the uploading or downloading of
                                 bulk CM files
 abortswsessionoperation         Interrupts software downloading
 activate                        Activates changes of attribute values
                                 specified in downloaded bulk CM XML file
 activateE1T1TimedLoopbackMode   Activates E1T1 loopback timeout
 activatesw                      Closes any established traffic connections and
                                 restarts STN with downloaded software
 activatetiusw                   Restarts TIU module with downloaded software
 approvesw                       Copies the software and config from the
                                 primary (active) area to the secondary
                                 (backup) area
 backup                          Orders the backup of OAM CM configuration to
                                 the destination file specified.  If <FileRef>
                                 contains an IPv6 address, then the address
                                 must be encapsulated in square brackets.  -u
                                 indicates that no password is supplied.
 caldate                         Displays or sets the calibration date
 calexpdate                      Displays or sets the calibration expire date
 calvalue                        Displays or sets the calibration value
 changePWD                       Set new password for admin or isp user. Usage:
                                 changePWD {user <userId>}|<old_pass>
                                 <new_pass> <ver_pass>
 checkconsistency                Checks the validity and consistency of an
                                 updated configuration
 clearDynamicMACFwTable          USAGE: clearDynamicMACFwTable all |
                                 <EthernetInterface> [<tagValue>] | help
 collectDCGInformation           Prints miscellaneous debuginformation
 commit                          Commits all configuration requests in the
                                 transaction
 createmo                        Creates the specified new MO
 dataencryption                  Activates data encryption or prints its status
 deleteAiMo                      Deletes all auto integration MO instances
 deletemo                        Deletes a MO identified by the
                                 baseObjectInstance
 destroyosmonsession             Destroy osmon session
 download                        Orders the downloading of a bulk CM XML
                                 configuration file for STN configuration. If
                                 <FileRef> contains an IPv6 address, then the
                                 address must be encapsulated in square
                                 brackets.
 downloadsw                      Orders the downloading of new software for the
                                 STN. If <FileRef> contains an IPv6 address,
                                 then the address must be encapsulated in
                                 square brackets.
 downloadtiusw                   Orders the downloading of new software for the
                                 TIU. If <FileRef> contains an IPv6 address,
                                 then the address must be encapsulated in
                                 square brackets.
 dump                            Reads the most recent restart dump
 endsession                      Ends a bulk CM session
 endswsession                    Ends a software upgrading or downgrading
                                 session
 endtransaction                  Ends a basic CM transaction
 exit                            Exits from shell
 generatekey                     Generate a new SSH host key.
 getalarmlist                    Returns all active alarms in the STN
 getcontainment                  Retrieves all MO instances in a specified MO
                                 containment hierarchy under and including the
                                 baseObjectInstance
 getcounters                     Displays Managed Object (MO) counters
 getirpversion                   Displays the version number of the Integration
                                 Reference Point(IRP) used between the STN and
                                 the OSS
 getlinkoam                      Displays Ethernet LinkOAM information
 getmoattribute                  Displays Managed Object(MO) attribute values
 getneighbors                    Returns current ARP and NDP cache
 getosmonsessions                Displays all osmon sessions
 getOSPF                         USAGE: getOSPF <OSPFv2Proc MO-DN>
                                 [border-routers | database [asbr-summary |
                                 external | max-age | network | nssa-external
                                 | router | summary] | interface | neighbor |
                                 route]
 getpendingconfiguration         Used to determine if there is a bulk CM
                                 download file ready to be activated
 getppplinkstats                 Traces get statistics of RTT on individual PPP
                                 links
 getsessionids                   Returns the identity of existing bulk CM
                                 sessions
 getsessionstatus                Returns the status of a specific bulk CM
                                 session
 getsubscriptionids              Returns all subscriptions existing in the STN
 getsubscriptionstatus           Returns the characteristics of subscriptions
 getswsessionids                 Returns the identity of existing software
                                 sessions
 getswsessionstatus              Returns the status of a specific software
                                 upgrading or downgrading session
 getTemperature                  Displays the readout of all temperature
                                 sensors
 gettime                         Displays the current system clock setting
 gettransactionid                Returns the identity of the transaction
 gettransactionstatus            Returns the status of the transaction, and is
                                 only possible to perform within a transaction
 help                            Displays all available commands
 log                             Reads or monitors the system logs
 ping                            Sends ICMP ECHO_REQUEST to network hosts
 ping6                           Sends ICMP ECHO_REQUEST to network hosts
 ping_ethernet                   Service OAM Loopback CLI command
 quit                            Exits from shell
 resettofactorysetting           Resets the STN to default factory settings
 restart                         Initiates a restart of the STN
 restore                         Restores new configuration on the node.  -d
                                 indicates that delayed restore shall be used.
                                  -c indicates that caller only wants to check
                                 if file will apply. The file will not
                                 actually be applied.  -u indicates that no
                                 password is supplied.
 resumepmmeasurements            Initiates/Enables PM data uploading.  If
                                 <fileStore> contains an IPv6 address, then
                                 the address must be encapsulated in square
                                 brackets.
 resumesubscription              Activates a defined but suspended subscription
 rev                             Returns revisions of everything
 setmoattribute                  Sets MO attribute values
 settime                         Sets the value of the system clock
 showMACFwTable                  USAGE: showMACFwTable all |
                                 <EthernetInterface> [<tagValue>] | help
 simpleping                      A simple function to make ping between source
                                 and destination address
 simpleping6                     A simple function to make ping6 between source
                                 and destination address
 startsession                    Starts a bulk CM session
 startswsession                  Starts a software upgrading or downgrading
                                 session
 starttransaction                Starts a basic CM transaction
 subscribe                       Defines a new IP address to subscribe for SNMP
                                 alarms & notifications
 suspendpmmeasurements           Stops/Disables PM data collection and PM data
                                 upload
 suspendsubscription             Disables or stops the sending of alarms and
                                 notifications
 syslog                          Reads or monitors the system logs
 timeservertest                  Displays information on the connectivity and
                                 the quality of the network towards a
                                 timeserver
 tiuCli                          Connects to the TIU cli
 traceallmoattributeinlog        Prints values of all MIB configuration
                                 attributes in log.  Note: Counter values are
                                 returned as raw data, accurate values of
                                 counters should be read with
                                 resumepmmeasurements command
 tracepath                       Traces path to a network host discovering MTU
                                 along this path
 tracepath6                      Traces path to a network host discovering MTU
                                 along this path
 traceroute                      Prints the route packets take to network hosts
 traceroute6                     Prints the route packets take to network hosts
 traceroute_ethernet             Service OAM Linktrace CLI command
 unsubscribe                     Disables or stops the sending of alarms,
                                 notifications and removes the subscription
 upload                          Orders the uploading of a bulk CM XML
                                 configuration file to the destination file
                                 specified. If <FileRef> contains an IPv6
                                 address, then the address must be
                                 encapsulated in square brackets.
 uptime                          Displays how long the system has been running
 uselocalsftp                    Use the local terminal for SFTP (default off).
                                 Usage: uselocalsftp <on|off>
 uselocalsshd                    This command no longer has any effect.
