# **********************************************************************
# %CCaseFile:	bif.txt %
# %CCaseRev:	/main/R60DJ/R60EH/R70N/1 %
# %CCaseDate:	2009-09-18 %
# Author:	xykgisi
#
# Short description:
# ET-IP Board Information File (BIF) used for IPG board with CEG BASIC FPGA
# **********************************************************************
#
# © Ericsson AB 2009 All rights reserved.
# The information in this document is the property of Ericsson.
# Except as specifically authorized in writing by Ericsson, the receiver of this
# document shall keep the information contained herein confidential and shall protect
# the same in whole or in part from disclosure and dissemination to third parties.
# Disclosure and disseminations to the receivers employees shall only be made
# on a strict need to know basis.
#
# **********************************************************************
#
# Rev          Date         Name        What
# -----        -------      --------    --------------------------
# cppdev/1     2009-09-18   xykgisi     File copied from 
#                                       /BIF-LM_CNX9010281/import/bif.txt cppdev/12
# **********************************************************************

# File format description
# -----------------------
# The BIF consists of 1..n records.  Each record consists of a number
# of lines described below.  The order of lines in each record is
# important; it has to be HEADER,DRIVER,FIRMWARE,TEST.  E.g., do not
# try to put TEST before FIRMWARE)
#
# The order of FIRMWARE and TEST lines within a record is also
# important.  The order of firmwares defines the load order, and the
# order of tests defines the test execution order.
#
# Record format:
# HEADER line       (1)
# DRIVER line       (1)
# FIRMWARE line(s)  (1..num firmware)
# TEST line(s)      (0..num tests)
#
# Line formats:
# HEADER=board product number, revision, num drivers, num firmware, num tests
# DRIVER=driver id, ... (NOTE: Number of driver id entries must match num drivers in HEADER)
# FIRMWARE=firmware product number, driver id, firmware id
# TEST=driver id, test id
#
# The board product number includes any index (e.g. /1, /2). Revision
# only uses the number and not the letter (e.g. R2A and R2B are both
# referred to as R2).  The enumerated values for driver id, firmware
# id, and test id are all defined in the BHDRV IWD (1/155 19-CXA 110
# 2996 Uen)


# ET-MFG R2
HEADER=ROJ1192232/1,R2,1,2,0
DRIVER=0
FIRMWARE=CXC1327341,0,1
FIRMWARE=CXC1327340,0,0

# ET-MFG default
HEADER=ROJ1192232/1,DEFAULT,1,2,0
DRIVER=0
FIRMWARE=CXC1327341,0,1
FIRMWARE=CXC1327340,0,0

# ET-MFX11 R4
HEADER=ROJ1192315/1,R4,2,2,0
DRIVER=1,2
FIRMWARE=CXC1722504,1,3
FIRMWARE=CXC1722863,1,2

# ET-MFX11 default
HEADER=ROJ1192315/1,DEFAULT,2,2,0
DRIVER=1,2
FIRMWARE=CXC1722504,1,3
FIRMWARE=CXC1722863,1,2

# ET-MFX12 default
HEADER=ROJ1192316/1,DEFAULT,2,2,0
DRIVER=1,2
FIRMWARE=CXC1722504,1,3
FIRMWARE=CXC1723089,1,2

# ET-MFX13 default
HEADER=ROJ1192317/1,DEFAULT,2,2,0
DRIVER=1,2
FIRMWARE=CXC1722504,1,3
FIRMWARE=CXC1723089,1,2

# ET-MFX14 R1A
HEADER=ROJ1192399/1,R1A,2,2,0
DRIVER=1,2
FIRMWARE=CXC1722504,1,3
FIRMWARE=CXC1723089,1,2

# ET-MFX11 ver2 default 
HEADER=ROJ1192315/2,DEFAULT,2,2,0 
DRIVER=1,2 
FIRMWARE=CXC1722504,1,3 
FIRMWARE=CXC1726411,1,2 

# ET-MFX12 ver2 default 
HEADER=ROJ1192316/2,DEFAULT,2,2,0 
DRIVER=1,2 
FIRMWARE=CXC1722504,1,3 
FIRMWARE=CXC1726412,1,2

# ET-MFX11 ver3 default 
HEADER=ROJ1192315/3,DEFAULT,2,2,0 
DRIVER=1,2 
FIRMWARE=CXC1722504,1,3 
FIRMWARE=CXC1726411,1,2 

# ET-MFX12 ver3 default 
HEADER=ROJ1192316/3,DEFAULT,2,2,0 
DRIVER=1,2 
FIRMWARE=CXC1722504,1,3 
FIRMWARE=CXC1726412,1,2

# ET-IPG default
HEADER=ROJ1192345/1,DEFAULT,1,2,0
DRIVER=3
FIRMWARE=CXC1728952,3,5
FIRMWARE=CXC1725371,3,4

# CBM test board
HEADER=ROJ1192359/1,DEFAULT,2,1,2
DRIVER=4,5
FIRMWARE=CXC1726213,4,6
TEST=4,1
TEST=4,3
ATTRIBUTES=MACI

# CBM ETIPM default
HEADER=ROZ104832/1,DEFAULT,2,1,2
DRIVER=4,5
FIRMWARE=CXC1726213,4,6
TEST=4,1
TEST=4,3
ATTRIBUTES=MACI

# DUW default
HEADER=ROA1282867/1,DEFAULT,2,1,2
DRIVER=4,5
FIRMWARE=CXC1726213,4,6
ATTRIBUTES=MACI

# DUW default
HEADER=ROA1282867/1,DEFAULT,2,1,2
DRIVER=4,5
FIRMWARE=CXC1726213,4,6
ATTRIBUTES=MACI

# DUW-M : ROZ 104 833/151
HEADER=ROA1285034/1,DEFAULT,2,1,2
DRIVER=4,5
FIRMWARE=CXC1726213,4,6
TEST=4,1
TEST=4,3
ATTRIBUTES=MACI

# DUW-E: ROZ 104 833/151
HEADER=ROA1285033/1,DEFAULT,2,1,2
DRIVER=4,5
FIRMWARE=CXC1726213,4,6
TEST=4,1
TEST=4,3
ATTRIBUTES=MACI

# DUL default
HEADER=ROA1282827/2,DEFAULT,2,1,2
DRIVER=4,5
FIRMWARE=CXC1726213,4,6
TEST=4,1
TEST=4,3
ATTRIBUTES=MACI

# DUL default
HEADER=ROA1282827/3,DEFAULT,2,1,2
DRIVER=4,5
FIRMWARE=CXC1726213,4,6
TEST=4,1
TEST=4,3
ATTRIBUTES=MACI

# DUL default
HEADER=ROA1282827/4,DEFAULT,2,1,2
DRIVER=4,5
FIRMWARE=CXC1726213,4,6
TEST=4,1
TEST=4,3
ATTRIBUTES=MACI

# CBM3 TP1 
HEADER=ROA1284144/1,DEFAULT,1,0,0
DRIVER=7
# Firmware embedded in same LM
ATTRIBUTES=MACI

# CBM3 KDU TP1 (Firmware embedded in same LM) 
HEADER=KDU137700/1,DEFAULT,1,0,0
DRIVER=7
# Firmware embedded in same LM
ATTRIBUTES=MACI

# CBM3 DUS 41 (Firmware embedded in same LM) 
HEADER=ROA1283711/1,DEFAULT,1,0,0
DRIVER=7
# Firmware embedded in same LM
ATTRIBUTES=MACI

# CBM3 DUS 31 (Firmware embedded in same LM) 
HEADER=KDU137624/3,DEFAULT,1,0,0
DRIVER=7
# Firmware embedded in same LM
ATTRIBUTES=MACI

# CBM3 DUS 41 (Firmware embedded in same LM) 
HEADER=KDU137624/1,DEFAULT,1,0,0
DRIVER=7
# Firmware embedded in same LM
ATTRIBUTES=MACI

# DUL21
HEADER=ROA1284608/1,DEFAULT,2,1,0
DRIVER=4,5
FIRMWARE=CXC1726213,4,6
ATTRIBUTES=MACI

# KDU/DUL21
HEADER=KDU137795/1,DEFAULT,2,1,0
DRIVER=4,5
FIRMWARE=CXC1726213,4,6
ATTRIBUTES=MACI

# KDU/DUL21
HEADER=KDU137834/1,DEFAULT,2,1,0
DRIVER=4,5
FIRMWARE=CXC1726213,4,6
ATTRIBUTES=MACI


