
===============================================
MTS2000 Radio Tuner Software R02.02.00
===============================================

 - VISTA (32-bit) with Service Pack 1 is now a supported operating system! 

Attention VISTA users:

The following configurations on Vista Home Premium and Business Premium 
must be set for the Tuner to function properly. 

•	Vista Theme should be set to “Windows Classic”
•	When saving radio's tuner information to a file, then name of the 
	file should not exceed 30 characters.
•	Vista Compatible Printer is required for using the Print 
	functionality in the Tuner.


Supported Operating Systems:
============================
RS232 Operation: 
 
 Windows NT 4.0 (SP 6 or higher)
 Windows 2000 Professional
 Windows XP Home Edition and Professional
 Windows Vista (32-bit) Home Premium and Business Premium
 Note:  (Pre-installed only, XP/VISTA upgrade from other 
        Operating systems is not supported at this time.)
	Windows ME and Windows 98 are no longer supported.
	You may choose to proceed with the installation, but 
        some features might not be functioning properly. 
        Upgrading the operating system is highly recommended.


Hardware Requirements:
---------------------

The following should be considered minimum hardware requirements
for running the ASTRO Radio Tuner.

Processor      400 MHz or higher Pentium grade Processor
Memory         128 MB RAM minimum (Win NT 4.0 SP6+ / Win2000/ XP)
               1 GB RAM minimum (Win Vista)

Hard Disk Space  500MB hard drive with 40MB free space
 
Peripherals    One Serial COM Port
               CD-ROM Drive

  
Installation:
------------

When you insert the Installation CD into the CD-ROM
drive of your computer, the installation should run 
automatically, if it does not, run  Setup.exe file 
which appears in the Installation CD window, and 
follow the instructions.


Uninstalling the Tuner:
--------------------

Before uninstalling the MTS2000 Tuner, the 
following must be performed.

   1) Close the Motorola Application Launcher, if its 
      icon appears in the system tray of the taskbar.
   2) Exit any active CPS/Tuner applications.

Then, to uninstall the MTS2000 Tuner, select 
Start->Settings->Control Panel.  Double-click on Add/
Remove Programs.  In the Add/Remove Programs window, 
select Motorola MTS2000 Tuner, and click 
on the Add/Remove button.  Follow the instructions that 
appear.  


Online Help:
-----------

Extensive online Help is available from within the 
MTS2000 Tuner application.  After activating the Tuner 
(Start>Programs->Motorola->MCS MTS 2000 Products->MTS2000 
Tuner), choose "Help Topics" from the Help menu. A full 
listing of Help topics will appear. 


Known Issues With the MTS2000 Tuner R02.02.00 Release:
---------------------------------------------------

1) Tuner performance varies with processor speed and RAM.

2) When any slider control is selected, the up cursor key 
will decrement the current value (move the slider to the 
left) and the down cursor key will increment the current 
value (move the slider to the right). To avoid this problem, 
use the mouse, the left/right cursor keys, or click on the 
value spin box instead.

3) The Program button will fail to store the value if the 
radio contains a non-standard serial number.
 
===============================================
