# MOTOTRBO AirTracer

### Table of Contents

1. Introduction

2. What's new in this release

3. Requirements

4. Installation, Removal

5. Legal notice

6. Motorola Open Source Software Legal Notices Document

### 1. Introduction

Welcome to the AirTracer for the MOTOTRBO portable and mobile radios.

### 2. What's new in this release

Version | Notes
5.1 (Build 20) | Support for Microsoft® Windows® 7 Home Premium and Professional Editions.
4.5 (Build 19) | Support for larger trace files.
4.0 (Build 16) | Support for the new radio software.
3.6 (Build 14) | Fix for the error message issue when there is no audio device available.
3.5 (Build 12) | Support for Microsoft® Windows® Vista Home Premium and Business Editions.
3.0 (Build 11) | Support for the new radio software.
1.0, 2.0 (Build 7, 8) | Support for the MOTOTRBO radios. Start/Stop Trace and logs the packets in a file. Read Error Log and logs the error in a file.

### 3. Requirements

Operating System |
Microsoft® Windows® 7 Home Premium Edition Microsoft® Windows® 7 Professional Edition Microsoft® Windows® Vista Home Premium Edition Microsoft® Windows® Vista Business Edition Microsoft® Windows® XP Home/Professional Edition with SP2 or SP3 |  |
Hardware Recommendations
· The application takes approximately 100 MB of free disk space on your PC. However, more space would be required to save the error log files or signal trace log files of your radios.
· For processor speed and RAM, the recommendations given by Microsoft for the release of the operating system that you are using should be sufficient.
· A USB port.
· A CD-ROM drive.

### 4. Installation, Removal

Installation
You need to have Administrator rights on the target PC in order to install the software. Follow the steps below for the CD-ROM version: · Insert the CD-ROM containing the installation into the CD-ROM drive. · If the installation application doesn't start within 30 seconds, the auto-run feature for CD-ROMs for you operating system is likely disabled. Browse to your CD-ROM and run the autorun.exe program. For example, if the E:\ drive is the CD-ROM, run E:\autorun.exe. Follow the steps below for the software package version: · Unzip the AirTracer package to a directory of a local disk. · Browse to this directory and run the setup.exe program. If a previous version of AirTracer has already been installed, you will be given the option to “Repair” or “Remove”. If you are upgrading the AirTracer, then remove the previous version and start the installation process again. If you are re-installing the AirTracer, then choose the repair option. Note: During re-install, settings for sound and language will be reset to their default values. You will need to check these settings after the new version has been installed and make changes as necessary.
Removal
From the Start button on the task bar of your operating system, select Settings > Control Panel. Select the Add/Remove Programs option within the control panel. Select the MOTOTRBO AirTracer item in the "Currently installed programs" box and click the remove button.

### 5. Legal notice

Motorola and MOTOTRBO are registered trademarks of Motorola, Inc.

Microsoft® and Windows® are registered trademarks of Microsoft Inc.

### 6. Motorola Open Source Software Legal Notices Document