# MOTOTRBO Tuner

### Table of Contents

1. Introduction

2. What's new in this release

3. Requirements

4. Installation, Removal

5. Legal notice

6. Motorola Open Source Software Legal Notices Document

### 1. Introduction

Welcome to the MOTOTRBO Tuner for the MOTOTRBO radios.

### 2. What's new in this release

Version | Notes
5.5 (Build 91) | Support for 350 MHz and CoS models. Support for T2000A/T3000A 800/900 bands models.
5.2 (Build 85) | Support for Dynamic Mixed Mode feature.
5.1 (Build 80) | Support for Microsoft® Windows® 7 Home Premium and Professional Editions. Support for 800/900 bands models.
5.0 (Build 79) | Support for T2000A/T3000A UHF Range 1 and Range 2 model. Support for 3600 Trunking Capable Radios.
4.6 (Build 72) | Support for Analog only models.
4.5 (Build 66) | Support for H55XDH9LA1AN, H55XDH9JA1AN, H55XDC9LA1AN and H55XDC9JA1AN models.
4.0 (Build 54) | Support for Front End Filter Auto Tuning. Enhanced validation for Power Tuning values.
3.6 (Build 46) | Support for UHF Band 2 models. Fix for the error message issue when there is no audio device available.
3.5 (Build 44) | Support for Microsoft® Windows® Vista Home Premium and Business Editions.
3.0 (Build 37) | Support for additional UHF/VHF high/low power models.
2.0 (Build 31) | Support for VHF high power models.
1.0 (Build 20) | Support for the MOTOTRBO radios. Tune the transmitter and receiver of the radio. One time programming of serial number on blank boards.

### 3. Requirements

Operating System |
Microsoft® Windows® 7 Home Premium Edition Microsoft® Windows® 7 Professional Edition Microsoft® Windows® Vista Home Premium Edition Microsoft® Windows® Vista Business Edition Microsoft® Windows® XP Home/Professional Edition with SP2 or SP3 and Windows Installer 3.1 |  |
Hardware Recommendations
· The application takes approximately 100 MB of free disk space on your PC. However, more space would be required to save archive files of your radios. Each archive file varies in size depending on the features of the radio.
· For processor speed and RAM, the recommendations given by Microsoft for the release of the operating system that you are using should be sufficient.
· A USB port.
· A CD-ROM drive.
· For best display results, set the DPI setting of your PC to the Normal size (96 DPI)

### 4. Installation, Removal

Installation
You need to have Administrator rights on the target PC in order to install the software. Proceed as follows for CD-ROM version: · Insert the CD-ROM containing the installation into the CD-ROM drive. · If the installation application doesn't start within 30 seconds, the auto-run feature for CD-ROMs in your operating system is likely disabled. Browse to your CD-ROM and run the autorun.exe program. For example, if the E:\ drive is the CD-ROM, run E:\autorun.exe.

Proceed as follows for software package version:

· Unzip the Tuner package to a directory of a local disk.

· Browse to this directory and run the setup.exe program.

If you are installing a newer version of Tuner, then remove the previous version and start the installation process again. If you are re-installing the same version of Tuner, then choose the repair option.

Note: During re-install, settings for preferences and dealer information will be reset to their default values. You will need to check these settings after the new version has been installed and make changes as necessary.

Removal
From the Start button on the task bar of your operating system, select Settings > Control Panel. Select the Add/Remove Programs option within the control panel. Select the MOTOTRBO Tuner item in the "Currently installed programs" box and click the remove button.

### 5. Legal notice

Motorola and MOTOTRBO are registered trademark of Motorola, Inc.

Microsoft® and Windows® are registered trademarks of Microsoft Inc.

### 6. Motorola Open Source Software Legal Notices Document