==================================================================================

 SOFTWARE RELEASE NOTE

==================================================================================

Product           : MPT1327 GOB Upgrade kit Package
Release           : R01.01.02
Date              : 14-May-2014
Language          : English
Supporting OS     : Win2k,WinXP,Win7

NOTICE: The CPS PROGRAMMING DATA WILL BE LOST AFTER UPGRADING. PLEASE SAVE YOUR 
EXISTING CODEPLUG TO AN ARCHIVE FILE. It is recommended to save an archive of the 
radio's codeplug using CPS before the update process. After upgrading, this archive 
can be used to recover the CPS programming data of the radio.

==================================================================================

 Purpose of this release

==================================================================================

Supported features:

- Up-version a radio to software version R01.01.01 with 
  codeplug R02.01.00 from previous released MPT1327 GOB 
  software.

Supported Software versions:

- Only official MPT1327 GOB software release version.
  R01.00.00
  R01.01.00

Supported model number:
Model Number    Latest Version    
----------------------------------
H55JDC9JA1AN    R01.01.00
H55JDC9JA2AN    R01.01.00
H55JDC9JC1AN    R01.01.00
H55JDC9LA1AN    R01.01.00
H55JDC9LA2AN    R01.01.00
H55JDC9LC1AN    R01.01.00
H55JDH9JA1AN    R01.01.00
H55JDH9JA2AN    R01.01.00
H55JDH9JC1AN    R01.01.00
H55JDH9LA1AN    R01.01.00
H55JDH9LA2AN    R01.01.00
H55JDT9JA1AN    R01.01.00
H55PDC9JA1AN    R01.01.00
H55PDC9LA1AN    R01.01.00
H55PDH9JA1AN    R01.01.00
H55PDH9LA1AN    R01.01.00
H55QDC9JA1AN    R01.01.00
H55QDC9JC1AN    R01.01.00
H55QDC9LA1AN    R01.01.00
H55QDH9JA1AN    R01.01.00
H55QDH9JC1AN    R01.01.00
H55QDH9LA1AN    R01.01.00
H55QDJ9JA1AN    R01.01.00
H55QDJ9LA1AN    R01.01.00
H55QDT9JA1AN    R01.01.00
H55TDC9JA1AN    R01.01.00
H55TDC9JC1AN    R01.01.00
H55TDC9LA1AN    R01.01.00
H55TDH9JA1AN    R01.01.00
H55TDH9LA1AN    R01.01.00
H55TDT9JA1AN    R01.01.00
H55XDC9JA1AN    R01.01.00
H55XDC9LA1AN    R01.01.00
H55XDH9JA1AN    R01.01.00
H55XDH9LA1AN    R01.01.00
M27JNC9JA1AN    R01.01.00
M27JNC9JA2AN    R01.01.00
M27JNC9JC2AN    R01.01.00
M27JNC9LA1AN    R01.01.00
M27JNC9LA2AN    R01.01.00
M27JNH9JA1AN    R01.01.00
M27JNH9JA2AN    R01.01.00
M27JNH9JC2AN    R01.01.00
M27JNH9LA1AN    R01.01.00
M27JNH9LA2AN    R01.01.00
M27JQC9JA1AN    R01.01.00
M27JQC9JA2AN    R01.01.00
M27JQC9JC1AN    R01.01.00
M27JQC9JC2AN    R01.01.00
M27JQC9LA1AN    R01.01.00
M27JQC9LA2AN    R01.01.00
M27JQH9JA1AN    R01.01.00
M27JQH9JA2AN    R01.01.00
M27JQH9JC2AN    R01.01.00
M27JQH9LA1AN    R01.01.00
M27JQH9LA2AN    R01.01.00
M27PNC9JA2AN    R01.01.00
M27PNC9LA2AN    R01.01.00
M27PNH9JA2AN    R01.01.00
M27PNH9LA2AN    R01.01.00
M27PRC9JA2AN    R01.01.00
M27PRC9LA2AN    R01.01.00
M27PRH9JA2AN    R01.01.00
M27PRH9LA2AN    R01.01.00
M27QNC9JA1AN    R01.01.00
M27QNC9JA2AN    R01.01.00
M27QNC9JC2AN    R01.01.00
M27QNC9LA1AN    R01.01.00
M27QNC9LA2AN    R01.01.00
M27QNH9JA1AN    R01.01.00
M27QNH9JA2AN    R01.01.00
M27QNH9JC2AN    R01.01.00
M27QNH9LA1AN    R01.01.00
M27QNH9LA2AN    R01.01.00
M27QPC9JA1AN    R01.01.00
M27QPC9JA2AN    R01.01.00
M27QPC9JC1AN    R01.01.00
M27QPC9JC2AN    R01.01.00
M27QPC9LA1AN    R01.01.00
M27QPC9LA2AN    R01.01.00
M27QPH9JA1AN    R01.01.00
M27QPH9JA2AN    R01.01.00
M27QPH9JC2AN    R01.01.00
M27QPH9LA1AN    R01.01.00
M27QPH9LA2AN    R01.01.00
M27TRC9JA1AN    R01.01.00
M27TRC9JA2AN    R01.01.00
M27TRC9JC1AN    R01.01.00
M27TRC9LA1AN    R01.01.00
M27TRC9LA2AN    R01.01.00
M27TRH9JA1AN    R01.01.00
M27TRH9JA2AN    R01.01.00
M27TRH9LA1AN    R01.01.00
M27TRH9LA2AN    R01.01.00
M27QNH9LC1AN    R01.01.00
M27QNC9LC1AN    R01.01.00
M27JNC9LC1AN    R01.01.00
M27JNH9LC1AN    R01.01.00
M27QPH9LC1AN    R01.01.00
M27QPC9LC1AN    R01.01.00
M27JQH9LC1AN    R01.01.00
M27JQC9LC1AN    R01.01.00
M27TRH9LC1AN    R01.01.00
M27TRC9LC1AN    R01.01.00
H55QDH9LC1AN    R01.01.00
H55JDH9LC1AN    R01.01.00
H55QDC9LC1AN    R01.01.00
H55TDH9LC1AN    R01.01.00
H55TDC9LC1AN    R01.01.00


==================================================================================

WARNING

==================================================================================

PLEASE READ:  WARNING FOR ALL RADIO TYPES 

PLEASE SAVE YOUR EXISTING MPT1327 GOB CODEPLUG AS AN ARCHIVE FILE. The codeplug 
programming information may be lost after the update process therefore, it is 
recommended to read the MPT1327 GOB using the CPS, and save an archive of the 
MPT1327 GOB's codeplug before starting the update process. After the update, this 
archive can now be used to recover the codeplug programming information by 
programming the archive back into the MPT1327 GOB.

Ensure the radio updating process is not interrupted. Interruption will cause the 
radio not to operate anymore and attempting to update the radio again will NOT be 
successful.

Do NOT create a shortcut of the program (e.g. on your desktop), the program might 
not be able to find the data files in that case!

Do not remove the programming cable or turn off the radio while the update is in 
progress.

In case of failure during the updating, a message box will appear to guide the user 
to recover from the failure, if possible.

You may not run more than one copy of the program at the same time.


==================================================================================

 How to install and run this software

==================================================================================

Installation of the software can be completed by double clicking the setup file 
"gobupgradekit.msi", and can be started through Programs Menu.

The procedure for upgrading 

1. Use CPS R02.00.02 to read MPT1327 GOB.
2. Record the channel information.
3. Use upgradekit to upgrade firmware and codeplug version number.
4. Use CPS to write codeplug to MPT1327 GOB(CPS will prompt you that the codeplug 
   will be upgraded).
5. Use CPS to read the MPT1327 GOB.


==================================================================================

INSTRUCTIONS ABOUT UPGRADING PROCESS

==================================================================================

The following instructions detail the operations of the Firmware Kit:

(Note: These instructions must be followed in the exact order to work properly):
 1.  Start the Firmware Kit by going to Start->Programs Menu-> Motorola -> 
     Matrix MPTGOB Upgrade Kit R01.01.02 -> GOB Upgrade Kit

 2. Connect a fully charged battery or a power supply to the radio and turn the
    radio on. Ensure that the radio has powered up properly and stay in MPT mode.

 3. Attach the programming cable to your portable radio. Connect the programming 
    cable to the computer.

 4. After the tool is launched, go to menu Config->Comm Setting. Make sure the IP 
    address of connected radio is present. If multiple radios connected, drop down
    list allow to one of radio as the operation target.

 5. Once the upgrade screen appears, click on the "PROGRAM" button and follow
    the instructions.

 6. You will now see a status bar indicating the percentage of completion.

 7. Once the radio is updated, remove the programming cable.
    Note: This is very important, even if you are going to update another radio.

 8. To update another radio, go to step #2.


==================================================================================

TROUBLESHOOTING

==================================================================================

If installation can't proceed on Window2000
1. Please double click "WindowsInstaller-KB893803-v2-x86.exe" from upgrade kit
   installation package to patch window. And then try installation again.

If Firmware Kit will not start

1. Make sure this is an original version of the kit and not copied off another
   computer
2. Make sure another copy is not running on your computer.
3. Make sure the virtual studio runtime library is installed in your computer. 
   If it is not, please double click "vcredist_x86.exe" from the upgrade kit 
   installation package.

If an error is returned when you select program, check the following:

1.  On the Comm setting menu, make sure that the IP is presented and proper IP is
    selected. This IP will also present in right-bottom corner of status bar.
2.  Make sure the radio is on and properly connected to the computer.
3.  Make sure the radio USB driver is properly installed. If it is not, please 
    re-install it from <upgrade installation directory>\MOTOTRBO_Driver according 
    to your OS version.

If an error is occurred in the middle of flashing and Upgrade kit can not continue
to proceed with the upgrading, then try the following:

1.  close upgrade kit application
2.  reset the radio
3.  launch upgrade kit application and try to program again.


==================================================================================

WARNING

==================================================================================

Ensure MPT1327 GOB flashing is not interrupted. Interruption will cause the MPT1327 
GOB not to operate anymore. Trying to flash the MPT1327 GOB again will not work. The 
MPT1327 GOB has to be returned to the depot for service.


===========================
RADIO SOFTWARE RELEASE NOTE
===========================

---------------------------------------
Release MPT1327 GOB - R01.01.01