# MOTOTRBO Tuner

### Table of Contents

1. Introduction

2. What's new in this release

3. Requirements

4. Installation, Removal

5. Legal notice

6. Motorola Solutions Publically Available Software Legal Notices Document

### 1. Introduction

Welcome to the MOTOTRBO Tuner for the MOTOTRBO radios.

### 2. What's new in this release

Version | Notes
11.5 (Build 196) | Support for MOTOTRBO 2 ATEX Ma UHF Range 1 and VHF Portable.
11.0 (Build 187) | Support for MOTOTRBO Light UHF Range 2 Portable. Support for MOTOTRBO Light UHF Range 1 Extended(403-480MHz) Portable.
10.9 (Build 181) | Support for SL Series Commercial VHF Band and UHF Range 1 Portable.
10.7 (Build 171) | Support for MOTOTRBO 2 300 MHz, 350 MHz and 800/900 MHz Band Mobile. Support for MOTOTRBO Light 350 MHz Portable. Support for MOTOTRBO 2 UHF and VHF radios with GNSS capability. Support for UHF enhancement Band for SL Series radio.
10.5 (Build 158) | Support for Digital RX only Repeater. Support for Customized PWM(pulse width modulation) Tx spur mitigation for MOTOTRBO 2 portables and SL Series radios. Support for UHF Band 2 for SL Series radio.
10.1 (Build 150) | Support for 800 MHz and 900 MHz bands for SL Series radios Support for 300/350 MHz band for MOTOTRBO 2.0 portables
10.0 (Build 148) | Support for MOTOTRBO Light radios.
9.5 (Build 144) | Support for MOTOTRBO 2 800/900 MHz band portable. Support for XiR E8600 Series, DP3441 and DGP 8050 Elite Portables. Support for Microsoft® Windows® 8.
9.0 (Build 136) | Support for MOTOTRBO 2 UHF Band 2 Mobile
8.5 (Build 123) | Support for MOTOTRBO 2 ATEX Radio
8.0 (Build 120) | Support for MOTOTRBO 2 Portable. Support for MOTOTRBO 2 Repeater.
7.0 (Build 114) | Support for MOTOTRBO 2 Mobile. Support for SL Series radios.
6.8 (Build 108) | Support for XPR 6580 IS models.
6.5 (Build 101) | Support for Rx Only MTR3000.
6.5 (Build 98) | Bug fixes.
6.0 (Build 97) | Support for Minimum Volume Setting.
5.6 (Build 93) | Support for additional analog portable models.
5.5 (Build 91) | Support for 350 MHz and CoS models. Support for MTR3000 800/900 bands models.
5.2 (Build 85) | Support for Dynamic Mixed Mode feature.
5.1 (Build 80) | Support for Microsoft® Windows® 7 Home Premium and Professional Editions. Support for 800/900 bands models.
5.0 (Build 79) | Support for MTR3000 UHF Range 1 and Range 2 model. Support for 3600 Trunking Capable Radios.
4.6 (Build 72) | Support for Analog only models.
4.5 (Build 66) | Support for H55XDH9LA1AN, H55XDH9JA1AN, H55XDC9LA1AN and H55XDC9JA1AN models.
4.0 (Build 54) | Support for Front End Filter Auto Tuning. Enhanced validation for Power Tuning values.
3.6 (Build 46) | Support for UHF Band 2 models. Fix for the error message issue when there is no audio device available.
3.5 (Build 44) | Support for Microsoft® Windows® Vista Home Premium and Business Editions.
3.0 (Build 37) | Support for additional UHF/VHF high/low power models.
2.0 (Build 31) | Support for VHF high power models.
1.0 (Build 20) | Support for the MOTOTRBO radios. Tune the transmitter and receiver of the radio. One time programming of serial number on blank boards.

### 3. Requirements

Please see the Installation Guide for more information about the system requirements for Tuner. |  |
Hardware Recommendations
· The application takes approximately 100 MB of free disk space on your PC. However, more space would be required to save archive files of your radios. Each archive file varies in size depending on the features of the radio.
· For processor speed and RAM, the recommendations given by Microsoft for the release of the operating system that you are using should be sufficient.
· A USB port.
· A CD-ROM drive.
· For best display results, set the DPI setting of your PC to the Normal size (96 DPI)

### 4. Installation, Removal

Installation
You need to have Administrator rights on the target PC in order to install the software. Proceed as follows for CD-ROM version: · Insert the CD-ROM containing the installation into the CD-ROM drive. · If the installation application doesn't start within 30 seconds, the auto-run feature for CD-ROMs in your operating system is likely disabled. Browse to your CD-ROM and run the autorun.exe program. For example, if the E:\ drive is the CD-ROM, run E:\autorun.exe.

Proceed as follows for software package version:

· Unzip the Tuner package to a directory of a local disk.

· Browse to this directory and run the setup.exe program.

If you are installing a newer version of Tuner, then remove the previous version and start the installation process again. If you are re-installing the same version of Tuner, then choose the repair option.

Note: During re-install, settings for preferences and dealer information will be reset to their default values. You will need to check these settings after the new version has been installed and make changes as necessary.

Removal
From the Start button on the task bar of your operating system, select Settings > Control Panel. Select the Add/Remove Programs option within the control panel. Select the MOTOTRBO Tuner item in the "Currently installed programs" box and click the remove button.

### 5. Legal notice

Motorola Solutions and MOTOTRBO are registered trademark of Motorola Solutions, Inc.

Microsoft® and Windows® are registered trademarks of Microsoft Inc.

### 6. Motorola Solutions Publically Available Software Legal Notices Document