# CP Series Customer Programming Software

## English 中文

### Table of Contents

1. Introduction

2. What's new in this release

3. Requirements

4. Installation, Removal

5. Driver installation

6. Legal notice

### 1. Introduction

Welcome to the CP Series Customer Programming Software (CPS) for CP1300, CP1600, CP1660, CP476, CP477, CP350, Walka Talka, CB PRO Plus, CP1200, CP246, CP1208, CP1308, CP1608 and CP1668 radios.

### 2. What's new in this release

Version R02.06 (Build 64) | Notes Support new model AZH03RDH8AC3 as AZH03RDH8AA3 is obsolete. The frequency band for CP477 has changed to 446MHz.
R02.05 (Build 63) | Support new model AZH03QDH8AD7, which has 138 channels.
R02.02 (Build 58) | Support Battery Type programmable button.
R02.01 (Build 56) | Support some new Korean and Australian models. Updated driver installation method.
R02.00 (Build 53) | Support MDC and Quik-Call II signaling system.
R01.07 (Build 46) | Support non-display model. Support for the V3, V4 radios.
R01.06 (Build 41) | Enhance CP350 radio feature.
R01.05 (Build 39) | Support CP350 and CB PRO Plus radio. Support band 350~390MHz radio.
R01.04 (Build 35) | Support new model AZH03KDH4AA4. Report feature enhancement.
R01.02 (Build 30) | Support for the UHF1 radios.
R01.01 (Build 28) | Support for the VHF radios. Add Simplified Chinese support. Add User/Dealer Mode Switch function. Add DTMF Reset Duration function.
R01.00 (Build 21) | Support for the UHF2 radios. Drag and drop support between models. Support for multiple selection configuration. For example, select several channels in the tree view and set the parameters to the same value at once. Support for custom views and undo/redo.

### 3. Requirements

Operating System
Microsoft® Windows® Vista Microsoft® Windows® 7 Microsoft® Windows® 8
Hardware Recommendations
· The application takes approximately 350 MB of free disk space on your PC. However, more space would be required to save archive files of your radios. Each archive file varies in size depending on the features of the radio.
· For processor speed and RAM, the recommendations given by Microsoft for the release of the operating system that you are using should be sufficient.
· A USB port.
· A CD-ROM drive.
· For best display results, set the DPI setting of your PC to the Normal size (96 DPI).

### 4. Installation, Removal

Installation
You need to have Administrator rights on the target PC in order to install the software. Follow the steps below for the CD-ROM version: · Insert the CD-ROM containing the installation into the CD-ROM drive. · If the installation application doesn’t start within 30 seconds, the auto-run feature for CD-ROMs for you operating system is likely disabled. Browse to your CD-ROM and run the setup.exe program. For example, if the E:\ drive is the CD-ROM, run E:\setup.exe. Follow the steps below for the software package version: · Unzip the CPS package to a directory of a local disk. · Browse to this directory and run the setup.exe program. Note: 1. During re-install, settings for preferences and dealer information will be reset to their default values. You will need to check these settings after the new version has been installed and make changes as necessary. 2. If a previous version of CPS has already been installed, you will be given the option to “Repair” or “Remove”. If you are upgrading the CPS, then remove the previous version and start the installation process again. If you are re-installing the CPS, then choose the repair option.
Removal
From the Start button on the task bar of your operating system, select Settings > Control Panel. Select the Add/Remove Programs option within the control panel. Select the CP Series Customer Programming Software item in the “Currently installed programs” box and click the remove button.

### 5. Driver installation

Windows Vista Operating System
Before connect the USB cable to computer, please make sure your Windows Update setting is “Ask me each time I connect a new device before checking for drivers” via right click “Computer” -> “Properties” -> “Advanced System Settings” -> “Hardware” -> “Windows Update Driver Settings”. Follow these steps to install the driver: 1. Connect the USB cable between the host computer and the radio. 2. Windows will open a “Found New Hardware” window. 3. Select “Locate and install driver software (recommended)”. 4. Wait while the computer searches and installs the driver.
Windows 7 Operating System
Before connect the USB cable to computer, please make sure your Windows Update setting is “Install driver software from Windows Update if it is not found on my computer” via right click “Computer” -> “Properties” -> “Advanced System Settings” -> “Hardware” -> “Device Installation Settings”. To Windows 7 (32 bit) operating system, the driver will be automatically installed and ready for use when connect the USB cable between the host computer and the radio. To Windows 7 (64 bit) operating system, follow these steps to install the driver: 1. Connect the USB cable between the host computer and the radio. The system prompts the driver was installed unsuccessfully. 2. Run Device Manager via right click My Computer -> System Properties -> Hardware -> Device Manager. 3. Select Other Devices then right click “CP2102 USB to UART Bridge Controller” and run Update Driver Software. 4. Choose Search automatically for updated driver software. 5. Wait while the computer searches and updates the driver.

### 6. Legal notice

MOTOROLA, MOTO, MOTOROLA SOLUTIONS and the Stylized M logo are trademarks or registered trademarks of Motorola Trademark Holdings, LLC and are used under license. All other trademarks are the property of their respective owners. © 2011-2014 Motorola Solutions, Inc. All rights reserved.

Microsoft® and Windows® are registered trademarks of Microsoft Inc.

### 目录

1. 简介
2. 此版本的新增功能
3. 要求
4. 安装、删除
5. 驱动安装
6. 法律声明

### 1. 简介

欢迎使用适用于 CP1300、CP1600、CP1660、CP476、CP477、CP350、Walka Talka、CB PRO Plus、CP1200、CP246、CP1208、CP1308、CP1608和CP1668 对讲机的 CP系列用户编程软件(CPS)。

### 2. 此版本的新增功能

版本 R02.06 (Build 64) | 备注 支持新型号：AZH03RDH8AC3, 旧型号AZH03RDH8AA3已被弃用。 CP477的频带改为446MHz。
R02.05 (Build 63) | 支持新型号：AZH03QDH8AD7, 信道数量为138个。
R02.02 (Build 58) | 支持配置对讲机按键为电池类型功能。
R02.01 (Build 56) | 支持一些新的韩国和澳大利亚型号的对讲机。 更新驱动安装的方法。
R02.00 (Build 53) | 支持MDC 和 Quik-Call II 信令系统。
R01.07 (Build 46) | 支持不带显示屏型号的对讲机。 支持V3,V4频段的对讲机。
R01.06 (Build 41) | 增强 CP350对讲机功能。
R01.05 (Build 39) | 支持CP350和CB PRO Plus对讲机。 支持350～390MHz 频段对讲机。
R01.04 (Build 35) | 支持新型号：AZH03KDH4AA4。 增强报表功能。
R01.02 (Build 30) | 支持 UHF1 对讲机。
R01.01 (Build 28) | 支持 VHF 对讲机。 增加简体中文支持。 增加用户/经销商模式切换功能。 增加 DTMF复位时间功能。
R01.00 (Build 21) | 支持 UHF2 对讲机。 支持在各型号之间进行拖放操作。 支持多选配置。例如，在树视图中选中几个信道，然后一次将所有信道的某些参数设置为相同的值。 支持自定义视图和撤消/重做。

### 3. 要求

操作系统
Microsoft® Windows® Vista Microsoft® Windows® 7 Microsoft® Windows® 8
硬件配置建议
· 该应用程序占用计算机上约 350 MB 可用磁盘空间。但您可能需要更多空间来保存对讲机的存档文件和设备更新软件包。具有不同功能的对讲机，其存档文件或设备更新软件包的大小也有所不同。
· Microsoft 为当前所用的操作系统版本推荐的处理器速度和 RAM 应该足以满足需求。
· 一个 USB 端口。
· 一个 CD-ROM 驱动器。
· 为获得最佳显示效果，请将计算机的 DPI 设置设为正常尺寸(96 DPI)。

### 4. 安装、删除

安装
您必须具有目标计算机的管理员权限才能安装该软件。 对于 CD-ROM 版本，按照下面的步骤操作： · 将包含安装程序的 CD-ROM 插入 CD-ROM 驱动器。 · 如果安装应用程序未在 30 秒内启动，则可能禁用了操作系统中的 CD-ROM 自动运行功能。找到 CD-ROM 并运行 setup.exe 程序。例如，如果驱动器 E:\ 为 CD-ROM，则运行 E:\setup.exe。 对于软件包版本，按照下面的步骤操作： · 将 CPS 包解压到本地磁盘的某一目录下。 · 找到此目录并运行 setup.exe 程序。 注意： 1、 在重新安装过程中，首选项和代理商信息的设置将重置为缺省值。新版本安装完成后，需要检查这些设置并进行必要的更改。 2、 如果已安装了 CPS 的先前版本，可以选择进行“修复”或“删除”。如果要进行 CPS 升级，请删除先前版本并再次进行安装。如果要重新安装 CPS，请选择“修复”选项。
删除
单击操作系统任务栏上的“开始”按钮，选择“设置”>“控制面板”。在控制面板中选择“添加/删除程序”选项。在“当前安装的程序”框中选择“CP Series Customer Programming Software”项目并单击“删除”按钮。

### 5. 驱动安装

系统在第一次检测到对讲机设备时，需要进行驱动程序的安装。请按照下面步骤进行：

Windows Vista 操作系统
在用 USB 编程线连接到电脑之前，请通过点击 “计算机” -> “属性” -> “高级系统设置” -> “硬件” -> “Windows Update 驱动设置” 确保你的 Windows Update 设置是“每次当我连接新设备在检查驱动程序之前都询问我”。 遵循下列步骤安装驱动： 1. 用 USB 编程线连接对讲机到主机。 2. Windows 将打开“找到新的硬件向导”窗口。 3. 选择“查找并安装驱动程序(建议)。 4. 等待计算机搜寻并安装驱动程序。
Windows 7 操作系统
在用 USB 编程线连接到电脑之前，请通过点击 “计算机” -> “属性” -> “高级系统设置” -> “硬件” -> “设备安装设置” 确保你的 Windows Update 设置是 “在我的计算机上找不到驱动程序软件时从 Windows Update 安装”。 对于 Windows 7(32 位)操作系统，当 USB 编程线连接对讲机到主机时，系统将会自动安装驱动程序。 对于 Windows 7(64 位)操作系统，需要按照下面步骤更新驱动程序。 1. 用 USB 编程线连接对讲机到主机。系统提示驱动程序没有被成功安装。 2. 右键单击“我的电脑” -> “系统属性” -> “硬件” -> “设备管理”，进入设备管理界面。 3. 选择“其它设备”，右键单击“CP2102 USB to UART Bridge Controller”，然后运行“更新驱动程序”。 4. 选择自动搜索来更新驱动程序。 5. 等待计算机搜索并更新驱动程序。

### 6. 法律声明

MOTOROLA，MOTO，MOTOROLA SOLUTIONS和独特的M徽标是Motorola Trademark Holdings, LLC的商标或注册商标，经授权后使用。所有其他商标均为其各自所有者的财产。©2011-2014 Motorola Solutions, Inc保留最终解释权。

Microsoft® 和 Windows® 是 Microsoft Inc. 的注册商标。