===========================================================================================
 
 SOFTWARE RELEASE NOTE

===========================================================================================

Product  : Unofficial Lab Firmware and Codeplugs for Lab FlashGrade Tool to use on commercial mobile radios.
Release  : R03.09.03 Lab
Date     : 23-May-2009
Language : English/German

============================================================================================

 Purpose Of This Release

============================================================================================

Supported features:

- Diese Lab Firmware und Codeplugs sind für CM3xx Funkgeräte bestimmt.
  Die Lab Firmware/Codeplugs sind zur Verwendung mit dem Lab Flashgrade Programm bestimmt.
  Codeplugs nur als "Phase 3 to Phase 3" programmieren!

- This Lab firmwarepack is for the CM3xx select 5 radios.
  Use it with the Lab Flashgrade tool,for the european Professional Series.
  For writing the codeplug,use only "Phase 3 to Phase 3".
 
============================================================================================

INSTRUCTIONS ABOUT UPGRADING PROCESS

============================================================================================

1.  Power on the radio. If the ignition is on, turn off all other accessories to
    ensure the quietest possible environment. Do not run the engine during this
    procedure.
2.  Connect all the items following the sequence: 
    PC com port --> Radio Interface Box(P/N RLN4008)(through P/N 3080369B72 for 9 pin 
    or P/N 3080369B71 for 25 pin) --> Programming Cable (RKN4083) --> Flash Adapter (FKN8096A) --> Radio.
3.  Start the Upgradetool from the 'Start Menu'.
4.  Select Options->Configuration to set the Flash Rate.
5.  Select Radio Access->Upgrade Radio or click "Upgrade Radio" icon on toolbar,
    and press Start Upgrade to upgrade the radio
6.  A message box will appear with instructions to put the radio in bootstrap
    mode.
	- Pull out the Programming Cable and turn off the radio.
        - Switch the flashing adapter into "Flash" mode.
          Then plug the flash cable back into the radio with the radio turned off.
        - Turn the radio on. Make sure the radio doesn't boot up like normal.
          Some of the LED's may light up but the Screen should stay blank.
          You may hear a static noise. This is "Bootstrap" Mode.


7.  After clicking Ok, upgrading should begin if properly put in bootstrap mode.
8.  When the process is complete, return the flashing switch to the 'CPS' position 
    before disconnecting the cable from the radio or powering it up.
9.  Connect another radio and repeat from step 4. Remember, the baud rate
    selection is done only the first time after starting up the program.

NOTE:
       1) Do not remove the programming cable or turn off the radio while
          upgrade is in progress.
       2) In case of failure during the upgrade, a message box will appear to
          guide the user to recover from the failure IF possible.
       3) You may not run more than one copy of the program at the same time.


===========================================================================================

===========================================================================================

 RADIO SOFTWARE RELEASE NOTE

===========================================================================================
======================
SOFTWARE RELEASE NOTE
======================

PRODUCT : ELM CM360(Marlin+)/CM340(Marlin) Radios

VERSION       : R03.09.03 Lab
DATE OF BUILD : 23-May-2009



NEW SUPPORTED MODEL NUMBERS:

Sales Model	S/Tanapa     	Description					Cp Version		
============================================================================================
M50FNF4AN2	FUC1603B	CM360:5tMobBMID-Marlin+  Mobile Mid band 	  04.00

============================================================================================


SUPPORTED MODEL NUMBERS:

Sales Model	S/Tanapa     	Description					Cp Version		
============================================================================================
M50FNC9AN2	FUC1601A	CM340:5tMobAMID-Mar Mobile Mid band	          04.01
M50FNC9AN2	FUC1601B	CM340:5tMobAMID-Mar Mobile Mid band	          04.01
M50FNF9AN2	FUC1603A	CM360:5tMobBMID-Mar+ Mobile Mid band	          04.01
M50FNF9AN2	FUC1603B	CM360:5tMobBMID-Mar+ Mobile Mid band		  04.01
M50JNC9AN2	PMUD1937A	CM340:5tMobAVHF1-Mar Mobile VHF1 band		  04.01
M50JNC9AN2	PMUD1937B	CM340:5tMobAVHF1-Mar Mobile VHF1 band		  04.01
M50JNF9AN2	PMUD1941A	CM360:5tMobBVHF1-Mar+ Mobile VHF1 band		  04.01
M50JNF9AN2	PMUD1941B	CM360:5tMobBVHF1-Mar+ Mobile VHF1 band		  04.01
M50KNC9AN2	PMUD1879A	CM340:5tMobAVHF-Mar Mobile VHF2 band		  04.01
M50KNC9AN2	PMUD1879B	CM340:5tMobAVHF-Mar Mobile VHF2 band		  04.01
M50KNF9AN2	PMUD1881A	CM360:5tMobBVHF-Mar+ Mobile VHF2 band		  04.01
M50KNF9AN2	PMUD1881B	CM360:5tMobBVHF-Mar+ Mobile VHF2 band		  04.01
M50QNC9AN2	PMUE2023A	CM340:5tMobAUHF-Mar Mobile UHF1 band		  04.01
M50QNC9AN2	PMUE2023B	CM340:5tMobAUHF-Mar Mobile UHF1 band		  04.01
M50QNF9AN2	PMUE2025A	CM360:5tMobBUHF-Mar+ Mobile UHF1 band		  04.01
M50QNF9AN2	PMUE2025B	CM360:5tMobBUHF-Mar+ Mobile UHF1 band		  04.01
M50RNC9AN2	PMUE2019A	CM340:5tMobAUHF2-Mar Mobile UHF2 band		  04.01
M50RNC9AN2	PMUE2019B	CM340:5tMobAUHF2-Mar Mobile UHF2 band		  04.01
M50RNF9AN2	PMUE2021A	CM360:5tMobBUHF2-Mar+ Mobile UHF2 band		  04.01
M50RNF9AN2	PMUE2021B	CM360:5tMobBUHF2-Mar+ Mobile UHF2 band		  04.01
M50SNC9AN2	PMUE2164A	CM340:5tMobAUHF3-Mar Mobile UHF3 band		  04.01
M50SNC9AN2	PMUE2164B	CM340:5tMobAUHF3-Mar Mobile UHF3 band		  04.01
M50SNF9AN2	PMUE2165A	CM360:5tMobBUHF3-Mar+ Mobile UHF3 band		  04.01
M50SNF9AN2	PMUE2165B	CM360:5tMobBUHF3-Mar+ Mobile UHF3 band		  04.01
M50TRC9AN2	PMUE2180A	CM340:5tMobAUHF4-Mar Mobile UHF4 band		  04.01
M50TRC9AN2	PMUE2180B	CM340:5tMobAUHF4-Mar Mobile UHF4 band		  04.01
M50TRF9AN2	PMUE2183A	CM360:5tMobBUHF4-Mar+ Mobile UHF4 band		  04.01
M50TRF9AN2	PMUE2183B	CM360:5tMobBUHF4-Mar+ Mobile UHF4 band	  	  04.01


==================
Build Environment
==================

- The Lab firmware and codeplugs are converted on a Fujitsu-Siemens Scenic D600 Series PC
  with Hexworkshop 6.01 and Tiny Hexer 1.7.1.6
