============================================================================

 SOFTWARE RELEASE NOTE

============================================================================

Product  : Unofficial Lab Firmware and Codeplugs for Lab FlashGrade Tool
Release  : R02.07.05 Lab
Date     : 12-July-2010
Language : English


============================================================================

 PURPOSE OF THE RELEASE

============================================================================
FIXES THE FOLLOWING ISSUES:
 
- This kit is for flashing GP3xx into GP6xx,and 
  upgrading/repairing,GP6xx,GP1280 radios.

HINTS:

- The ESN will set to zero after programming a codeplug.

- Supported model number:

Model Number	Tanapa		Latest	Description
		Number		Version
---------------------------------------------------------------------------
H25EDC9CK3	PMUD1511A	07.00	pop 300 band
H25EDH9CK6	PMUD1512A	07.00	pref with KEYPAD 300 band
H25EDN9CK8	PMUD1513A	07.00	prime 300 band
H25KCH4CK6	PMUD1972A	07.00	pref with kp VHF band
H25KCH6CK6	PMUD2048A	07.00	pref with kp VHF band
H25KCH6CK6	PMUD2048B	07.00	Laz ATEX EPP pref VHF
H25KDC9CK3	PMUD1484A	07.00	pop VHF band
H25KDC9CK3	PMUD1484B	07.00	pop VHF band
H25KDC9CK3	PMUD1484C	07.00	pop VHF band
H25KDH9CK6	PMUD1485A	07.00	pref with kp VHF band
H25KDH9CK6	PMUD1485B	07.00	pref with KEYPAD VHF band
H25KDH9CK6	PMUD1485C	07.00	pref with KEYPAD VHF band
H25KDN9CK8	PMUD1486A	07.00	PRIME VHF band
H25KHC4CK6	PMUD1972B	07.00	Laz ATEX EPP pref VHF
H25PDC9CK3	PMUD1538A	07.00	pop 330 band
H25PDC9CK3	PMUD1538B	07.00	pop 330 band
H25PDH9CK6	PMUD1539A	07.00	pref with kp 330 band
H25PDH9CK6	PMUD1539B	07.00	pref with KEYPAD 330 band
H25PDN9CK8	PMUD1540A	07.00	prime 330 band
H25RCH4CK6	PMUE2216B	07.00	pref with kp UHF band
H25RCH4CK6	PMUE2216C	07.00	pref with kp UHF band
H25RCH4CK6	PMUE2216E	07.00	Laz ATEX EPP pref UHF1
H25RCH6CK6	PMUE2256B	07.00	pref with kp UHF band
H25RCH6CK6	PMUE2256C	07.00	pref with kp UHF band
H25RCH6CK6	PMUE2256E	07.00	Laz ATEX EPP pref UHF1
H25RDC9CK3	PMUE1436A	07.00	pop UHF band
H25RDC9CK3	PMUE1436B	07.00	pop UHF band
H25RDC9CK3	PMUE1436C	07.00	pop UHF band
H25RDC9CK3	PMUE1436D	07.00	Laz EPP Portable pop UHF band
H25RDH9CK6	PMUE1437A	07.00	pref with kp UHF band
H25RDH9CK6	PMUE1437B	07.00	pref with KEYPAD UHF band
H25RDH9CK6	PMUE1437C	07.00	pref with KEYPAD UHF band
H25RDH9CK6	PMUE1437D	07.00	Laz EPP Portable pref with Keypad UHF band
H25RDN9CK8	PMUE1439A	07.00	prime UHF band
H25SDC9CK3	PMUE1481A	07.00	pop UHF2 band
H25SDC9CK3	PMUE1481B	07.00	pop UHF2 band
H25SDC9CK3	PMUE1481C	07.00	pop UHF2 band
H25SDC9CK3	PMUE1481D	07.00	Laz EPP Portable pop UHF2 band
H25SDH9CK6	PMUE1482A	07.00	pref with kp UHF2 band
H25SDH9CK6	PMUE1482B	07.00	pref with KEYPAD UHF2 band
H25SDH9CK6	PMUE1482C	07.00	pref with KEYPAD UHF2 band
H25SDH9CK6	PMUE1482D	07.00	Laz EPP Portable pref with Keypad UHF2 band
H25SDN9CK8	PMUE1486A	07.00	prime UHF2 band
H38RDC9CK3	PMUE1961A	07.00	pop UHF band
H38RDC9CK3	PMUE1961B	07.00	pop UHF band
H38RDC9CK3	PMUE1961C	07.00	Min EPP Portable pop UHF band
H38RDC9CK3	PMUE2794A	07.00	pop UHF band
H38RDC9CK3	PMUE2794B	07.00	Min IP67 pop UHF1
H38RDF9CK5	PMUE2780A	07.00	pref without kp UHF band
H38RDF9CK5	PMUE2780B	07.00	Min IP67 pref LK UHF1
H38RDH9CK6	PMUE1962A	07.00	pref with kp UHF band
H38RDH9CK6	PMUE1962B	07.00	pref with kp UHF band
H38RDH9CK6	PMUE1962C	07.00	Min EPP Portable pref with Keypad UHF band
H38RDH9CK6	PMUE2795A	07.00	pref with kp UHF band
H38RDH9CK6	PMUE2795B	07.00	Min IP67 pref FK UHF1


============================================================================
For the usage of this software the following radio accessories are required:

    - Flash adapter, P/N HLN9742A or B
    and (i)
    - Radio Interface Box, P/N RLN4008
      with battery or power supply
    - RIB to PC cable, P/N 3080369B72 (9pin) or 3080369B71 (25pin)
    - Programming/test cable, P/N RKN4074 (GP3xx, GP6xx, GP12xx)
    - Programming/test cable, P/N MDJMKN4123 (GP344, GP388)
    or (ii)
    -  RIBless programming cable, P/N RKN4075 (GP3xx, GP6xx, GP12xx)

    By using equipment (i) the Flash adapter has to be connected between the 
    Radio Interface Box and the Programming/test cable.Maximum baud rate for 
    this equipment is 19,200 Bd.

    By using equipment (ii) the Flash adapter has to be connected between the 
    PC and the RIBless programming cable.

    For Flash Adapter HLN9742A, "Flash mode on" means switch position "ON".

    For Flash Adapter HLN9742B, "Flash mode on" means switch position "A", 
    position "B" is not used for portable flashing.


============================================================================

 RADIO SOFTWARE RELEASE NOTE

============================================================================
======================
SOFTWARE RELEASE NOTE
======================

PRODUCT : WARIS MPT GP640/GP680/GP1280/Minnow GP688/Minnow GP644/ATEX Portable Radio
          Lab Firmware

VERSION       : R02.07.05 Lab
DATE OF BUILD : 12-July-2010


