====================================================================================

 SOFTWARE RELEASE NOTE

====================================================================================

Product          	 : Professional Radio Firmware Kit
Release 	       	 : R05.10.02
Date                     : 12-Jul-2011
Language                 : English
Supporting OS            : Win 95,Win98,Win2000,WinNT,WinXP

NOTICE: The CPS PROGRAMMING DATA WILL BE LOST AFTER UPGRADING. PLEASE SAVE YOUR EXISTING CODEPLUG 
TO AN ARCHIVE FILE. It is recommended to save an archive of the radio's codeplug using CPS before 
the update process. After upgrading, this archive can be used to recover the CPS programming data 
of the radio.

====================================================================================

 Purpose of this release

====================================================================================

Supported features:

- Up-version a radio to software version R05.10.02 from previous released versions. 


Supported Software versions:

- Only official radio software release version and bands.
  In this version:
  R02.00.00, R02.00.01, R02.00.02, R03.00.00, R03.00.01
  R04.00.00, R04.01.00, R04.01.14, R04.01.15, R04.01.18
  R04.02.01, R04.02.08, R05.00.00, R05.01.00, R05.02.00
  R05.02.03, R05.03.00, R05.04.00, R05.04.01, R05.05.02
  R05.05.03, R05.05.04, R05.05.05, R05.05.10, R05.05.12
  R05.05.15, R05.05.17, R05.05.19, B05.05.20, R05.05.22
  R05.06.04, R05.07.02, R05.08.01, R05.08.02, R05.08.05
  R05.09.01, R05.10.01, R05.10.02



- Supported model number:

Model Number    	Tanapa Number     Latest Version       Description
--------------------------------------------------------------------------------
M25BKA9AA0A             IMUB6000A         11.00                F7Conv Data lb1 sd com   
M25BKC9AA1A             IMUB6000A         11.00                F7Conv Plain lb1 sd com   
M25BKD9AA2A             IMUB6000A         11.00                F7Conv Pop lb1 sd com   
M25BKF9AA5A             IMUB6000A         11.00                F7Conv Pref lb1 sd com   
M25CKA9AA0A             IMUB6001A         11.00                F7Conv Data lb2 sd com   
M25CKC9AA1A             IMUB6001A         11.00                F7Conv Plain lb2 sd com   
M25CKD9AA2A             IMUB6001A         11.00                F7Conv Pop lb2 sd com   
M25CKF9AA5A             IMUB6001A         11.00                F7Conv Pref lb2 sd com   
M25CKA9AA0A             IMUB6001C         11.00                F7NO DISPLAY LOW2    
M25CKC9AA1A             IMUB6001C         11.00                F7NO DISPLAY LOW2    
M25CKD9AA2A             IMUB6001C         11.00                F71 LINE DISPLAY LOW2    
M25CKF9AA5A             IMUB6001C         11.00                F71 LINE DISPLAY LOW2    
M25DKA9AA0A             IMUB6002A         11.00                F7Conv Data lb3 sd com   
M25DKC9AA1A             IMUB6002A         11.00                F7Conv Plain lb3 sd com   
M25DKD9AA2A             IMUB6002A         11.00                F7Conv Pop lb3 sd com   
M25DKF9AA5A             IMUB6002A         11.00                F7Conv Pref lb3 sd com   
M25DKA9AA0A             IMUB6002C         11.00                F7NO DISPLAY LOW3    
M25DKC9AA1A             IMUB6002C         11.00                F7NO DISPLAY LOW3    
M25DKD9AA2A             IMUB6002C         11.00                F71 LINE DISPLAY LOW3    
M25DKF9AA5A             IMUB6002C         11.00                F71 LINE DISPLAY LOW3    
M25KHA9AA0A             IMUD6010B         11.00                F7Conv Data VB1 lo bnc EPP com   
M25KHC9AA1A             IMUD6010B         11.00                F7Conv Plain VB1 lo bnc EPP com   
M25KHD9AA2A             IMUD6010B         11.00                F7Conv Pop VB1 lo bnc EPP com   
M25KHF4AA5              IMUD6010B         11.00                F7Conv Pref VB1 lo bnc 12.5k EPP com   
M25KHF9AA5A             IMUD6010B         11.00                F7Conv Pref VB1 lo bnc EPP com   
M25KKC9AA1A             IMUD6011C         11.00                F7Conv Plain VB1 hi bnc EPP com   
M25KKF4AA5A             IMUD6011C         11.00                F7Conv Pref VB1 hi bnc EPP com 12.5K   
M25KKF9AA5A             IMUD6011C         11.00                F7Conv Pref VB1 hi bnc EPP com   
M25KHA9AA0A             IMUD6014A         11.00                F7Conv Data VB1 lo com   
M25KHC9AA1A             IMUD6014A         11.00                F7Conv Plain VB1 lo com   
M25KHD9AA2A             IMUD6014A         11.00                F7Conv Pop VB1 lo com   
M25KHF9AA5A             IMUD6014A         11.00                F7Conv Pref VB1 lo com   
M25KHA9AA0A             IMUD6014B         11.00                F7Conv Data VB1 lo EPP com   
M25KHC9AA1A             IMUD6014B         11.00                F7Conv Plain VB1 lo EPP com   
M25KHD9AA2A             IMUD6014B         11.00                F7Conv Pop VB1 lo EPP com   
M25KHF9AA5A             IMUD6014B         11.00                F7Conv Pref VB1 lo EPP com   
M25KKA9AA0A             IMUD6015A         11.00                F7Conv Data VB1 hi com   
M25KKC9AA1A             IMUD6015A         11.00                F7Conv Plain VB1 hi com   
M25KKD9AA2A             IMUD6015A         11.00                F7Conv Pop VB1 hi com   
M25KKF9AA5A             IMUD6015A         11.00                F7Conv Pref VB1 hi com   
M25KKC9AA1A             IMUD6015B         11.00                F7Conv Plain VB1 hi ldmos com   
M25KKD9AA2A             IMUD6015B         11.00                F7Conv Pop VB1 hi ldmos com   
M25KKF9AA5A             IMUD6015B         11.00                F7Conv Pref VB1 hi ldmos com   
M25KKC9AA1A             IMUD6015C         11.00                F7Conv Plain VB1 hi ldmos EPP com   
M25KKD9AA2A             IMUD6015C         11.00                F7Conv Pop VB1 hi ldmos EPP com   
M25KKF9AA5A             IMUD6015C         11.00                F7Conv Pref VB1 hi ldmos EPP    
M25KHN9AA8A             IMUD6023A         06.00                F7Conv Prime VB1 lo com   
M25KHN9AA8A             IMUD6023B         06.00                F7Conv Prime VB1 lo EPP com   
M25KKN9AA8A             IMUD6025C         06.00                F7Conv Prime VB1 hi ldmos EPP com   
M25KKN9AA8A             IMUD6026A         06.00                F7Conv Prime VB1 hi com   
M25KKN9AA8A             IMUD6026B         06.00                F7Conv Prime VB1 hi ldmos com   
M25KKN9AA8A             IMUD6026C         06.00                F7Conv Prime VB1 hi ldmos EPP com   
M25RKC9AA1A             IMUE6012C         11.00                F7Conv Plain UB1 hi bnc EPP com   
M25RKD9AA2A             IMUE6012C         11.00                F7Conv Pop UB1 hi bnc EPP com   
M25RKF4AA5A             IMUE6012C         11.00                F7Conv Pref UB1 hi bnc EPP com 12.5K   
M25RKF9AA5A             IMUE6012C         11.00                F7Conv Pref UB1 hi bnc EPP com   
M25SKD9AA2A             IMUE6019B         11.00                F7Conv Pop UB2 hi b ldmos com   
M25SKF9AA5A             IMUE6019B         11.00                F7Conv Pref UB2 hi b ldmos com   
M25RHA9AA0A             IMUE6021B         11.00                F7Conv Data UB1 lo bnc EPP com   
M25RHC9AA1A             IMUE6021B         11.00                F7Conv Plain UB1 lo bnc EPP com   
M25RHD9AA2A             IMUE6021B         11.00                F7Conv Pop UB1 lo bnc EPP com   
M25RHF4AA5              IMUE6021B         11.00                F7Conv Pref UB1 lo bnc 12.5k EPP com   
M25RHF9AA5A             IMUE6021B         11.00                F7Conv Pref UB1 lo bnc EPP com   
M25SHA9AA0A             IMUE6022A         11.00                F7Conv Data UB2 lo b ldmos com   
M25SHC9AA1A             IMUE6022A         11.00                F7Conv Plain UB2 lo b ldmos com   
M25SHD9AA2A             IMUE6022A         11.00                F7Conv Pop UB2 lo b ldmos com   
M25SHF9AA5A             IMUE6022A         11.00                F7Conv Pref UB2 lo b ldmos com   
M25RKA9AA0A             IMUE6024A         11.00                F7Conv Data UB1 hi a com   
M25RKC9AA1A             IMUE6024A         11.00                F7Conv Plain UB1 hi a com   
M25RKD9AA2A             IMUE6024A         11.00                F7Conv Pop UB1 hi a com   
M25RKF9AA5A             IMUE6024A         11.00                F7Conv Pref UB1 hi a com   
M25RKF9DU5A             IMUE6024A         11.00                F7LS Trunking Pref UB1 hi a com   
M25RKA9AA0A             IMUE6024B         11.00                F7Conv Data UB1 hi b com   
M25RKC9AA1A             IMUE6024B         11.00                F7Conv Plain UB1 hi b com   
M25RKD9AA2A             IMUE6024B         11.00                F7Conv Pop UB1 hi b com   
M25RKF9AA5A             IMUE6024B         11.00                F7Conv Pref UB1 hi b com   
M25RKF9DU5A             IMUE6024B         11.00                F7LS Trunking Pref UB1 hi b com   
M25RKA9AA0A             IMUE6024C         11.00                F7Conv Data UB1 hi ldmos com   
M25RKC9AA1A             IMUE6024C         11.00                F7Conv Plain UB1 hi ldmos com   
M25RKD9AA2A             IMUE6024C         11.00                F7Conv Pop UB1 hi ldmos com   
M25RKF9AA5A             IMUE6024C         11.00                F7Conv Pref UB1 hi ldmos com   
M25RKF9DU5A             IMUE6024C         11.00                F7LS Trunking Pref UB1 hi ldmos com   
M25RKA9AA0A             IMUE6024D         11.00                F7Conv Data UB1 hi ldmos EPP com   
M25RKC9AA1A             IMUE6024D         11.00                F7Conv Plain UB1 hi ldmos EPP com   
M25RKD9AA2A             IMUE6024D         11.00                F7Conv Pop UB1 hi ldmos EPP com   
M25RKF9AA5A             IMUE6024D         11.00                F7Conv Pref UB1 hi ldmos EPP com   
M25SKA9AA0A             IMUE6025A         11.00                F7Conv Data UB2 hi com   
M25SKC9AA1A             IMUE6025A         11.00                F7Conv Plain UB2 hi com   
M25SKD9AA2A             IMUE6025A         11.00                F7Conv Pop UB2 hi com   
M25SKF9AA5A             IMUE6025A         11.00                F7Conv Pref UB2 hi com   
M25SKF9DU5A             IMUE6025A         11.00                F7LS Trunking Pref UB2 hi com   
M25SKA9AA0A             IMUE6025B         11.00                F7Conv Data UB2 hi com   
M25SKC9AA1A             IMUE6025B         11.00                F7Conv Plain UB2 hi com   
M25SKD9AA2A             IMUE6025B         11.00                F7Conv Pop UB2 hi com   
M25SKF9AA5A             IMUE6025B         11.00                F7Conv Pref UB2 hi com   
M25SKF9DU5A             IMUE6025B         11.00                F7LS Trunking Pref UB2 hi com   
M25SKA9AA0A             IMUE6025C         11.00                F7Conv Data UB2 hi com   
M25SKC9AA1A             IMUE6025C         11.00                F7Conv Plain UB2 hi com   
M25SKD9AA2A             IMUE6025C         11.00                F7Conv Pop UB2 hi com   
M25SKF9AA5A             IMUE6025C         11.00                F7Conv Pref UB2 hi com   
M25SKF9DU5A             IMUE6025C         11.00                F7LS Trunking Pref UB2 hi com   
M25SKC9AA1A             IMUE6025D         11.00                F7Conv Plain UB2 hi ldmos com   
M25SKD9AA2A             IMUE6025D         11.00                F7Conv Pop UB2 hi ldmos com   
M25SKF4AA5A             IMUE6025D         11.00                F7Conv Pref UB2 hi bnc 12.5K com    
M25SKF9AA5A             IMUE6025D         11.00                F7Conv Pref UB2 hi ldmos com   
M25SKF9DU5A             IMUE6025D         11.00                F7LS Trunking Pref UB2 hi ldmos com   
M25RHA9AA0A             IMUE6027A         11.00                F7Conv Data UB1 lo ldmos com   
M25RHC9AA1A             IMUE6027A         11.00                F7Conv Plain UB1 lo ldmos com   
M25RHD9AA2A             IMUE6027A         11.00                F7Conv Pop UB1 lo ldmos com   
M25RHF9AA5A             IMUE6027A         11.00                F7Conv Pref UB1 lo ldmos com   
M25RHF9DU5A             IMUE6027A         11.00                F7LS Trunking Pref UB1 lo ldmos com   
M25RHA9AA0A             IMUE6027B         11.00                F7Conv Data UB1 lo ldmos EPP com   
M25RHC9AA1A             IMUE6027B         11.00                F7Conv Plain UB1 lo ldmos EPP com   
M25RHD9AA2A             IMUE6027B         11.00                F7Conv Pop UB1 lo ldmos EPP com   
M25RHF9AA5A             IMUE6027B         11.00                F7Conv Pref UB1 lo ldmos EPP com   
M25SHA9AA0A             IMUE6028A         11.00                F7Conv Data UB2 lo com   
M25SHC9AA1A             IMUE6028A         11.00                F7Conv Plain UB2 lo com   
M25SHD9AA2A             IMUE6028A         11.00                F7Conv Pop UB2 lo com   
M25SHF9AA5A             IMUE6028A         11.00                F7Conv Pref UB2 lo com   
M25SHF9DU5A             IMUE6028A         11.00                F7LS Trunking Pref UB2 lo com   
M25SHA9AA0A             IMUE6028B         11.00                F7Conv Data UB2 lo ldmos com   
M25SHC9AA1A             IMUE6028B         11.00                F7Conv Plain UB2 lo ldmos com   
M25SHD9AA2A             IMUE6028B         11.00                F7Conv Pop UB2 lo ldmos com   
M25SHF4AA5              IMUE6028B         11.00                F7LS Trunking Pref UB2 lo ldmos 12.5k com   
M25SHF9AA5A             IMUE6028B         11.00                F7Conv Pref UB2 lo ldmos com   
M25SHF9DU5A             IMUE6028B         11.00                F7LS Trunking Pref UB2 lo ldmos com   
M25RHN9AA8A             IMUE6039A         06.00                F7Conv Prime UB1 lo ldmos com   
M25RHN9AA8A             IMUE6039B         06.00                F7Conv Prime UB1 lo ldmos EPP com   
M25RKN9AA8A             IMUE6040C         06.00                F7Conv Prime UB1 hi ldmos EPP com   
M25SKN9AA8A             IMUE6041B         06.00                F7Conv Prime UB2 hi ldmos com    
M25SHN9AA8A             IMUE6043A         06.00                F7Conv Prime UB2 lo ldmos com   
M25RKN9AA8A             IMUE6044A         06.00                F7Conv Prime UB1 hi a com   
M25RKN9AA8A             IMUE6044B         06.00                F7Conv Prime UB1 hi b com   
M25RKN9AA8A             IMUE6044C         06.00                F7Conv Prime UB1 hi ldmos com   
M25RKN9AA8A             IMUE6044D         06.00                F7Conv Prime UB1 hi ldmos EPP com   
M25SKN9AA8A             IMUE6045A         06.00                F7Conv Prime UB2 hi a com   
M25SKN9AA8A             IMUE6045B         06.00                F7Conv Prime UB2 hi b com   
M25SKN9AA8A             IMUE6045C         06.00                F7Conv Prime UB2 hi ldmos com   
M25MHF4DP5A             PMUD1765A         11.00                F7PPT Conv MDC LS Trunking Pref 220 lo ldmos com   
M25MHF4DP5A             PMUD1765B         11.00                F7PPT Conv MDC LS Trunking Pref 220 lo b ldmos com   
M25KHF9DU6A             PMUD1810A         11.00                F7Conv MDC LS Trunking Pref VB1 lo com   
M25KKF9DU6A             PMUD1811A         11.00                F7Conv MDC LS Trunking Pref VB1 hi ldmos com   
M25KKF9DU6A             PMUD1811B         11.00                F7Conv MDC LS Trunking Pref VB1 hi ldmos com    
M25KHF9DU5A             PMUD1850A         11.00                F7LS Trunking Pref VB1 lo com   
M25KKF9DU5A             PMUD1851A         11.00                F7LS Trunking Pref VB1 hi ldmos com   
M25KHF9DP5AN            PMUD2063A         11.00                F7PPT Pref LS Trunking VHF B1 (25W 16CH)   
M25KHF9DP5AN            PMUD2063B         11.00                F7PPT Pref LS Trunking VHF B1 (25W 16CH)   
M25KHF9DP5AN            PMUD2063C         11.00                F7ST CDM1550LS+ 136-174M 25W 16CH   
M25KHF9DP6AN            PMUD2064A         11.00                F7PPT Conv MDC Pref LS Trunking VHF B1 (45W 16CH)   
M25KHF9DP6AN            PMUD2064B         11.00                F7PPT Conv MDC Pref LS Trunking VHF B1 (45W 16CH)   
M25KHF9DP6AN            PMUD2064C         11.00                F7ST CDM1550LS+ 136-174 25W 160CH   
M25KKF9DP5AN            PMUD2065A         11.00                F7PPT Pref LS Trunking VHF B1(45W 16CH)   
M25KKF9DP5AN            PMUD2065B         11.00                F7PPT Pref LS Trunking VHF B1(45W 16CH)   
M25KKF9DP5AN            PMUD2065C         11.00                F7ST CDM1550LS+136-174 45W 16C   
M25KKF9DP6AN            PMUD2066A         11.00                F7PPT Conv MDC Pref LS Trunking VHF B1 (45W 16CH)   
M25KKF9DP6AN            PMUD2066B         11.00                F7PPT Conv MDC Pref LS Trunking VHF B1 (45W 16CH)   
M25KKF9DP6AN            PMUD2066C         11.00                F7ST CDM1550LS+ 137-174M 45W 160CH   
M25KHD9AA2A             PMUD2217A         11.00                F7Conv LS Trunking Pop VB1 lo   
M25KHF9AA5A             PMUD2217A         11.00                F7Conv LS Trunking Pref VB1 lo   
M25KHD9AA2A             PMUD2217B         11.00                F7Conv LS Trunking Pop VB1 lo EPP   
M25KHF9AA5A             PMUD2217B         11.00                F7Conv LS Trunking Pref VB1 lo EPP   
M25KKD9AA2A             PMUD2218A         11.00                F7Conv LS Trunking Pop VB1 hi   
M25KKF9AA5A             PMUD2218A         11.00                F7Conv LS Trunking Pref VB1 hi   
M25KKD9AA2A             PMUD2218B         11.00                F7Conv LS Trunking Pop VB1 hi ldmos   
M25KKF9AA5A             PMUD2218B         11.00                F7Conv LS Trunking Pref VB1 hi ldmos   
M25KKD9AA2A             PMUD2218C         11.00                F7Conv LS Trunking Pop VB1 hi EPP   
M25KKF9AA5A             PMUD2218C         11.00                F7Conv LS Trunking Pref VB1 hi EPP   
M25MHF4AA5A             PMUD2599A         11.00                F71 LINE DISPLAY 220-232MHz    
M25RHF9DP5A             PMUE1754A         11.00                F7PPT LS Trunking Pref UB1 lo ldmos com   
M25RHF9DP5A             PMUE1754B         11.00                F7PPT LS Trunking Pref UB1 lo ldmos com   
M25RHF9DP5A             PMUE1754C         11.00                F7PPT LS Trunking Pref UB1 lo ldmos com   
M25RHF9DP5A             PMUE1754D         11.00                F7WM PASSPORT UHF R1 LP   
M25SHF9DP5A             PMUE1755A         11.00                F7PPT LS Trunking Pref UB2 lo ldmos com   
M25SHF9DP5A             PMUE1755B         11.00                F7PPT LS Trunking Pref UB2 lo ldmos com   
M25RKF9DP5A             PMUE1756A         11.00                F7PPT LS Trunking Pref UB1 hi com   
M25RKF9DP5A             PMUE1756B         11.00                F7PPT LS Trunking Pref UB1 hi ldmos com   
M25RKF9DP5A             PMUE1756C         11.00                F7PPT LS Trunking Pref UB1 hi ldmos com   
M25RKF9DP5A             PMUE1756D         11.00                F7PPT LS Trunking Pref UB1 hi ldmos com   
M25RKF9DP5A             PMUE1756E         11.00                F7WM PASSPORT UHF R1 HP   
M25SKF9DP5A             PMUE1757A         11.00                F7PPT LS Trunking Pref UB2 hi com   
M25SKF9DP5A             PMUE1757B         11.00                F7PPT LS Trunking Pref UB2 hi ldmos com   
M25SKF9DP5A             PMUE1757C         11.00                F7PPT LS Trunking Pref UB2 hi ldmos com   
M25SKC9PW1A             PMUE1874A         11.00                F7Conv Plain UB2 1 5ppm hi ldmos com   
M25SKD9PW2A             PMUE1874A         11.00                F7Conv Pop UB2 1 5ppm hi ldmos com   
M25SKF9PW5A             PMUE1874A         11.00                F7Conv Pref UB2 1 5ppm hi ldmos com   
M25RHF9DP6AN            PMUE1939A         11.00                F7PPT Conv MDC LS Trunking Pref UB1 lo ldmos com   
M25RHF9DP6AN            PMUE1939B         11.00                F7PPT Conv MDC LS Trunking Pref UB1 lo ldmos com   
M25RHF9DP6AN            PMUE1939C         11.00                F7PPT Conv MDC LS Trunking Pref UB1 lo ldmos com   
M25RHF9DP6AN            PMUE1939D         11.00                F7WM S/T LS+ UHF R1 LP MDC/CONV   
M25RKF9DP6AN            PMUE1940A         11.00                F7PPT Conv MDC LS Trunking Pref UB1 hi com   
M25RKF9DP6AN            PMUE1940B         11.00                F7PPT Conv MDC LS Trunking Pref UB1 hi ldmos com   
M25RKF9DP6AN            PMUE1940C         11.00                F7PPT Conv MDC LS Trunking Pref UB1 hi ldmos com   
M25RKF9DP6AN            PMUE1940D         11.00                F7PPT Conv MDC LS Trunking Pref UB1 hi ldmos com   
M25RKF9DP6AN            PMUE1940E         11.00                F7WM S/T LS+ UHF R1 HP MDC/CONV   
M25SHF9DP6AN            PMUE1941A         11.00                F7PPT Conv MDC LS Trunking Pref UB2 lo ldmos com   
M25SHF9DP6AN            PMUE1941B         11.00                F7PPT Conv MDC LS Trunking Pref UB2 lo ldmos com   
M25SKF9DP6AN            PMUE1942A         11.00                F7PPT Conv MDC LS Trunking Pref UB2 hi com   
M25SKF9DP6AN            PMUE1942B         11.00                F7PPT Conv MDC LS Trunking Pref UB2 hi ldmos com   
M25SKF9DP6AN            PMUE1942C         11.00                F7PPT Conv MDC LS Trunking Pref UB2 hi ldmos com   
M25SHD6AA2A             PMUE2305A         11.00                F7Conv Pop UB2 lo fixed2 ldmos com   
M25SHD6AA2A             PMUE2306A         11.00                F7Conv Pop UB2 lo fixed1 ldmos com   
M25RHD9AA2A             PMUE2724A         11.00                F7Conv LS Trunking Pop UB1 lo ldmos   
M25RHF9AA5A             PMUE2724A         11.00                F7Conv LS Trunking Pref UB1 lo ldmos   
M25RHD9AA2A             PMUE2724B         11.00                F7Conv LS Trunking Pop UB1 lo EPP   
M25RHF9AA5A             PMUE2724B         11.00                F7Conv LS Trunking Pref UB1 lo EPP   
M25RKD9AA2A             PMUE2725A         11.00                F7Conv LS Trunking Pop UB1 hi   
M25RKF9AA5A             PMUE2725A         11.00                F7Conv LS Trunking Pref UB1 hi   
M25RKD9AA2A             PMUE2725B         11.00                F7Conv LS Trunking Pop UB1 hi b   
M25RKF9AA5A             PMUE2725B         11.00                F7Conv LS Trunking Pref UB1 hi b   
M25RKD9AA2A             PMUE2725C         11.00                F7Conv LS Trunking Pop UB1 hi ldmos   
M25RKF9AA5A             PMUE2725C         11.00                F7Conv LS Trunking Pref UB1 hi ldmos   
M25RKD9AA2A             PMUE2725D         11.00                F7Conv LS Trunking Pop UB1 hi EPP   
M25RKF9AA5A             PMUE2725D         11.00                F7Conv LS Trunking Pref UB1 hi EPP   
M25SHD9AA2A             PMUE2726A         11.00                F7Conv LS Trunking Pop UB2 lo   
M25SHF9AA5A             PMUE2726A         11.00                F7Conv LS Trunking Pref UB2 lo   
M25SHD9AA2A             PMUE2726B         11.00                F7Conv LS Trunking Pop UB2 lo ldmos   
M25SHF9AA5A             PMUE2726B         11.00                F7Conv LS Trunking Pref UB2 lo ldmos   
M25SKD9AA2A             PMUE2727A         11.00                F7Conv LS Trunking Pop UB2 hi   
M25SKF9AA5A             PMUE2727A         11.00                F7Conv LS Trunking Pref UB2 hi   
M25SKD9AA2A             PMUE2727B         11.00                F7Conv LS Trunking Pop UB2 hi b   
M25SKF9AA5A             PMUE2727B         11.00                F7Conv LS Trunking Pref UB2 hi b   
M25SKD9AA2A             PMUE2727C         11.00                F7Conv LS Trunking Pop UB2 hi c   
M25SKF9AA5A             PMUE2727C         11.00                F7Conv LS Trunking Pref UB2 hi c   
M25SKD9AA2A             PMUE2727D         11.00                F7Conv LS Trunking Pop UB2 hi ldmos   
M25SKF9AA5A             PMUE2727D         11.00                F7Conv LS Trunking Pref UB2 hi ldmos   
M255HF4DP5A             PMUF1111A         11.00                F7PPT Conv MDC LS Trunking Pref 700 lo ldmos com   
M255HF4DP5A             PMUF1111B         11.00                F7PPT Conv MDC LS Trunking Pref 700 lo b ldmos com   

====================================================================================

WARNING

====================================================================================

PLEASE READ:  WARNING'S FOR ALL RADIO TYPES 

PLEASE SAVE YOUR EXISTING CODEPLUG AS AN ARCHIVE FILE. The codeplug programming 
information may be lost after the update process therefore, it is recommended to 
read the radio using the CPS, and save an archive of the radio's codeplug before 
starting the update process. After the update, this archive can now be used to 
recover the codeplug programming information by programming the archive back into 
the radio.

Ensure the radio updating process is not interrupted. Interruption will cause the 
radio not to operate anymore and attempting to update the radio again will NOT be 
successful.

Do NOT create a shortcut of the program (e.g. on your desktop), the program might 
not be able to find the data files in that case!

Do not remove the programming cable or turn off the radio while the update is in progress.

In case of failure during the updating, a message box will appear to guide the user 
to recover from the failure, if possible.

The flashing rate can be changed only by restarting the program.

You may not run more than one copy of the program at the same time.

Baud rate 115k can only be supported by certain Radio Interface Boxes (RIB). 
Use 19k baud rate when using a RIB. RKN4075A RIBless cable supports 115k baud.


===========================================================

 How to install and run this software

===========================================================

Installation of the software can be completed by double clicking 
the setup file "UpgradeKit_Conv_Mobile_R05.10.02.exe",and can be 
started through Programs Menu.

REQUIRED EQUIPMENT

For the usage of this software the following radio accessories
are required:

- Flash adapter, P/N HLN9742, RIB programming cable, P/N AARKN4083A
  and RIBless programming cable, P/N AARKN4081B

  the Flash adapter has to be connected between the PC and the RIBless programming cable.

  For Flash Adapter HLN9742B, "Flash mode on" means switch to
  i) Position "B", For RIBless programming cable, P/N AARKN4081B 
  ii) Position "A", For RIB programming cable, P/N AARKN4083A

==================================================================================

The following instructions detail the operations of the Firmware Kit:

(Note: These instructions must be followed in the exact order to work properly):

1.  Power on the radio. If the ignition is on, turn off all other accessories to
    ensure the quietest possible environment. Do not run the engine during this
    procedure.

2.  (i) For Ribless cable
    --------------------	
    Connect the AARKN4081B programming cable to the microphone jack of the radio.
    The Programming cable is connected to the adapter, and the adapter is
    connected to the computer serial port (9 pin) through the 25 to 9 pin Converter. 
    Note: the Converter is not requiring if serial port is 25 pin.

    (ii) For Rib Cable
    ----------------
    Connect the AARKN4083A programming cable to the rear connector of the radio.
    The Programming cable is connected to RLN4008E Radio Interface Box and it connected
    to the computer serial port by RIB to PC cable, P/N 3080369B72 (9pin) or 3080369B71 (25pin) 
    Note: The Converter is not requiring if serial port is 25 pin.
        : Maximum baud rate for this equipment is 19,200 Bd.

3.  If you using a laptop ensure that "Transmit Buffer" in the Advanced Port Settings
    window is not positioned at the highest setting.  See troubleshooting section
    "Adjusting Transmit Buffer" below for details.

4.  Make sure that the switch in the HLN9742B adapter is in the OFF position.

5.  Start the Firmware Kit by going to Programs-> Motorola-> Professional Series Radio Upgrade Kit
    -> Mobile Upgrade Kit R05.10.02-> Mobile Upgrade Kit R05.10.02.

6.  Once the upgrade screen appears, press the PROGRAM button.

7.  For the first attempt of upgrade after the tool is launched, the flash baud
    rate selection dialog will appear. Select a baud rate and press OK button.

8.  A message box will appear with instructions to put the radio in bootstrap
    mode.
    Turn the radio to bootstrap mode by follow the following steps.
	- Move the flash adapter switch (HLN9742B) to the "B" position for RIBless cable or "A" position for RIB cable.
	- Press the ON/OFF button on the radio 2 times, waiting a minimum of 1 second between presses. 
	  This process puts the radio into bootstrap mode.

	  NOTE: Please be aware, when pressing the ON/OFF button,you will not recieve any response from the radio.
	  This is normal operation for putting the radio into a mode for flasing.
	  Without the 1 second wait time, the radio will not properly go into bootstrap mode.

9.  After clicking Ok, upgrading should begin if properly put in bootstrap mode.

10. If the radio is not properly put in bootstrap mode, a message box will appear with instructions to set the
    radio in bootstrap mode again.
	- Flashing operation could not be started.
	- The radio may not be in bootstrap mode.
	- Caution: Carefully follow these instructions to restore the radio.
	  Do not press "OK" until after steps 1 thru 3 have been performed.
		1. Switch the flash adapter back to OFF position.
		2. Disconnect and reconnect the radio's power supply.
		3. If the radio is off, turn it back on by pressing the ON/OFF button.
		4. Press "OK" and try to "Program" again.

11. When the process is complete, return the flashing switch to the OFF position
    before disconnecting the cable from the radio or powering it up.  The radio
    will power off when the cable is removed.

12. Connect another radio and repeat from step 5. Remember, the baud rate
    selection is done only the first time after starting up the program.

13. After upgrading all radios, remove the flashing adapter.


============================================================================

TROUBLESHOOTING

============================================================================

If Firmware Kit will not start

1. Make sure this is an original version of the kit and not copied off another
   computer
2. Make sure another copy is not running on your computer.

If an error is returned when you select program, check the following:

1.  On the Comm setting menu, make sure that the port selected is the one to
    which the radio is connected.
2.  Make sure the radio is on and properly connected to the computer.
3.  Make sure the HLN9742B adapter is in the OFF position.

If an error is returned immediately after the radio is put in bootstrap and Ok
is clicked put the adapter in the OFF position, put the radio off, on and try
again.

Adjusting Transmit Buffer:
1.  Press Start button.
2.  Select Setting and click on Control Panel.
3.  Double click on System.
4.  Select the Device Manager tab and double click on the Communication Port (COM1).
5.  Select the Port Settings tab and click on the Advanced button.
6.  Adjust the Transmit Buffer to one step lower than the highest.

============================================================================

WARNING

============================================================================

Ensure radio flashing is not interrupted. Interruption will cause the radio
not to operate anymore. Trying to flash the radio again will not work. 
The radio has to be returned to the depot for service.



==============================================================

RADIO SOFTWARE RELEASE NOTE

==============================================================

Release CONV_MOBILE_R05.10.02
Previous Release CONV_MOBILE_R05.10.01