============================================================================

 SOFTWARE RELEASE NOTE

============================================================================

Product  : Unofficial Lab Firmware and Codeplugs for Lab FlashGrade Tool
Release  : R02.07.05 Lab
Date     : 12-July-2010
Language : English

============================================================================

 PURPOSE OF THIS RELEASE

============================================================================

FIXES THE FOLLOWING ISSUES:

- This kit is for flashing GM3xx into GM6xx,and 
  upgrading/repairing,GM6xx,GM1280 radios.

HINTS:

- The ESN will set to zero after programming a codeplug.


- Supported model number:
Model Number	Tanapa		Latest	       Description
		Number		Version
----------------------------------------------------------------------------------------
M25RHC9CK1      IMUE6009A	07.00	       GM640(MCX720):  Mobile Pop UHF1 
M25SHC9CK1      IMUE6010A	07.00          GM640(MCX720):  Mobile Pop UHF2
M25KHC9CK1      IMUD6018A	07.00          GM640(MCX720):  Mobile Pop VHF
M25RHF9CK5      IMUE6009A	07.00          GM660(MCX760):  Mobile Pref UHF1 
M25SHF9CK5      IMUE6010A	07.00          GM660(MCX760):  Mobile Pref UHF2
M25KHF9CK5      IMUD6018A	07.00          GM660(MCX760):  Mobile Pref VHF
M25RHN9CK8      IMUE6009A	07.00          GM1280(MCX780): Mobile Prime UHF1
M25SHN9CK8      IMUE6010A	07.00          GM1280(MCX780): Mobile Prime UHF2
M25KHN9CK8      IMUD6018A	07.00          GM1280(MCX780): Mobile Prime VHF 
M25RHA9CK7      IMUE6009A	07.00	       GM1280(MCX700): Mobile Data Box UHF1
M25SHA9CK7      IMUE6010A	07.00	       GM1280(MCX700): Mobile Data Box UHF2
M25KHA9CK7      IMUD6018A	07.00 	       GM1280(MCX700): Mobile Data Box VHF
M25RHA9CK0      IMUE6009A	07.00	       GM1280(MCX700): Mobile Data Box Asia UHF1 
M25SHA9CK0      IMUE6010A	07.00	       GM1280(MCX700): Mobile Data Box UHF2
M25KHA9CK0      IMUD6018A	07.00	       GM1280(MCX700): Mobile Data Box Asia UHF2 

==============
EPP Models
==============         
M25RHC9CK1      IMUE6009B	07.00	       GM640(MCX720):  Mobile Pop UHF1 EPP
M25KHC9CK1      IMUD6018B	07.00	       GM640(MCX720):  Mobile Popu VHF EPP
M25RHF9CK5      IMUE6009B	07.00	       GM660(MCX760):  Mobile Pref UHF1 EPP
M25KHF9CK5      IMUD6018B	07.00          GM660(MCX760):  Mobile Pref VHF EPP 
M25RHN9CK8      IMUE6009B	07.00          GM1280(MCX780): Mobile Prime UHF1 EPP
M25KHN9CK8      IMUD6018B	07.00          GM1280(MCX780): Mobile Prime VHF EPP  
M25RHA9CK7      IMUE6009B	07.00          GM1280(MCX700): Mobile Data Box UHF1 EPP
M25KHA9CK7      IMUD6018B	07.00          GM1280(MCX700): Mobile Data Box VHF EPP  
M25RHA9CK0      IMUE6009B	07.00          GM1280(MCX700): Mobile Data Box Asia UHF1 EPP
M25KHA9CK0      IMUD6018B	07.00          GM1280(MCX700): Mobile Data Box Asia VHF EPP 


============================================================================

For the usage of this software the following radio accessories
are required:

(A) Flashing mobiles via the rear connector:

    - Flash adapter, P/N HLN9742A or B
    and (i)
    - Radio Interface Box, P/N RLN4008
      with battery or power supply
    - RIB to PC cable, P/N 3080369B72 (9pin) or 3080369B71 (25pin)
    - Programming/test cable, P/N RKN4083
    or (ii)
    - RIBless programming cable, P/N RKN4081
    - 10 pin (Mic) to 20 pin (rear) adapter RLN4853

    By using equipment (i) the Flash adapter has to be connected between the 
    Radio Interface Box and the Programming/test cable. Maximum baud rate for 
    this equipment is 19,200 Bd.

    By using equipment (ii) the Flash adapter has to be connected between the
    PC and the RIBless programming cable.

    For Flash Adapter HLN9742A, "Flash mode on" means switch position "ON".

    For Flash Adapter HLN9742B, "Flash mode on" means switch position "A", 
    position "B" is used for mic connector flashing.

    It is not possible to use Programming cable GTF374 for upgrading radios.

or

(B) Flashing mobiles via the mic connector:

    - RIBless programming cable, P/N RKN4081B
    - Flash adapter, P/N HLN9742B
    
    "Flash mode on" means flash adapter switch position "B",position "A" is 
    used for rear connector flashing.

    RIBless programming cable, P/N RKN4081A cannot be used for mic Connector 
    flashing.

    It is not possible to use Programming cable GTF374 for upgrading radios.

============================================================================

======================
SOFTWARE RELEASE NOTE
======================

PRODUCT : WARIS MPT GM640/GM660/GM1280 

VERSION       : R02.07.05 Lab
DATE OF BUILD : 12-July-2010