===========================================================

 SOFTWARE RELEASE NOTE

===========================================================

Product  : Unofficial Lab Firmware and Codeplugs for Lab FlashGrade Tool
KIT No   : ENVN4026H
Release  : R03.00.30 Lab Phase 3
Date     : 28-Aug-2002
Language : English

===========================================================

 PURPOSE OF THIS RELEASE

===========================================================
FIXES THE FOLLOWING ISSUES:
 
- This kit is for flashing GM6xx into GM3xx,GM1280 into GM380 and 
  upgrading/repairing,GM3xx radios.

HINTS:

- Use it only on Waris radios,build before Dec-2004!
  For radios after Dec-2004,the codeplugs are different and will follow later.


===========================================================
For the usage of this software the following radio accessories
are required:

(A) Flashing mobiles via the rear connector:

    - Flash adapter, P/N HLN9742A or B
    and (i)
    - Radio Interface Box, P/N RLN4008
      with battery or power supply
    - RIB to PC cable, P/N 3080369B72 (9pin) or 3080369B71 (25pin)
    - Programming/test cable, P/N RKN4083
    or (ii)
    - RIBless programming cable, P/N RKN4081
    - 10 pin (Mic) to 20 pin (rear) adapter RLN4853

    By using equipment (i) the Flash adapter has to be connected between the 
    Radio Interface Box and the Programming/test cable. Maximum baud rate for 
    this equipment is 19,200 Bd.

    By using equipment (ii) the Flash adapter has to be connected between the
    PC and the RIBless programming cable.

    For Flash Adapter HLN9742A, "Flash mode on" means switch position "ON".

    For Flash Adapter HLN9742B, "Flash mode on" means switch position "A", 
    position "B" is used for mic connector flashing.

    It is not possible to use Programming cable GTF374 for upgrading radios.

or

(B) Flashing mobiles via the mic connector:

    - RIBless programming cable, P/N RKN4081B
    - Flash adapter, P/N HLN9742B
    
    "Flash mode on" means flash adapter switch position "B", position "A" is 
    used for rear connector flashing.

    RIBless programming cable, P/N RKN4081A cannot be used for mic Connector 
    flashing.

    It is not possible to use Programming cable GTF374 for upgrading radios.

===========================================================

 RADIO SOFTWARE RELEASE NOTE

===========================================================

======================
SOFTWARE RELEASE NOTE
======================

PRODUCT : WARIS 5T GM300/GM340/GM360/GM380 Mobile Radio Lab Firmware
VERSION       : R03.04.00 Lab
DATE OF BUILD : 28-Aug-2002


Associated Part Numbers :

Description
WARIS Mobile CHA/CHC/CHD/Databox Radios

Models Supported :-
Description                 Sales Model NO      TANAPA
GM300 Databox VHF           M25KHA9AN0          IMUD6013A
GM300 Databox UHF           M25RHA9AN0          IMUE6015A

GM340 CHA VHF               M25KHC9AN1          IMUD6013A
GM340 CHA UHF               M25RHC9AN1          IMUE6015A

GM360 CHC LB1               M25BKF9AN5          IMUB6003A
GM360 CHC LB2               M25CKF9AN5          IMUB6004A
GM360 CHC LB3               M25DKF9AN5          IMUB6005A
GM360 CHC VHF               M25KHF9AN5          IMUD6013A
GM360 CHC UHF               M25RHF9AN5          IMUE6015A
GM360 CHC UHF2	            M25SHF9AN5		IMUE6016A
    
GM380 CHD VHF               M25KHN9AN8          IMUD6024A
GM380 CHD UHF               M25RHN9AN8          IMUE6038A
GM380 CHD UHF2		    M25SHN9AN8		IMUE6042A
 

==================
Build Environment
==================

- The Lab firmware and codeplugs are converted on a Siemens Scenic 860 series PC 
  with Hexworkshop 3.11
