===========================================================
 
 SOFTWARE RELEASE NOTE

===========================================================

Product  : Unofficial Lab Firmware and Codeplugs for Lab FlashGrade Tool to use on commercial radios.
Release  : R03.07.00 Lab
Date     : 12-Oct-2004
Language : English/German

===========================================================

 Purpose Of This Release

===========================================================

Supported features:

- Diese Lab Firmware und Codeplugs sind für die CM3xx Funkgeräte bestimmt.
  Die Lab Firmware und Codeplugs sind zur Verwendung mit dem Lab Flashgrade Programm bestimmt.
  Codeplugs nur als "Phase 3 to Phase 3" programmieren.

- This Lab firmwarepack is for the CM3xx select 5 radios.
  Use it with the Lab Flashgrade tool,for the Professional Series.
  For writing the codeplug,use only "Phase 3 to Phase 3".
 
============================================================================

INSTRUCTIONS ABOUT UPGRADING PROCESS

============================================================================

1.  Power on the radio. If the ignition is on, turn off all other accessories to
    ensure the quietest possible environment. Do not run the engine during this
    procedure.
2.  Connect all the items following the sequence: 
    PC com port --> Radio Interface Box(P/N RLN4008)(through P/N 3080369B72 for 9 pin 
    or P/N 3080369B71 for 25 pin) --> Programming Cable (RKN4083) --> Flash Adapter (FKN8096A) --> Radio.
3.  Start the Upgradetool from the 'Start Menu'.
4.  Select Options->Configuration to set the Flash Rate.
5.  Select Radio Access->Upgrade Radio or click "Upgrade Radio" icon on toolbar, and press Start Upgrade to upgrade the radio
6.  A message box will appear with instructions to put the radio in bootstrap
    mode.
	- Pull out the Programming Cable and turn off the radio.
        - Switch the flashing adapter into "Flash" mode. Then plug the flash cable back into the radio with the radio turned off.
        - Turn the radio on. Make sure the radio doesn't boot up like normal. Some of the LED's may light up but the Screen should stay blank. You may hear a static noise. This is "Bootstrap" Mode.


7.  After clicking Ok, upgrading should begin if properly put in bootstrap mode.
8.  When the process is complete, return the flashing switch to the 'CPS' position 
    before disconnecting the cable from the radio or powering it up.
9.  Connect another radio and repeat from step 4. Remember, the baud rate
    selection is done only the first time after starting up the program.

NOTE:
       1) Do not remove the programming cable or turn off the radio while
          upgrade is in progress.
       2) In case of failure during the upgrade, a message box will appear to
          guide the user to recover from the failure IF possible.
       3) You may not run more than one copy of the program at the same time.


============================================================================

===========================================================

 RADIO SOFTWARE RELEASE NOTE

===========================================================
======================
SOFTWARE RELEASE NOTE
======================

PRODUCT : ELM CM360(Marlin+)/CM340(Marlin) Radios

VERSION       : R03.07.00 Lab
DATE OF BUILD : 12-Oct-2004


Associated Part Numbers :

Description

ELM CM360(Marlin+)/CM340(Marlin) Radios

Applicable Models And Kits At Time Of Release
Description				          	Sales Model NO	TANAPA
CM340:5tMobAVHF1-Marlin  Mobile VHF1 band		M50JNC9AN2	PMUD1937A
CM360:5tMobBVHF1-Marlin+ Mobile VHF1 band               M50JNF9AN2      PMUD1941A

CM340:5tMobAVHF-Marlin   Mobile VHF2 band 		M50KNC9AN2	PMUD1879A
CM360:5tMobBVHF-Marlin+  Mobile VHF2 band 		M50KNF9AN2	PMUD1881A
                       
CM340:5tMobAUHF-Marlin   Mobile UHF1 band		M50QNC9AN2	PMUE2023A
CM360:5tMobBUHF-Marlin+  Mobile UHF1 band		M50QNF9AN2	PMUE2025A
                                             
CM340:5tMobAUHF2-Marlin  Mobile UHF2 band		M50RNC9AN2	PMUE2019A
CM360:5tMobBUHF2-Marlin+ Mobile UHF2 band		M50RNF9AN2	PMUE2021A
 
CM340:5tMobAUHF3-Marlin  Mobile UHF3 band		M50SNC9AN2	PMUE2164A
CM360:5tMobBUHF3-Marlin+ Mobile UHF3 band		M50SNF9AN2	PMUE2165A
 
CM340:5tMobAUHF4-Marlin  Mobile UHF4 band	        M50TRC9AN2	PMUE2180A
CM360:5tMobBUHF4-Marlin+ Mobile UHF4 band	        M50TRF9AN2	PMUE2183A
 
CM340:5tMobAMID-Marlin   Mobile Mid band		M50FNC9AN2	FUC1601A
CM360:5tMobBMID-Marlin+  Mobile Mid band		M50FNF9AN2	FUC1603A


====================
ASSOCIATED SOFTWARE
====================

CODEPLUG COMPATIBILITY : R03.16.00

CPS COMPATIBILITY: R01.12.00


=====================
NEW FEATURES / NOTES
=====================

Problems Solved since previous Release (R03.06.08)

  New feature Added
 ----------------- 
 CDDts02436:Add support for ELM 5T UHF4 band in firmware

  Problems Fixed
 ----------------- 
 CDDts02466(GCC8070431):CM300 series Pin 2 not deviating carrier with Pin 3 Voice/Data PTT.
 Description: 
 CM300 series Pin 2 not deviating carrier with Pin 3 set to voice/Data PTT. 
 If Pin3 is assigned to fast data ptt or fast v/d ptt, the high level PTT request will be disabled.
 Effect: ELM 5T firmware
 
 CDDts03112(GCC8160616):CM340 Occasionally hangs when vehicle started
 Description: 
 1. Connect a mid band radio (CM340 or CM360 to power supply.
 2. Adjust the voltage to the power supply, decrease the voltage little by little from 13V.
 3. When the voltage fall into 5 to 6V, the radio will alternatively flash red and green led and the keypad is locked(Synthesiser unclock state ).
 4. Increase the voltage little by little back to 13V .
 5. The radio will still alternatively flash red and green led and the keypad is locked 
    (Still in synthesiser unclock state).
 Effect: ELM 5T firmware
 
 CDDts03129(GCC8185138):CM3xx, if PL 'Turn off Code' checked radio will not TX with data or v/d
 Description: 
 This problem only happens if the debounce is disabled.
 When GPIO pin 3 set to data ptt or voice/data ptt and debounce is disabled, 
 if one or more of following conditions are enabled, 
 this problem(radio can not keyup) will occur:
 - PTT keyup mode
 - Authorisation
 - TX admit criteria (except 'Always Allowed')
 - TX time-out timer mode
 - PTT dekey encode
 - PL Reversed burst / DPL TOC
 - Scan list enable
 Effect: ELM 5T firmware

 CDDts03390(GCC8178388):CM360 dead after menu scroll
 Description: 
 CPS Configuration:
 P1 Menu only programmed with Channel switch
 P3 programmed with Call 1
 duplicate procedure:
 1. Radio is switched on
 2. P3 pushed for call then
 3. P1 pushed (Display is empty, only Symbol LA and L), now 
 4. push up or down
 5. now the radio is "dead" with lightened display, and is not possible to switch off the radio
 Effect: ELM 5T firmware
 
 CDDts03663:ELM 5T Freq drift issue(second change after R03.06.08 change)
 Description: In R03.06.08, a fix was done for the ELM freq drift issue.  But with that fix, 
 the fast data ptt still has the freq drift problem sometimes the freq drift is about 1k.
 Effect: ELM 5T firmware


==================
Build Environment
==================


