===============================================================================

 SOFTWARE RELEASE NOTE

===============================================================================

Product  : Unofficial Lab Firmware and Codeplugs for Lab FlashGrade Tool
Release  : R03.10.03 Lab Phase 3
Date     : 01-Dec-07
Language : English

===============================================================================

 PURPOSE OF THE RELEASE
 
===============================================================================
FIXES THE FOLLOWING ISSUES:
 
-N/A

  
- Supported model number:

Model Number	Tanapa Number	Latest Version	Description
-------------------------------------------------------------------------------
New models (CCB364)
-------------------------------------------------------------------------------
M25KHF4AN5	IMUD6013B	06.00		GM360(GM339)pref vhf epp 12_5K
M25RHF4AN5	IMUE6015B	06.00		GM360(GM339)pref Uhf epp 12_5K
M25SHF4AN5	IMUE6016A	06.00		GM360(GM339)pref uhf2 12_5K


EPP models
-------------------------------------------------------------------------------
M25KHA9AN0	IMUD6013B	06.00		GM300 databox vhf epp
M25KHC9AN1	IMUD6013B	06.00		GM340 plain vhf epp
M25KHF9AN5	IMUD6013B	06.00		GM360(GM339)pref vhf epp
M25KHN9AN8	IMUD6024B	06.00		GM380(GM399)prime vhf epp
M25RHA9AN0  	IMUE6015B	06.00		GM300 databox uhf epp
M25RHC9AN1 	IMUE6015B	06.00		GM340 plain uhf epp
M25RHF9AN5	IMUE6015B	06.00		GM360(GM339)pref uhf epp
M25RHN9AN8	IMUE6038B	06.00		GM380(GM399)prime uhf epp


Non-EPP models
-------------------------------------------------------------------------------
M25BKF9AN5	IMUB6003A	06.00		GM360(GM339)pref lb1
M25CKF9AN5	IMUB6004A	06.00		GM360(GM339)pref lb2
M25DKF9AN5	IMUB6005A	06.00		GM360(GM339)pref lb3
M25KHA9AN0	IMUD6013A	06.00		GM300 databox vhf
M25KHC9AN1	IMUD6013A	06.00		GM340 plain vhf
M25KHF9AN5	IMUD6013A	06.00		GM360(GM339)pref vhf
M25KHN9AN8	IMUD6024A	06.00		GM380(GM399)prime vhf
M25RHA9AN0	IMUE6015A	06.00		GM300 databox uhf 
M25RHC9AN1	IMUE6015A	06.00		GM340 plain uhf
M25RHF9AN5	IMUE6015A	06.00		GM360(GM339)pref uhf
M25RHN9AN8	IMUE6038A	06.00		GM380(GM399)prime uhf
M25SHF9AN5	IMUE6016A	06.00		GM360(GM339)pref uhf2
M25SHN9AN8	IMUE6042A	06.00		GM380(GM399)prime uhf2


===============================================================================
For the usage of this software the following radio accessories are required:

(A) Flashing mobiles via the rear connector:

    - Flash adapter, P/N HLN9742A or B 
      and (i)
    - Radio Interface Box, P/N RLN4008
      with battery or power supply
    - RIB to PC cable, P/N 3080369B72 (9pin) or 3080369B71 (25pin)
    - Programming/test cable, P/N RKN4083
      or (ii)
    - RIBless programming cable, P/N RKN4081
    - 10 pin (Mic) to 20 pin (rear) adapter RLN4853

    By using equipment (i) the Flash adapter has to be connected between the 
    Radio Interface Box and the Programming/test cable. Maximum baud rate for 
    this equipment is 19,200 Bd.

    By using equipment (ii) the Flash adapter has to be connected between the
    PC and the RIBless programming cable.

    For Flash Adapter HLN9742A, "Flash mode on" means switch position "ON".

    For Flash Adapter HLN9742B, "Flash mode on" means switch position "A", 
    position "B" is used for mic connector flashing.

    It is not possible to use Programming cable GTF374 for upgrading radios.

or

(B) Flashing mobiles via the mic connector:

    - RIBless programming cable, P/N RKN4081B
    - Flash adapter, P/N HLN9742B
    
    "Flash mode on" means flash adapter switch position "B",position "A" is 
    used for rear connector flashing.

    RIBless programming cable, P/N RKN4081A cannot be used for mic Connector 
    flashing.

    It is not possible to use Programming cable GTF374 for upgrading radios.



=======================================================================================

RADIO SOFTWARE RELEASE NOTE

=======================================================================================
Release waris5t-R03.10.03

==================
Build Environment
==================

- The Lab firmware and codeplugs are converted on a Dell Inspiron 8000 and Fujitsu-Siemens 
  Scenic D series PC with Hexworkshop 5 and HxD 1.7.1.0 beta