============================================================================

 SOFTWARE RELEASE NOTE

============================================================================

Product  : Unofficial Lab Firmware and Codeplugs for Lab FlashGrade Tool
Release  : R02.00.22 Lab
Date     : 09-July-2005
Language : English

============================================================================

 PURPOSE OF THIS RELEASE

============================================================================

FIXES THE FOLLOWING ISSUES:

- This kit is for flashing GM3xx into GM6xx,and 
  upgrading/repairing,GM6xx,GM1280 radios.

HINTS:

- Use it only on Waris radios,build before Dec-2004!
  For radios after Dec-2004,the codeplugs are different and will follow later.

- The ESN will set to zero after programming a codeplug.

============================================================================

For the usage of this software the following radio accessories
are required:

(A) Flashing mobiles via the rear connector:

    - Flash adapter, P/N HLN9742A or B
    and (i)
    - Radio Interface Box, P/N RLN4008
      with battery or power supply
    - RIB to PC cable, P/N 3080369B72 (9pin) or 3080369B71 (25pin)
    - Programming/test cable, P/N RKN4083
    or (ii)
    - RIBless programming cable, P/N RKN4081
    - 10 pin (Mic) to 20 pin (rear) adapter RLN4853

    By using equipment (i) the Flash adapter has to be connected between the 
    Radio Interface Box and the Programming/test cable. Maximum baud rate for 
    this equipment is 19,200 Bd.

    By using equipment (ii) the Flash adapter has to be connected between the
    PC and the RIBless programming cable.

    For Flash Adapter HLN9742A, "Flash mode on" means switch position "ON".

    For Flash Adapter HLN9742B, "Flash mode on" means switch position "A", 
    position "B" is used for mic connector flashing.

    It is not possible to use Programming cable GTF374 for upgrading radios.

or

(B) Flashing mobiles via the mic connector:

    - RIBless programming cable, P/N RKN4081B
    - Flash adapter, P/N HLN9742B
    
    "Flash mode on" means flash adapter switch position "B",position "A" is 
    used for rear connector flashing.

    RIBless programming cable, P/N RKN4081A cannot be used for mic Connector 
    flashing.

    It is not possible to use Programming cable GTF374 for upgrading radios.

============================================================================

======================
SOFTWARE RELEASE NOTE
======================

PRODUCT : WARIS MPT GM640/GM660/GM1280 

VERSION       : R02.00.22 Lab
DATE OF BUILD : 09-July-2005



Associated Part Numbers :

Description

WARIS MPT Mobile GM640/GM660/GM1280 Radios

Applicable Models And Kits At Time Of Release
Description				      Sales Model NO		TANAPA
GM640:          Control Head A UHF1   		M25RHC9CK1      	IMUE6009A
GM640:          Control Head A UHF2   		M25SHC9CK1      	IMUE6010A
GM640:          Control Head A VHF    		M25KHC9CK1      	IMUD6018A

GM660(MCX760):  Control Head C UHF1   		M25RHF9CK5      	IMUE6009A
GM660(MCX760):  Control Head C UHF2   		M25SHF9CK5      	IMUE6010A
GM660(MCX760):  Control Head C VHF    		M25KHF9CK5      	IMUD6018A

GM1280(MCX780): Control Head D UHF1   		M25RHN9CK8      	IMUE6009A
GM1280(MCX780): Control Head D UHF2   		M25SHN9CK8      	IMUE6010A
GM1280(MCX780): Control Head D VHF    		M25KHN9CK8      	IMUD6018A
GM1280(MCX780): Data Box UHF1             	M25RHA9CK7      	IMUE6009A
GM1280(MCX780): Data Box UHF2            	M25SHA9CK7      	IMUE6010A
GM1280(MCX780): Data Box VHF               	M25KHA9CK7 		IMUD6018A

==================
Build Environment
==================

- The Lab firmware and codeplugs are converted on a Siemens Scenic 860 series PC 
  with Hexworkshop 3.11