===========================================================

 SOFTWARE RELEASE NOTE

===========================================================

Product  : Unofficial EU Waris Lab Upgrade Kit
KIT No   : AG 10a
Release  : R02.05.01	
Date     : 03-Dec-2008		
Language : English

===========================================================

 PURPOSE OF THIS RELEASE

===========================================================

Supported features:

- Reading Radio information

- Upgrade a radio with new firmware and codeplug.

Radios supported:

 -EU Waris (GM3xx,GP3xx,GM6xx,GP6xx,GM12xx,GP12xx)radios
 -Conventional Marlin (CM3xx)radios

Supported Software versions:

- Depends of the used firmware.All Regions are supported.


===========================================================
NEW FEATURES / NOTES
===========================================================
 -Added the firmware/codeplugs R03.12.03 for GP3xx radios.
 -All actual models are supported. 

===========================================================

 HOW TO INSTALL AND RUN THIS SOFTWARE

===========================================================
 -Copy all files into a directory and run the Lab Upgrade Tool
  to program the radio with a default codeplug and flash new 
  firmware.
 -Before you flash the new firmware,program the radio with a 
  default codeplug!
 
===========================================================
For the usage of this softwarekit the following radio accessories
are required:

(A) Flashing mobiles via the rear connector:

    - Flash adapter, P/N HLN9742A or B
    and (i)
    - Radio Interface Box, P/N RLN4008
      with battery or power supply
    - RIB to PC cable, P/N 3080369B72 (9pin) or 3080369B71 (25pin)
    - Programming/test cable, P/N RKN4083
    or (ii)
    - RIBless programming cable, P/N RKN4081
    - 10 pin (Mic) to 20 pin (rear) adapter RLN4853

    By using equipment (i) the Flash adapter has to be connected between the 
    Radio Interface Box and the Programming/test cable. Maximum baud rate for 
    this equipment is 19,200 Bd.

    By using equipment (ii) the Flash adapter has to be connected between the
    PC and the RIBless programming cable.

    For Flash Adapter HLN9742A, "Flash mode on" means switch position "ON".

    For Flash Adapter HLN9742B, "Flash mode on" means switch position "A", 
    position "B" is used for mic connector flashing.

    It is not possible to use Programming cable GTF374 for upgrading radios.


(B) Flashing mobiles via the mic connector:

    - RIBless programming cable, P/N RKN4081B
    - Flash adapter, P/N HLN9742B
    
    "Flash mode on" means flash adapter switch position "B", position "A" is 
    used for rear connector flashing.

    RIBless programming cable, P/N RKN4081A cannot be used for mic Connector 
    flashing.

    It is not possible to use Programming cable GTF374 for upgrading radios.

===========================================================

 UPGRADETOOL RELEASE NOTE

===========================================================
Release Lab Upgrade Tool

Created on Aug 23 12:00:00 BST 2007
--------------------------------------------------------------
======================
SOFTWARE RELEASE NOTE
======================

PRODUCT : EU Waris Lab Upgradetool (EN)
VERSION       : R03.01.00
DATE OF BUILD : 03-Aug-2008


=====================
NEW FEATURES / NOTES
=====================

Problems Fixed since last version
---------------------------------
 -Corrected faulty popup.

==================
Build Environment
==================

Created and edited on Fujitsu-Siemens Scenic D Series PC 
with Hexworkshop 3.11.
Extended edit on Dell Inspiron 8000 PC with PE Explorer.