===========================================================

 SOFTWARE RELEASE NOTE

===========================================================

Product  : Unofficial US Waris Lab Upgrade
KIT No   : AG 22
Release  : R02.08.00	
Date     : 14-Jan-2009		
Language : English

===========================================================

 PURPOSE OF THIS RELEASE

===========================================================

Supported features:

- Reading Radio information

- Upgrade a radio with new firmware and codeplug.
  You can use it on all Professional and Commercial Series Radios.

- To upgrade the european GM/GP3xx,GM/GP6xx,GM/GP12xx and CM3xx,
  you need a different lab upgradekit like
  Lab Firmware-Codeplugkit EU Waris!

Radios supported:

 -Waris conventional radios
 -Conventional Marlin (CMxxx)radios
 -Guppy and Piranha (CPxxx) radios
 -GP580 support

Supported Software versions:

- Latest Professional and Entry Series CPS.All Regions are supported.
===========================================================

 HOW TO INSTALL AND RUN THIS SOFTWARE

===========================================================
  Copy all files into a directory and run the US Waris Codeplug Tool
  to program the radio with a default codeplug,to upgrade or fix a
  checksum error.The "no serial" codeplugs will let you set a new
  serial number without any tuner modifications.
  Use the US Waris Firmware Tool for flashing a new firmware.

===========================================================
For the usage of this softwarekit the following radio accessories
are required:

(A) Flashing mobiles via the rear connector:

    - Flash adapter, P/N HLN9742A or B
    and (i)
    - Radio Interface Box, P/N RLN4008
      with battery or power supply
    - RIB to PC cable, P/N 3080369B72 (9pin) or 3080369B71 (25pin)
    - Programming/test cable, P/N RKN4083
    or (ii)
    - RIBless programming cable, P/N RKN4081
    - 10 pin (Mic) to 20 pin (rear) adapter RLN4853

    By using equipment (i) the Flash adapter has to be connected between the 
    Radio Interface Box and the Programming/test cable. Maximum baud rate for 
    this equipment is 19,200 Bd.

    By using equipment (ii) the Flash adapter has to be connected between the
    PC and the RIBless programming cable.

    For Flash Adapter HLN9742A, "Flash mode on" means switch position "ON".

    For Flash Adapter HLN9742B, "Flash mode on" means switch position "A", 
    position "B" is used for mic connector flashing.

    It is not possible to use Programming cable GTF374 for upgrading radios.


(B) Flashing mobiles via the mic connector:

    - RIBless programming cable, P/N RKN4081B
    - Flash adapter, P/N HLN9742B
    
    "Flash mode on" means flash adapter switch position "B", position "A" is 
    used for rear connector flashing.

    RIBless programming cable, P/N RKN4081A cannot be used for mic Connector 
    flashing.

    It is not possible to use Programming cable GTF374 for upgrading radios.

===========================================================

 RADIO SOFTWARE RELEASE NOTE

===========================================================

======================
SOFTWARE RELEASE NOTE
======================

PRODUCT : US Waris Lab Firmware/Codeplugkit
VERSION       : R02.08.00
DATE OF BUILD : 14-Jan-2008



====================
ASSOCIATED SOFTWARE
====================
 
CPS COMPATIBILITY      : Latest Professional,Commercial and Entry Series CPS


=====================
NEW FEATURES / NOTES
=====================

 Problems Fixed since last version
 ---------------------------------

 - Latest firmware/codeplugs for conventional Waris radio.

