Release Notes for Tuner for Professional Radios Version R02.00.01

This version of the tuner supports the following tuning operations:-

	Rx(Receive) Alignments

	1. Front End Filter Tuning
	2. Squelch Attn (12.5,20,25kHz)
	3. Rated Volume Tuning
	4. RSSI Tuning 

	Tx(Transmit) Alignments

	1. Reference Oscillator Warp
	2. Transmit Power Tuning (High/Low Power)
	   /Mobile K&M tuning
	3. Modulation Balance Attenuation
	4. VCO Attenuation (12.5,20,25kHz)
	5. DTMF Signalling Deviation
	6. MDC 1200 Signalling Deviation
	7. PA Bias Tuning (High/Low Power) 
	8. Select 5 Signalling
	9. MPT 1327 Signalling deviation
	10.Battery Threshold tuning 

This version of the tuner supports full tuner OLE compliance (i.e. launch of tuner archive file
via double-clicking on the SFP file).

This version also supports multiple Read All/Write All softpots for radios containing firmware that
supports the operation. It is also backwards compatible with current firmware releases which do not
support the read/write all operations.

Battery Threshold and Mobile K & M tuning is fully supported in this release. Load/Save/Program
and Print Preview support has already been added into this version.

Please take note that Save/Load/Program All for K&M tuning, PA Bias 2/3 has been added in this 
release. Battery Threshold tuning has also been implemented in this release.

This version sets PA Bias 1,2 and 3 to 0 after Toggle Voltage has been pressed. This is to avoid 
potential confusion regarding current measurements observed.

This version contains the Baseband offset configuration file which will also work for Entry Level
portable radios.

Please take note that this version contains the modified baseband offset config file.

Context sensitive help has also been added for K & M and Battery Threshold tuning.

 