Release Notes for Tuner for Professional Radios Version R02.00.02

This version of the tuner supports the following tuning operations:-

	Rx(Receive) Alignments

	1. Front End Filter Tuning
	2. Squelch Attn (12.5,20,25kHz)
	3. Rated Volume Tuning
	4. RSSI Tuning 

	Tx(Transmit) Alignments

	1. Reference Oscillator Warp
	2. Transmit Power Tuning (High/Low Power)
	   /Mobile K&M tuning
	3. Modulation Balance Attenuation
	4. VCO Attenuation (12.5,20,25kHz)
	5. DTMF Signalling Deviation
	6. MDC 1200 Signalling Deviation
	7. PA Bias Tuning (High/Low Power) 
	8. PA Voltage Limit 
	9. Select 5 Signalling
	10.MPT 1327 Signalling deviation
	11.High Speed Trunking Signalling 
	12.Battery Threshold tuning 

PA Voltage Limit auto tuning is fully supported for LB Low Power Mobile radios. Load/Save/Program All and Print Preview support has been already added into this version.

High Speed Trunking Signalling is fully supported for Privacy Plus radios. Load/Save/Program All and Print Preview support has been already added into this version.

This version also supports multiple Read All/Write All softpots for radios containing firmware that
supports the operation. It is also backwards compatible with current firmware releases which do not
support the read/write all operations.

Support for radios which has invalid(0) frequency points such as 800MHz radios. 

This version contains the Baseband offset configuration file which will also work for Entry Level
portable radios, Privacy Plus radios and Aoba radios.

Context sensitive help text has also been added for PA Voltage Limit, High Speed Trunking Signalling, Baseband Offset and Program Serial Number.

Help text for specific tuning options for UHF Band 1, UHF Band 2, 330Mhz and 300MHz radios.