 NOTES ON GTX RSS Release R01.01.00 RVN4150B
 ===========================================

 The GTX Radio Service Software is being updated to R01.01.00.

 The GTX RSS has been issued to support for new models and features.

 The models are:

  M11WGD4CU1AN - GTX, 10 Conventional Channel, 10 Systems, 8 Talkgroup,
                 900MHz.
  H11WCD4CU1AN - GTX, 10 Conventional Channel, 10 Systems, 8 Talkgroup,
                 900MHz.
  M11RHD4DB1AN - GTX, 10 Conventional Channel, 10 Systems, 8 Talkgroup,
                 UHF1.
  H11QDH4DB1AN - GTX, 10 Conventional Channel, 10 Systems, 8 Talkgroup,
                 UHF1.
  M11WGD4CB1AN - GTX, 10 Conventional Channel, 10 Systems, 8 Talkgroup,
                 900MHz.
  H11WCD4CB1AN - GTX, 10 Conventional Channel, 10 Systems, 8 Talkgroup,
                 900MHz.

 DISK CONTENTS:
 =============
 
 The GTX RSS, version R01.01.00, comes in one 3.5" Double Sided/Double 
 Density disk.  The disk contain the following files:

        DISK #1
        -------
        DISK.ID
        INSTALL.DAT
        INSTALL.EXE
        GTX.LIB
        README.TXT


 INSTALLATION PROCEDURE:
 =======================

 1. Place Disk 1 in your floppy disk drive. 
 2. Go to the floppy disk drive.
 3. Type "INSTALL" and press return.
 4. Follow the installation directions displayed on your screen.
 5. When installation is complete, make sure that you are in the 
    directory where the GTX RSS application was installed. 
 6. Type "GTX" at the DOS prompt to start the GTX RSS application.

 Please refer to the user manual for more information.
 
 If you have problems programming or using this product,
 contact your sales representative.
