
===============================================
MCS2000 Radio Tuner Software R02.01.00
===============================================


Introduction:
------------

Welcome to the MCS2000 Windows Tuner Software 
by Motorola.  The notes below 
serve to introduce you to the software you are 
about to install.  Please read these notes in 
their entirety before installing and using the 
MCS2000 Tuner R02.01.00 Release.

Enhancements / fixes :
----------------------

1) A new PA Bias screen has been added to the Tuner
which is applicable only for 900Mhz radios with a 
R/F PA Revision "B".

2) The Microphone Alignment - Secure Gain screen 
has been removed for all 900 Mhz radios since it 
does not apply to the 900Mhz radios.


System Requirements:
--------------------
Operating Systems:   Windows 98 Second Edition,
                     Windows NT 4.0 (SP 6a or higher),
                     Windows 2000
                     Windows XP Home Edition 
                     Windows XP Professional 
                     Note: Windows ME, Windows 95 and Windows 98
		     First Edition are no longer supported.
                     You may choose to proceed with the installation, but
                     some features might not be functioning properly.
                     Upgrading the operating system is highly recommended. 


Hardware Requirements:
---------------------

The following should be considered minimum hardware 
requirements for running the MCS2000 Tuner.

   *  233MHz Processor (400MHz recommended)
   *  32MB RAM for Windows 98 Second Edition(128MB
      RAM recommended)
   *  128MB RAM for Windows NT 4.0 
   *  500MB hard drive with 40MB free space 
   *  One Serial COM Port
   *  CD-ROM Drive

 
Installation:
------------

When you insert the Installation CD into the CD-ROM
drive of your computer, the installation should run 
automatically, if it does not, run  Setup.exe file 
which appears in the Installation CD window, and 
follow the instructions.


Uninstalling the Tuner:
--------------------

Before uninstalling the MCS2000 Tuner, the 
following must be performed.

   1) Close the Motorola Application Launcher, if its 
      icon appears in the system tray of the taskbar.
   2) Exit any active CPS/Tuner applications.

Then, to uninstall the MCS2000 Tuner, select 
Start->Settings->Control Panel.  Double-click on Add/
Remove Programs.  In the Add/Remove Programs window, 
select Motorola MCS2000 Tuner, and click 
on the Add/Remove button.  Follow the instructions that 
appear. 


Online Help:
-----------

Extensive online Help is available from within the 
MCS2000 Tuner application.  After activating the Tuner 
(Start>Programs->Motorola->MCS MTS 2000 Products->MCS2000 
Tuner), choose "Help Topics" from the Help menu.  A full 
listing of Help topics will appear.  



Known Issues With the MCS2000 Tuner R02.01.00 Release:
---------------------------------------------------

1) Tuner does not check the serial number of the radio in 
Tx Power 3 screen, so do not change radios while using this 
screen.

2) Tuner performance varies with processor speed and RAM.

3) When any slider control is selected, the up cursor key 
will decrement the current value (move the slider to the 
left) and the down cursor key will increment the current 
value (move the slider to the right). To avoid this problem, 
use the mouse, the left/right cursor keys, or click on the 
value spin box instead.

4) The Program button will fail to store the value if the 
radio contains a non-standard serial number.


===============================================
