Release Notes for Tuner for Professional Radios Version R01.00.00

This version of the tuner supports the following tuning operations:-

	Rx(Receive) Alignments

	1. Front End Filter Tuning
	2. Squelch Attn. (12.5,20,25KHz)
	3. Rated Volume Tuning.

	Tx(Transmit) Alignments

	1. Reference Oscillator Warp
	2. Transmit Power Tuning (High/Low Power)
	3. Modulation Balance Attenuation
	4. VCO Attenuation (12.5,20,25KHz)
	5. DTMF Signalling Deviation
	6. MDC 1200 Signalling Deviation
	7. PA Bias Tuning (High/Low Voltage)

This version DOES NOT support MPT tuning operations such as Select 5, MPT 1200 Signalling
and RSSI tuning. These features will be added into Version R01.00.01.

If you have any questions concerning this release of the tuner, you may contact:-

	Chee Chin Yaik
	R N D Software Engineer,
	Motorola Penang FTZ Phase III,
	11900 Penang, 
	Malaysia.

	Ext	: 60-4-8504013
	Email	: CCC050@email.mot.com

