Release Notes for Tuner for Professional Radios Version R02.00.03

This version of the tuner supports the following tuning operations:-

	Rx(Receive) Alignments

	1. Front End Filter Tuning
	2. Squelch Attn (12.5,20,25kHz)
	3. Rated Volume Tuning
	4. RSSI Tuning 

	Tx(Transmit) Alignments

	1. Reference Oscillator Warp
	2. Transmit Power Tuning (High/Low Power)
	   /DAC tuning for LB Mobile
	   /Mobile K&M tuning
	3. Modulation Balance Attenuation
	4. VCO Attenuation (12.5,20,25kHz)
	5. DTMF Signalling Deviation
	6. MDC 1200 Signalling Deviation
	7. PA Bias Tuning (High/Low Power) 
	8. PA Voltage Limit 
	9. Select 5 Signalling
	10.MPT 1327 Signalling deviation
	11.High Speed Trunking Signalling 
	12.Battery Threshold tuning 

The main addition to this release is the DAC tuining screen 
which is used for Low Band Mobile Radios K&M tuning.
                                 
Send a dekey request when the user presses the program button in radio keyed up state.

Do a limit check on K&M values before programming in the softpots. An error message
will be displayed if any of the K&M values exceeds its limit.
