Differences Between XTS 3000 & ASTRO Saber CPS and XTS 2500 & XTS 5000 CPS:
---------------------------------------------------------------------------
1) Conventional frequencies are no longer input on the Conventional
   Personality. They are now located on the Zone Channel Assignment table.
   This interface is similar to the trunking interface and it also enables
   the radio to support many more Conventional Channels than Conventional
   Personalities.
2) New cabling is required for the XTS 2500 & XTS 5000. The new cable does
   not use a RIB or SRIB. Refer to the 'Connecting the PC to the Radio'
   section of this file for the part number.