This is exciter firmware R020.09.018. It is current as of 1/1/2013.

It is paired with Station Control Module firmware R020.14.048.

Exciter firmware does not automatically update during the Quantar RSS firmware update procedure as the exciter does not have a flash ROM.

You must use a AT27C512R 28-pin DIP EPROM chip (or equivalent OTP ROM) with this firmware build. Simply pop open the exciter module and replace the existing chip with a new one. It is socketed and easy to remove.