[NetAdmin]
LocalSocket=23
RemoteHost=0
RemoteSocket=0
Timeout=10000

[TestTone]
Enabled=N               ;Y to enable,N to disable, default=N
Freq1=1000              ;1st frequency (Hz) 1-3000, default is 1000
Freq2=1000              ;2nd frequency (Hz) 1-3000, default is 1000
Volume1=0               ;(Neg.dB) 0-40, loudest is 0,default is 0
Volume2=0               ;(Neg.dB) 0-40, loudest is 0,default is 0
Repeat=1                ;times to play tone, default is 1
On1=1000                ;first on interval in ms, default is 1000
Off1=500                ;first off interval in ms, default is 500
On2=0                   ;second on interval in ms, default is 0
Off2=0                  ;second off interval in ms, default is 0

[TimeZones]
TZ01="GMT~Greenwhich Mean Time~0"
TZ02="EST~Eastern Standard Time~-500"
TZ03="CST~Central Standard Time~-600"
TZ04="MST~Mountain Standard Time~-700"
TZ05="PST~Pacific Standard Time~-800"
TZ06="KST~Seoul,South Korea~+900"
TZ07="AET~Eastern Standard,Australia~+1000"
TZ08="ACT~Central Standard,Australia~+950"
TZ09="AWT~Western Standard,Australia~+800"
TZ10="IRT~Rome,Italy~+100"
TZ11="RCT~Capetown,South Africa~+200"
TZ12="SST~Singapore,Singapore~+800"
TZ13="INT~New Delhi,India~+500"

[Tones]
; Tone definition section, used to define global detect tones.
; Tone definitions are of the form:
;    Name=F1,F2,E,N1,N1D,F1,F1D,N2,N2D,F2,F2D,R
; where:
;    'Name' is the name of the tone being identified
;    'ID'   is the number the tone is referenced by internally, do not change
;    'F1'   is the first frequency (lower tone) in Hz
;    'F2'   is the second frequency (higher tone, if any) in Hz
;    'E'    is the tone detection edge, 1 for leading, 2 for trailing
;    'N1'   is the first cadence tone on time in 1/100 of a second
;    'N1D'  is the first cadence tone on time as a percentage
;    'F1'   is the first cadence tone off time in 1/100 of a second
;    'F1D'  is the first cadence tone off time as a percentage
;    'N2'   is the second cadence tone on time in 1/100 of a second
;    'N2D'  is the second cadence tone on time as a percentage
;    'F2'   is the second cadence tone off time in 1/100 of a second
;    'F2D'  is the second cadence tone off time as a percentage
;    'R'    is the number of times the cadence is heard before recognition
;
; Leave any values that do not apply (second tone, repeats, etc.) at 0.
; Set to "ID,0,0,0,0,0,0,0,0,0,0,0,0" to disable.
; Valid tone names are: FaxReceive, FaxTransmit, Dial, Busy, and Reorder.
;
; Industry Standards:
; Fax Receive Tone:  2100Hz for 3000ms
; Fax Transmit Tone: 1100Hz +/-38Hz, 500ms On +/-15%, 3000ms Off +/-15%
; Dial Tone:         350Hz and 440Hz, continuous
; Busy Tone:         480Hz and 620Hz, 500ms On, 500ms Off
; Reorder Tone:      480Hz and 620Hz, 250ms On, 250ms Off
;
; Default values:
FaxReceive=5,2150,0,1,500,10,0,10,0,10,0,10,1
FaxTransmit=5,1100,0,1,500,15,0,10,0,10,0,10,1
; Dial=1,350,440,1,1000,10,0,10,0,10,0,10,2
; Busy=2,480,620,1,50,10,50,10,0,10,0,10,1
Busy=2,400,0,1,500,10,500,10,0,10,0,10,2
; Reorder=3,480,620,1,25,10,25,10,0,10,0,10,1
