CGTHREE(4S)

NAME
cgthree - 8-bit color memory frame buffer

CONFIG — Desktop SPARCsystems
device-driver cgthree

CONFIG — Sun386i SYSTEM
device cgthree0 at obmem ? csr 0xA0400000

AVAILABILITY
Desktop SPARCsystems and Sun386i systems only.

DESCRIPTION
cgthree is a color memory frame buffer. It provides the standard frame buffer interface as defined in fbio(4S).

FILES
/dev/cgthree[0-9]

SEE ALSO
mmap(2), fbio(4S)