T_OPTMGMT(3N)

NAME
t_optmgmt - manage options for a transport endpoint

SYNOPSIS

#include <tiuser.h>

int t_optmgmt(fd, req, ret)
int fd;
struct t_optmgmt *req;
struct t_optmgmt *ret;

DESCRIPTION

t_optmgmt() enables a transport user to retrieve, verify, or negotiate protocol options with the transport provider. fd identifies a bound transport endpoint.

The req and ret arguments point to a t_optmgmt() structure containing the following members:
	struct netbuf opt;
	long	flags;

The opt field identifies protocol options and the flags field is used to specify the action to take with those options.

The options are represented by a netbuff structure in a manner similar to the address in t_bind(3N). The maxlen, len, and buf members of the netbuf structure are described in t_accept(3N). req is used to request a specific action of the provider and to send options to the provider. len specifies the number of bytes in the options, buf points to the options buffer, and maxlen has no meaning for the req argument. The transport provider may return options and flag values to the user through ret. For ret, maxlen specifies the maximum size of the options buffer and buf points to the buffer where the options are to be placed. On return, len specifies the number of bytes of options returned. maxlen has no meaning for the req argument, but must be set in the ret argument to specify the maximum number of bytes the options buffer can hold. The actual structure and content of the options is imposed by the transport provider.

The flags field of req can specify one of the following actions:

T_NEGOTIATE
    Enables the user to negotiate the values of the options specified in req with the transport provider. The provider will evaluate the requested options and negotiate the values, returning the negotiated values through ret.

T_CHECK
    Enables the user to verify whether the options specified in req are supported by the transport provider. On return, the flags field of ret will have either T_SUCCESS or T_FAILURE set to indicate to the user whether the options are supported. These flags are only meaningful for the T_CHECK request.

T_DEFAULT
    Enables a user to retrieve the default options supported by the transport provider into the opt field of ret. In req, the len field of opt must be zero and the buf field may be NULL.

If issued as part of the connectionless-mode service, t_optmgmt() may block due to flow control constraints. t_optmgmt() will not complete until the transport provider has processed all previously sent data units.

RETURN VALUES

t_optmgmt() returns:

0   on success.

-1  on failure and sets t_errno to indicate the error.

ERRORS

TACCES
    The user does not have permission to negotiate the specified options.

TBADF
    The specified file descriptor does not refer to a transport endpoint.

TBADFLAG
    An invalid flag was specified.

TBADOPT
    The specified protocol options were in an incorrect format or contained illegal information.

TBUFOVFLW
    The number of bytes allowed for an incoming argument is not sufficient to store the value of that argument. The information to be returned in ret will be discarded.

TOUTSTATE
    The function was issued in the wrong sequence.

TSYSERR
    The function failed due to a system error and set errno to indicate the error.

SEE ALSO
intro(3), t_getinfo(3N), t_open(3N)