MOUSE(4S)

NAME
mouse - Sun mouse

CONFIG
None; included in standard system.

DESCRIPTION

The mouse indirect device provides access to the Sun Workstation mouse. When opened, it redirects operations to the standard mouse device for the workstation (attached either to a CPU serial or parallel port), and pushes the ms(4M) and ttcompat(4M) STREAMS modules on top of that device.

FILES
/dev/mouse

SEE ALSO
ms(4M), ttcompat(4M), win(4S), zs(4S)