COMMENTS:

1. This EEPROM package is for AOC-S40-i2q using XL710 LAN controller.
2. New EEUPDATE v5.24.33.07


EEPROM REVISION INFO:

5) S40GI220 (3/4/2015)
	a. Based on Intel XL710_4p42_QSFP_MCTP_CFGID4p5_Dual.bin
	b. SMC
		0x015	0200h
		0xC8A	15D9h
		0xC8B	084Ah
	c. Preboot
		0x33	4033h
	d. Enable GLPCI_CAPCTRL.VPD_EN bit to expose VPD capability on the PCI-E interface.
		0xC97	0001h

4) S40GI21C (1/15/2015)
	EEPROM correction from H.W design.
	a. SMC: 
		0x015	010Ch

3) S40GI21B (10/30/2014)
	a. Based on Intel XL710_4_26_QSFP_MCTP_CFGID4p5_Dual_800014B5.bin
	b. SMC: 
		0x015	010Bh
		0xC8A	159Dh
		0xC8B	084Ah
	c. Preboot
		0x33	4033h
	d. Enable GLPCI_CAPCTRL.VPD_EN bit to expose VPD capability on the PCI-E interface.
		0xC97	0001h

2) S40GI21A (9/4/2014)
	a. SMC: 
		0x015	010Ah
	b. Enable GLPCI_CAPCTRL.VPD_EN bit to expose VPD capability on the PCI-E interface.
		0xC97	0001h  

1) S40GI210 (8/12/2014)
	a. Based on Intel XL710_4_24_QSFP_MCTP_CFGID4p5_Dual_800012F3.bin	
	b. SMC: 
		0x015	0100h
		0xC8A	159Dh
		0xC8B	084Ah
	c. Preboot
		0x33	4033h

