AOC-S40G-i2Q production note:

1. Assign 4 sets of MAC and SANMAC addresses for AOC-S40G-i2Q.
2. Pre-program U10 with file s40Gi410.bin.
3. Run "Prod2x40.bat" to program MAC and SANMAC addresses for 4 ports.