COMMENTS:

This combination EEPROM package is for AOC-S40-i2q using XL710 LAN controller contains both 4x10G and 2x40G images.

NVM updating:
a- Use UP2x40.BAT if update from older 2x40G to current 2x40G, or changing the setup from 4x10G to 2x10G.  
	
b- Use UP4x10.BAT if changing the setup from 2x40G to 4x10G. 4 (four) set of MAC and SANMAC addresses is needed to obtain first before starting update the NVM. Recycle A/C power the system after running UP4x10.BAT then continue with UP4MAC.BAT to update the MAC and SANMAC addresses.


EEPROM REVISION INFO:
6) S40GC22A (6/1/2015)
	i. S40G20.bin    2x10G image is from LAN package S40GI220
		a. Based on Intel XL710_4p42_QSFP_MCTP_CFGID4p5_Dual.bin
		b. SMC
			0x015	0200h
			0xC8A	15D9h
			0xC8B	084Ah
		c. Preboot
			0x33	4033h
		d. Enable GLPCI_CAPCTRL.VPD_EN bit to expose VPD capability on the PCI-E interface.
			0xC97	0001h

	ii. S40Gi410.bin  4x10G image is from LAN package S40GI410
		a. Based on Intel XL710_4p42_QSFP_Breakout_MCTP_CFGID6p0_Quad.bin
		b. SMC: 
			0x015	0100h
			0xC8A	159Dh
			0xC8B	084Ah
		c. Preboot
			0x33	4033h
		d. Enable GLPCI_CAPCTRL.VPD_EN bit to expose VPD capability on the PCI-E interface.
			0xC97	0001h

5) S40GI220 (3/4/2015)
	a. Based on Intel XL710_4p42_QSFP_MCTP_CFGID4p5_Dual.bin
	b. SMC
		0x015	0200h
		0xC8A	15D9h
		0xC8B	084Ah
	c. Preboot
		0x33	4033h
	d. Enable GLPCI_CAPCTRL.VPD_EN bit to expose VPD capability on the PCI-E interface.
		0xC97	0001h

4) S40GI21C (1/15/2015)
	EEPROM correction from H.W design.
	a. SMC: 
		0x015	010Ch

3) S40GI21B (10/30/2014)
	a. Based on Intel XL710_4_26_QSFP_MCTP_CFGID4p5_Dual_800014B5.bin
	b. SMC: 
		0x015	010Bh
		0xC8A	159Dh
		0xC8B	084Ah
	c. Preboot
		0x33	4033h
	d. Enable GLPCI_CAPCTRL.VPD_EN bit to expose VPD capability on the PCI-E interface.
		0xC97	0001h

2) S40GI21A (9/4/2014)
	a. SMC: 
		0x015	010Ah
	b. Enable GLPCI_CAPCTRL.VPD_EN bit to expose VPD capability on the PCI-E interface.
		0xC97	0001h  

1) S40GI210 (8/12/2014)
	a. Based on Intel XL710_4_24_QSFP_MCTP_CFGID4p5_Dual_800012F3.bin	
	b. SMC: 
		0x015	0100h
		0xC8A	159Dh
		0xC8B	084Ah
	c. Preboot
		0x33	4033h

