; AST VBIOS Release Notes
;===============================================================================
v.0.97.06: ycchen@030113
01.[New] Modify for Read EDID Stability (over sample)
02.[New] Support AST2300 + Sil164 (AST2300.DVO)
 - move AST2300 + ITE66121 support to AST2300.ITE  
v.0.97.05: ycchen@121212
01.[Bug] Remove Wide Screen Support in VBIOS currently
v.0.97.04: ycchen@112512
01.[New] support vbios that display banner for 5sec
02.[New] Modify for ITE66121 support
03.[Bug] Fixed 800x600 16c mode display abnormal issue (v09700 issue)
v.0.97.03: ycchen@111512
01.[Bug] fixed memory allocation failed issue for some DOS Tools
v.0.97.02: ycchen@110112
01.[Bug] Modify DRAM Setting by H/W request
02.[Bug] Fixed ReadEDID cause system hanged with Avocent KVM
v.0.97.01: ycchen@102912
01.[Bug] Fixed WHCK - PnP Stress Test not Stable Issue
v.0.97.00: ycchen@102612
01.[New] [AST2300/2400] support AST2300/2400 + ITE66121
02.[Bug] Fixed WHCK PnP Stress Test Random Failed Issue
03.[New] Support WXGA modes in VBIOS, including 1280x800, 1440x900, 1680x1050, 1920x1080, 1366x768, 1600x900
04.[Bug] [AST2300/2400] Modify DRAM settings by H/W request
---------------------------------------------------------------------------------       
v.0.96.00: ycchen@081412
01.[New] [AST2400] Support AST2400 A0
02.[Bug] [AST2300] Modify DRAM settings for VBIOS coding bug
03.[New] [AST2300/2400] Set DAC source as VGA on POST
04.[New] Modify show logo time to 1sec
---------------------------------------------------------------------------------       
v.0.95.01: ycchen@052112
01.[Bug] Fixed iKVM cannot display properly if new VBIOS (v.0.92.00 and after) with older X Windows driver (before v.0.92.00)
02.[New] [AST2300] Modify DRAM settings by H/W request (2012_05_09)
v.0.95.00: ycchen@120224
01.[New] Support AST2400 FPGA
---------------------------------------------------------------------------------       
v.0.94.03: ycchen@112311
01.[New] Enable MMIO access by default
02.[Bug] [Flash] Fixed update flash unstable issue on some platform.
v.0.94.02: ycchen@102811
01.[New] [AST2300] Remove the patch for v.0.94.00 #2, Fixed in AMI CRB014 BIOS finally, ycchen@102811
v.0.94.01: ycchen@091611
01.[Bug] [AST2300] Fixed DRAM setting procedure issues
v.0.94.00: ycchen@091311
01.[New] [AST2300] Modify DRAM Settings by H/W Request (07/06/11), ycchen@081011
02.[Bug] [AST2300] Fixed ASPM can't be disabled properly on some specific platform, ycchen@090911
03.[New] [Flash Utility] Modify for General SPI Flash Support                                
---------------------------------------------------------------------------------       
v.0.93.08: ycchen@053111
01.[New] [AST2300] Modify MCLK to 396MHz by H/W request, ycchen@053111
v.0.93.07: ycchen@050911
01.[Bug] Fixed it takes too long time to get EDID from EDID failed monitor
02.[New] Display Bannner include AST1300
v.0.93.04: ycchen@030211
01.[New] [AST2300] Modify for DDR3 2Gb Support
02.[Bug] Fixed Intel iSCSI cursor disappear issue, ycchen@030411
03.[New] [AST2300] Slow CPU/AHB clock in VGA only mode
v.0.93.03: ycchen@021011
01.[New] [AST2300] Modify AST2300 DRAM Timing by H/W Request (020811)
02.[New] [AST2100/2150] Enable AST2100/2150 DRAM Calibration by H/W Request (021411)
v.0.93.02: ycchen@122410
01.[Bug] Fixed INT10 far jmp ptr failed issue
02.[New] Support EFI + VBIOS in one expansion ROM, ycchen@122210
v.0.93.01: ycchen@121410
01.[New] [AST2300] Modify CRT Threshold by H/W Request, ycchen@121410
02.[New] [AST2300] Disable ASPM for VGA Only solution
v.0.93.00: ycchen@121210
01.[New] Modify AST2300 DRAM Timing by H/W Request (121010)
02.[New] Add INT10 Far Call at the offset of 0x06 by DELL's request
---------------------------------------------------------------------------------       
v.0.92.02: ycchen@102010
01.[New] Set 800x600 default refresh rate to 60Hz
02.[Bug] Fixed wave form issue on 1280x1024 75Hz and 1280x800 60Hz 
03.[New] [AST2300] DRAM type and size selection based on H/W trapping
v.0.92.00: ycchen@080410
01.[New] Add More Mode Info to Scratch for General KVM Need
02.[New] Add for AST2300 VGA only solution
03.[New] Add for AST2300 A1 support
04.[New] Fixed display noise issue during linux kernel reboot (only fixed in AST2300)
---------------------------------------------------------------------------------       
v.0.91.0A: ycchen@062210
01.[Bug] Disable E2M for A0 chips issue
v.0.91.09: ycchen@062110
01.[New] Support AST2300 Real chips
02.[New] Disable E2M Read for A0 chips issue
v.0.91.07: ycchen@042110
01.[New] Modify display banner for AST2150/2200
v.0.91.06: ycchen@030410
01.[New] Show Framebuffer size while VBIOS POST
v.0.91.05: ycchen@020310
01.[New] modify for AST2300 FPGA DDR2 & DDR3 support, ycchen@110609
02.[New] Disable PCI-E to M-Bus for AST2300, ycchen@012710
03.[New] Remove Virtual EDID support for other than AST2000, ycchen@020310
v.0.91.00: ycchen@011110
01.[New] Support AST2300 FPGA Board
---------------------------------------------------------------------------------       
v.0.90.07: ycchen@102109 
01.[BUG] Fix DELL Diag failed issue, ycchen@102109
v.0.90.01: ycchen@082709
01.[Bug] Fixed have chance to get incorrect frame buffer base address if plug two ASPEED's Graphics, ycchen@072709
02.[New] Remove 8bpp VESA modes support above and equal than 1280x1024 due to backwidth issue
03.[New] Add DDR2 512Mx16 266MHz, 1Gx16 266 MHz support for AST2150
v.0.90.00: ycchen@071409
01.[New] remove AST1150 A0 PATCH
---------------------------------------------------------------------------------       
v.0.89.07:
01.[New] Modify DRAM timing by H/W request
02.[Bug] Fixed scrolling too slow in EGA mode, ycchen@050809
03.[Bug] Fixed SLES10.2 boot option wait too long issue, ycchen@051109
v.0.89.00: ycchen@121808
01.[New] Add DDR2 1Gx32.266 VBIOS Release for AST2100, ycchen@112608
02.[New] Add patch for AST1150, ycchen@121808
---------------------------------------------------------------------------------       
v.0.88.04: ycchen@101408
01.[New] Add AST2100 DVO Support, ycchen@100808
02.[Bug] Fixed code error in SetWriteBank & SetReadBank, ycchen@101408
03.[New] Modify DRAM Reg. Settings by H/W  Request, ycchen@102808
v.0.88.03: ycchen@100208
01.[Bug] Fix DELL RBU cause display blank issue, ycchen@100208
02.[New] Modify for the request of recovery BIOS by QCI
03.[Bug] Modify AST2100 DRAM timing for unstable issue (restore to v.0.88.01)
v.0.88.02: ycchen@090908
01.[New] Bump Version for AST1160
v.0.88.01: ycchen@090208
01.[New] Add AST1100/2050/2100 A2 Chip Identity, ycchen@090108
02.[New] Modify AST1100/2050/2100 DDR2 DRAM Timing by Jason's Request
v.0.88.00: ycchen@082808
01.[BUG] Fixed VGA2 Mirror Display on board solution can't work properly in Windows, ycchen@082708
---------------------------------------------------------------------------------       
v.0.87.00: ycchen@072908
01.[PATCH] Patch for AST2100/1100 A2 X-Window Compatible Issue, ycchen@072908
---------------------------------------------------------------------------------       
v.0.86.09: ycchen@051208
01.[New] Add DDR2 1Gx16 200MHz support
v.0.86.04: ycchen@032108
01.[Bug] Fixed the background color of edit is incorrect after run cls, ycchen@032108
v.0.86.00: ycchen@012808
01.[New] Modify DRAM settings by H/W (01108)
---------------------------------------------------------------------------------       
v.0.85.03: ycchen@010308
01.[New] Modify for DDR 512x16 200MHz settings
v.0.85.02: ycchen@121207
01.[Bug] Fixed DCT/SVGA/INT10 failed issue
02.[New] Modify DDR 512x16 200MHz parameters by H/W  request
v.0.85.01: ycchen@112707
01.[New] Modify DRAM timing by H/W request (11/08/07)
02.[Bug] Fixed display abnormal while new PLL modes change to standard modes, ycchen@112807
03.[New] Remove 1920x1200 for AST1100
04.[New] Modify Display banner for AST1100/2050/2100
05.[Bug] Change 1920x1200x60Hz's polarity to NP
v.0.85.00: ycchen@103107
01.[New] Modify 1920x1200x60Hz to reduced blank mode, ycchen@081307
02.[New] Support ECC
03.[Bug] Fixed PCCheck VGA Palette Test Failed Issue, ycchen@103107
04.[Bug] Fixed Scanline info incorrect in scratch, ycchen@103107
05.[Patch] Patch WDT can't detect mode change properly, ycchen@103107
06.[New] Set Scratch after DRAM Initial
07.[New] Enable Read Cache for AST2100 A1
---------------------------------------------------------------------------------       
v.0.84.05: ycchen@072607
01.[New] Disable ReadCache for AST2100 by H/W request
02.[New] Set VGA DRAM Trapping to DRAM Controller, ycchen@072607
v.0.84.04: ycchen@070907
01.[New] Modify DRAM timing for H/W request
v.0.84.03: ycchen@062107
01.[New] Modify DRAM timing to 266MHz
v.0.84.02: ycchen@061507        
01.[Bug] Fixed 1920x1200x60Hz can't display
02.[New] Modify DRAM timing by H/W request
v.0.84.01: ycchen@060807        
01.[New] Remove Chrontel Setting for real chip
02.[New] Use 512Mb x32 setting as default DRAM type
v.0.84.00: ycchen@060507        
01.[New] Support AST2100 A0, ycchen@053107
02.[New] Support 1920x1200x60Hz for AST2100, ycchen@060407
---------------------------------------------------------------------------------       
v.0.83.04: ycchen@051507
001.[Bug] Fixed bug check 0xf7 in vista64
v.0.83.03: ycchen@021607
001.[Bug] Fix AST2100 VGA & Video Threshold Issue, ycchen@02160
v.0.83.02: ycchen@020607
001.[Bug] Fix CMDQ & MMIO CMD reorder issue
v.0.83.01: ycchen@011207
001.[New] Modify for AST2100 New IP (0606)
002.[Bug] Fix BCMDiag video memory test failed, ycchen@011206
v.0.83.00: ycchen@120406
001.[New] Support AST2100 FPGA EVB Board
---------------------------------------------------------------------------------       
v.0.82.00b: ycchen@092906
001.[New] Initial VGA only if Class Code is VGA Device, ycchen@091506
002.[New] Add the support for VGA initial SOC RTC
003.[New] Add scratch for scan line infor, ycchen@092906
v.0.82.00: ycchen@061406
001. Bump Version Only
---------------------------------------------------------------------------------       
v.0.81.01: ycchen@051106                       
001.[Bug] Fixed save/restore PLL setting incorrect by ycchen@051106
v.0.81.00: ycchen@042406                       
001.[New] Set MCLK166 as default, ycchen@042406
---------------------------------------------------------------------------------       
v.0.80.00: ycchen@031306        
001.[BUG] Fixed PCDR/AMIDIAG/BCMDIAG RAMDAC Test too long issue, ycchen@030606                
002.[PATCH] Fixed ARC1220 RAID controller display message abnormal issue, ycchen@031006
---------------------------------------------------------------------------------       
v.0.63.00: ycchen@020906         
001. [Bug] Run PCDR/Video memory test cause KVM crash
---------------------------------------------------------------------------------       
v.0.62.00: ycchen@020606            
001. [Patch] QCI LCD Monitor display dummy under the bottom of the screen
---------------------------------------------------------------------------------       
v.0.61.00: ycchen@011106   
001.[Bug] fixed VRS/VRE incorrect issue, ycchen@122805
002.[New] 32k VBIOS as default
003.[New] Modify for product description
004.[New] Support 16/32 DRAM in one VBIOS
005.[Bug] Can't Set VESA Mode: 1280x1024x32bpp, ycchen@010606
006.[Bug] 640x480x72Hz Border issue
007.[Bug] Modify for low-reslution timing, ycchen@011005
008.[Bug] fixed AMIDIAG\VESA memory test failed issue, ycchen@011206
009.[Bug] Modify for CRTC timing for STD. mods, ycchen@011206
---------------------------------------------------------------------------------       
v.0.60.00: ycchen@12202005, first release for A1    
001.[New] Modify for A1 support
002.[New] Integrate LFB/UMA VBIOS into one (ASTVBIOS.ROM)
---------------------------------------------------------------------------------       
v.0.52.00: ycchen@11042005
1. [New] Change Device to 0x1A03
---------------------------------------------------------------------------------       
v.0.51.00: ycchen@10252005
1. [Bug] Fixed ReadHat9 Install Shell Display Abnormal Issue
2. [New] Modify for DRAM init status check in UMA mode
3. [New] Support Customizded DRAM timing in binary level
4. [New] Support Virtual EDID
5. [Bug] Install RHEL hanged before enter into X-Window on Operon
6. [Bug] Modify for CRTC Timing for standrad mode & low resolution mode
7. [New] Add Support VESA Mode: 1280x1204, 1600x1200, 320x240, 400x300 and 512x384
---------------------------------------------------------------------------------       
v.0.50.00: ycchen@10122005
1. The first release for A0
